<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<library>
<packages>
<package name="RS485-LCTECH">
<description>RS485 Module
from LC-Tech
based on Max485</description>
</package>
<package name="USR-ES1">
</package>
</packages>
<symbols>
<symbol name="RS485-LCTECH">
<description>RS485 Module
from LC-Tech
based on Max485</description>
<pin name="RO"/>
<pin name="DI"/>
<pin name="DE"/>
<pin name="RE"/>
<pin name="VCC"/>
<pin name="B"/>
<pin name="A"/>
<pin name="GND"/>
</symbol>
<symbol name="USR-ES1">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCLK" direction="in"/>
<pin name="!INT!" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V+@1" direction="pwr"/>
<pin name="!SCS!" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="RES" direction="in"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RS485-LCTECH">
<description>RS485 Module
from LC-Tech
based on Max485</description>
<gates>
<gate name="G$1" symbol="RS485-LCTECH"/>
</gates>
<devices>
<device name="" package="RS485-LCTECH">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="DE" pad="DE"/>
<connect gate="G$1" pin="DI" pad="DI"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RE" pad="RE"/>
<connect gate="G$1" pin="RO" pad="RO"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LAN-USR-ES1" prefix="IC">
<gates>
<gate name="G$1" symbol="USR-ES1"/>
</gates>
<devices>
<device name="" package="USR-ES1">
<connects>
<connect gate="G$1" pin="!INT!" pad="6"/>
<connect gate="G$1" pin="!SCS!" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="3"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="RES" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="4"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="V+@1" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
