(module TTB_Power (layer F.Cu) (tedit 57827189)
  (fp_text reference REF** (at 0 6.1) (layer F.SilkS))
  (fp_text value TTB_Power (at 0 -9.9) (layer F.Fab))
  (pad 1 thru_hole oval (at 0 -8.8) (size 5 2.2) (drill oval 3.2 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 -2.6) (size 5 2.2) (drill oval 2.6 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 5 -5.7) (size 2.2 5) (drill oval 0.8 2.6) (layers *.Cu *.Mask))
  (model Connect.3dshapes/JACK_ALIM.wrl
    (at (xyz 0 0.1 0))
    (scale (xyz 0.8 0.8 0.8))
    (rotate (xyz 0 0 270))
  )
)
