<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>Holtek LDO, Voltage Regulator
Vout 3V3, Vin max. 12V, Vdrop 90mV, Iss 4uA, Iout min. 250mA</description>
<packages>
<package name="TO92-4">
<description>TO-92 in line with additional Pin 4, compability</description>
</package>
<package name="SOT89">
<description>SOT-89 LDO, 3pin+Tab</description>
</package>
</packages>
<symbols>
<symbol name="VREG_SOT89">
<description>Voltage Regulator, 3pin+Tab</description>
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
<pin name="IN@0" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HT7333-A" prefix="U" uservalue="yes">
<description>LDO Voltage Regulator</description>
<gates>
<gate name="G$1" symbol="VREG_SOT89"/>
</gates>
<devices>
<device name="SOT89" package="SOT89">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN" route="any"/>
<connect gate="G$1" pin="IN@0" pad="TAB"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name="SOT89"/>
</technologies>
</device>
<device name="TO92-4" package="TO92-4">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="IN@0" pad="IN@0"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
