<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="24.11" y2="0" width="0" layer="20"/>
<wire x1="24.11" y1="0" x2="24.11" y2="37.77" width="0" layer="20"/>
<wire x1="24.11" y1="37.77" x2="0" y2="37.77" width="0" layer="20"/>
<wire x1="0" y1="37.77" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="28c256dil">
<packages>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
</packages>
</library>
<library name="memory-hitachi">
<packages>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="28c256dil" package="DIL28-6" value="28C256DIL"/>
<element name="IC2" library="memory-hitachi" package="DIL28-6" value="27c256">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
</elements>
<signals>
<signal name="A01">
<contactref element="IC2" pad="9"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="A02">
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="A03">
<contactref element="IC2" pad="7"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="A04">
<contactref element="IC2" pad="6"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="A05">
<contactref element="IC2" pad="5"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="A06">
<contactref element="IC2" pad="4"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="A07">
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="A08">
<contactref element="IC2" pad="25"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="A10">
<contactref element="IC2" pad="21"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="A11">
<contactref element="IC2" pad="23"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="A12">
<contactref element="IC2" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="A13">
<contactref element="IC2" pad="26"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="A14">
<contactref element="IC2" pad="27"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="A09">
<contactref element="IC2" pad="24"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="D00">
<contactref element="IC2" pad="11"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="D01">
<contactref element="IC2" pad="12"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="D02">
<contactref element="IC2" pad="13"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="D03">
<contactref element="IC2" pad="15"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="D04">
<contactref element="IC2" pad="16"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="D05">
<contactref element="IC2" pad="17"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="D06">
<contactref element="IC2" pad="18"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="D07">
<contactref element="IC2" pad="19"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="A00">
<contactref element="IC2" pad="10"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="28"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="27"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="OE">
<contactref element="IC2" pad="22"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="CE">
<contactref element="IC2" pad="20"/>
<contactref element="IC1" pad="20"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
