<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<hole x="139" y="5" drill="3.1"/>
<hole x="140" y="135" drill="3.1"/>
<hole x="5" y="135" drill="3.1"/>
<hole x="5" y="5" drill="3.1"/>
<hole x="5" y="47" drill="3.1"/>
<hole x="80" y="5" drill="3.1"/>
<hole x="139" y="70" drill="3.1"/>
<hole x="95" y="135" drill="3.1"/>
<wire x1="0" y1="0" x2="0" y2="140" width="0.254" layer="20"/>
<wire x1="0" y1="140" x2="144" y2="140" width="0.254" layer="20"/>
<wire x1="144" y1="140" x2="144" y2="0" width="0.254" layer="20"/>
<wire x1="144" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>Batt Extension</text>
<text>Vin 12 - 24V</text>
<text>Vout0 (drive)</text>
<text>Vout1 (mow)</text>
<text>T-Mow Energy V1.1, © 2020, Anton Schegg</text>
<text>5V out
(Raspberry)</text>
<text>GND   +5V</text>
<text>CAN Termination: 120Ohm</text>
<text>GND</text>
<text>GND</text>
<text>CAN</text>
<text>CAN</text>
<text>CR1220
RTC Battery</text>
<text>MAIN SWITCH</text>
</plain>
<libraries>
<library name="as-resistors">
<packages>
<package name="0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
</packages>
</library>
<library name="as-capacitors">
<packages>
<package name="RCL_C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="RCL_C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="as-connectors">
<packages>
<package name="MOLEX-MICRO-FIT3_43650-0216">
<description>Micro-Fit 3.0 Vertical Header, 3.00mm Pitch, Single Row, 2 Circuits, with PCB Polarizing Peg, Gold, Glow Wire Capable, Black</description>
</package>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MOLEX-C-GRID-SL_70543-POS4">
<description>Molex C-Grid/SL - 70543 - Header, Shrouded, Thru Hole, Latch Holder
&lt;p&gt;&lt;a href='http://www.molex.com/pdm_docs/sd/705430001_sd.pdf'&gt;http://www.molex.com/pdm_docs/sd/705430001_sd.pdf&lt;/a&gt;</description>
</package>
<package name="MOLEX-MICRO-FIT+_3206832-0201">
</package>
<package name="MOLEX-ULTRA-FIT_172286-1102">
</package>
<package name="MOLEX-ULTRA-FIT_172299-1206">
</package>
</packages>
</library>
<library name="as-linear">
<packages>
<package name="WQFN32-4X4-TI-RSN">
</package>
<package name="HTSSOP16">
<description>Package LP, 16-Pin TSSOP with Exposed Thermal Pad</description>
</package>
</packages>
</library>
<library name="as-transistors">
<packages>
<package name="HSMT8">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="SOP-8">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="SOT95P230X110-3N">
</package>
</packages>
</library>
<library name="as-inductors">
<packages>
<package name="WE-LHMI_8040_PW5">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-LHMI SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8040
&lt;/b&gt;PW5 means the width of the pin is 5.0 mm</description>
</package>
<package name="WE-TPC_2828_OLD">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2828</description>
</package>
<package name="WE-XHMI_1090">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-XHMI SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1090</description>
</package>
</packages>
</library>
<library name="as-jumpers">
<packages>
<package name="SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="JUMPER_2_NC_PASTE_NO-SILK">
</package>
</packages>
</library>
<library name="as-digital">
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SO8">
</package>
<package name="TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SO-18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
</packages>
</library>
<library name="as-crystals">
<packages>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="as-leds">
<packages>
<package name="LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="as-regulators">
<packages>
<package name="TPS56637RPAR">
</package>
<package name="SOT95P280X110-6N">
</package>
</packages>
</library>
<library name="as-diodes">
<packages>
<package name="SOD-323F">
<description>Diode, Small Outline Diode (SOD); 1.70 mm L X 1.30 mm W X 1.12 mm H body&lt;p&gt;&lt;i&gt;PCB Libraries Packages&lt;/i&gt;</description>
</package>
</packages>
</library>
<library name="as-displays">
<packages>
<package name="OLED-128X64-I2C-V2">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;&lt;br /&gt;
Variant with I2C interface</description>
</package>
</packages>
</library>
<library name="as-switches">
<packages>
<package name="MULTIMEC-5GTH935RAS">
</package>
<package name="E101J1ABE2">
</package>
</packages>
</library>
<library name="as-electrics">
<packages>
<package name="MICROBUILDER_">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J4" library="as-connectors" package="MOLEX-MICRO-FIT3_43650-0216" value="MOLEX-MICRO-FIT-3_V_2">
<attribute name="DIGIKEY" value="WM1922-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="0436500216"/>
</element>
<element name="U1" library="as-linear" package="WQFN32-4X4-TI-RSN" value="BQ25703A">
<attribute name="DIGIKEY" value="296-46956-1-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="BQ25703ARSNT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="as-resistors" package="2010" value="0.01 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="as-resistors" package="0603" value="4.99">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="as-resistors" package="0603" value="4.99">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="as-capacitors" package="RCL_C0603" value="33nF">
<attribute name="DIGIKEY" value="399-9068-1-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C333J3RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="33nF"/>
</element>
<element name="C6" library="as-capacitors" package="RCL_C0603" value="33nF">
<attribute name="DIGIKEY" value="399-9068-1-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C333J3RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="33nF"/>
</element>
<element name="C7" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="C9" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="as-capacitors" package="RCL_C0805" value="1uF">
<attribute name="DIGIKEY" value="1276-6606-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL21B105KBFVPNE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="as-capacitors" package="RCL_C0805" value="1uF">
<attribute name="DIGIKEY" value="1276-6606-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL21B105KBFVPNE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="as-capacitors" package="RCL_C0805" value="1uF">
<attribute name="DIGIKEY" value="1276-6606-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL21B105KBFVPNE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="as-resistors" package="0603" value="10">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD10R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD10R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="as-resistors" package="0603" value="10">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD10R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD10R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="as-capacitors" package="RCL_C0603" value="33pF">
<attribute name="DIGIKEY" value="399-C0603C330K5RAC7800CT-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C330K5RAC7800"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="as-resistors" package="0603" value="40k2">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD4022FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD4022F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="as-capacitors" package="RCL_C0603" value="1800pF">
<attribute name="DIGIKEY" value="399-7867-1-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C182K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="as-capacitors" package="RCL_C0603" value="15pF">
<attribute name="DIGIKEY" value="399-20391-1-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C150K5RAC7867"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="15pF"/>
</element>
<element name="R15" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="C18" library="as-capacitors" package="RCL_C0603" value="680pF">
<attribute name="DIGIKEY" value="478-12730-1-ND"/>
<attribute name="MANUFACTURER" value="AVX Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="06035C681K4T2A"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="680pF"/>
</element>
<element name="R8" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="as-capacitors" package="RCL_C0805" value="2.2uF">
<attribute name="DIGIKEY" value="445-174216-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="CGA4J3X7R1H225K125AB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="as-capacitors" package="RCL_C0603" value="47nF">
<attribute name="DIGIKEY" value="445-C1608X7R1H473K080AACT-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C1608X7R1H473K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="as-capacitors" package="RCL_C0603" value="47nF">
<attribute name="DIGIKEY" value="445-C1608X7R1H473K080AACT-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C1608X7R1H473K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="as-inductors" package="WE-LHMI_8040_PW5" value="2u2H">
<attribute name="DIGIKEY" value="732-7208-1-ND"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MANUFACTURER_PARTNO" value="74437358022"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="2u2H"/>
</element>
<element name="Q10" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="as-transistors" package="SOP-8" value="MCQ4435-TP">
<attribute name="DIGIKEY" value="MCQ4435-TPMSCT-ND"/>
<attribute name="MANUFACTURER" value="Micro Commercial Co"/>
<attribute name="MANUFACTURER_PARTNO" value="MCQ4435-TP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="as-resistors" package="2010" value="0.01 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="as-resistors" package="0603" value="10">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD10R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD10R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="as-resistors" package="0603" value="10">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD10R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD10R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="as-resistors" package="0603" value="40k2">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD4022FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD4022F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="as-resistors" package="0603" value="137k">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD1373FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD1373F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="as-capacitors" package="RCL_C0603" value="100pF">
<attribute name="DIGIKEY" value="399-C0603C101J5RACAUTOCT-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C101J5RACAUTO"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="as-jumpers" package="SJW" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="as-digital" package="TSSOP20" value="MCP2515_TSOP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="as-digital" package="SO8" value="SN65HVD230D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q14" library="as-crystals" package="CTS406" value="16MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="as-capacitors" package="RCL_C0603" value="18pF">
<attribute name="DIGIKEY" value="1276-2206-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10C180FB8NNNC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="as-capacitors" package="RCL_C0603" value="18pF">
<attribute name="DIGIKEY" value="1276-2206-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10C180FB8NNNC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="as-resistors" package="0603" value="4k7">
<attribute name="DIGIKEY" value="A129696CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F4K7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="as-resistors" package="0603" value="120">
<attribute name="DIGIKEY" value="A129677CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F120R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="as-digital" package="TQFP44" value="ATMEGA32A-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="as-resistors" package="0603" value="4k7">
<attribute name="DIGIKEY" value="A129696CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F4K7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="as-connectors" package="MA05-2" value="Prog/Debug">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="as-capacitors" package="RCL_C0603" value="10nF">
<attribute name="DIGIKEY" value="1276-CL10B103KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B103KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="as-leds" package="LED0603" value="green">
<attribute name="DIGIKEY" value="475-2709-1-ND"/>
<attribute name="MANUFACTURER" value="OSRAM Opto Semiconductors Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="LG L29K-G2J1-24-Z"/>
<attribute name="NAME"/>
<attribute name="SPANNUNG" value="1,7V"/>
<attribute name="STROM" value="2mA"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="as-resistors" package="0603" value="820">
<attribute name="DIGIKEY" value="A129687CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F820R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="as-connectors" package="MOLEX-C-GRID-SL_70543-POS4" value="MOLEX-C-GRID-SL_HEADER_POS470543"/>
<element name="X2" library="as-connectors" package="MOLEX-C-GRID-SL_70543-POS4" value="MOLEX-C-GRID-SL_HEADER_POS470543"/>
<element name="Q6" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="as-resistors" package="1206W" value="47">
<attribute name="DIGIKEY" value="2019-WK73R2BTTD47R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="WK73R2BTTD47R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q11" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="as-resistors" package="1206W" value="47">
<attribute name="DIGIKEY" value="2019-WK73R2BTTD47R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="WK73R2BTTD47R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q12" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="as-resistors" package="1206W" value="47">
<attribute name="DIGIKEY" value="2019-WK73R2BTTD47R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="WK73R2BTTD47R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q13" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q9" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="as-resistors" package="1206W" value="47">
<attribute name="DIGIKEY" value="2019-WK73R2BTTD47R0FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="WK73R2BTTD47R0F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="as-regulators" package="SOT95P280X110-6N" value="TPS54308DDCR">
<attribute name="DIGIKEY" value="296-47880-1-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="TPS54308DDCR"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="TPS54308DDCR"/>
</element>
<element name="C32" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="as-inductors" package="WE-TPC_2828_OLD" value="10uH">
<attribute name="DIGIKEY" value="732-2617-1-ND"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MANUFACTURER_PARTNO" value="744025100"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="as-resistors" package="0603" value="100k">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD1003FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD1003F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="as-resistors" package="0603" value="22k">
<attribute name="DIGIKEY" value="A129704CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F22K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="as-capacitors" package="RCL_C0805" value="22uF">
<attribute name="DIGIKEY" value="490-9956-1-ND"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PARTNO" value="GRM21BC81C226ME44L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="as-resistors" package="0603" value="5k36">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD5361FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD5361F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="as-resistors" package="0603" value="1k2">
<attribute name="DIGIKEY" value="A129689CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F1K2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="as-capacitors" package="RCL_C0603" value="1uF">
<attribute name="DIGIKEY" value="587-3305-1-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="MANUFACTURER_PARTNO" value="EMK107B7105KAHT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="as-capacitors" package="RCL_C0603" value="1uF">
<attribute name="DIGIKEY" value="587-3305-1-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="MANUFACTURER_PARTNO" value="EMK107B7105KAHT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="as-capacitors" package="RCL_C0603" value="1uF">
<attribute name="DIGIKEY" value="587-3305-1-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="MANUFACTURER_PARTNO" value="EMK107B7105KAHT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="as-capacitors" package="RCL_C0603" value="1uF">
<attribute name="DIGIKEY" value="587-3305-1-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="MANUFACTURER_PARTNO" value="EMK107B7105KAHT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="as-resistors" package="0603" value="1k2">
<attribute name="DIGIKEY" value="A129689CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F1K2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="as-resistors" package="0603" value="3k3">
<attribute name="DIGIKEY" value="A129694CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F3K3"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="as-resistors" package="0603" value="3k3">
<attribute name="DIGIKEY" value="A129694CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F3K3"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="as-resistors" package="0603" value="1k2">
<attribute name="DIGIKEY" value="A129689CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F1K2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="as-resistors" package="0603" value="5k36">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD5361FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD5361F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="as-resistors" package="0603" value="3k57">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD3571FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD3571F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="as-jumpers" package="SJW" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="as-regulators" package="TPS56637RPAR" value="TPS56637RPAR">
<attribute name="DIGIKEY" value="296-TPS56637RPARCT-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="TPS56637RPAR"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="TPS56637RPAR"/>
</element>
<element name="C42" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="as-capacitors" package="RCL_C0805" value="10uF">
<attribute name="DIGIKEY" value="445-14419-1-ND"/>
<attribute name="MANUFACTURER" value="TDK Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="C2012X5R1V106M085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="as-resistors" package="0603" value="20k">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD2002FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD2002F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="as-resistors" package="0603" value="33">
<attribute name="DIGIKEY" value="A129670CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F33R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="as-capacitors" package="RCL_C0603" value="100pF">
<attribute name="DIGIKEY" value="399-C0603C101J5RACAUTOCT-ND"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURER_PARTNO" value="C0603C101J5RACAUTO"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="as-resistors" package="0603" value="73k2">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD7322FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD7322F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="as-inductors" package="WE-XHMI_1090" value="3.3uH">
<attribute name="DIGIKEY" value="732-10709-1-ND"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MANUFACTURER_PARTNO" value="74439369033"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="as-capacitors" package="RCL_C0805" value="22uF">
<attribute name="DIGIKEY" value="490-9956-1-ND"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PARTNO" value="GRM21BC81C226ME44L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="as-capacitors" package="RCL_C0805" value="22uF">
<attribute name="DIGIKEY" value="490-9956-1-ND"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PARTNO" value="GRM21BC81C226ME44L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="as-capacitors" package="RCL_C0805" value="22uF">
<attribute name="DIGIKEY" value="490-9956-1-ND"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PARTNO" value="GRM21BC81C226ME44L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="as-capacitors" package="RCL_C0805" value="22uF">
<attribute name="DIGIKEY" value="490-9956-1-ND"/>
<attribute name="MANUFACTURER" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PARTNO" value="GRM21BC81C226ME44L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="as-resistors" package="0603" value="2k2">
<attribute name="DIGIKEY" value="A129692CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F2K2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="as-resistors" package="0603" value="2k2">
<attribute name="DIGIKEY" value="A129692CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F2K2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="as-resistors" package="0603" value="4k7">
<attribute name="DIGIKEY" value="A129696CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F4K7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="as-diodes" package="SOD-323F" value="1N4148WS">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="as-linear" package="HTSSOP16" value="TPS2HB16AQPWPRQ1">
<attribute name="DIGIKEY" value="296-TPS2HB16AQPWPRQ1CT-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="TPS2HB16AQPWPRQ1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="as-connectors" package="MOLEX-MICRO-FIT+_3206832-0201" value="MOLEX-MICRO_FIT+_">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Connector Header Through Hole 2 position "/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="206832-0201"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="as-connectors" package="MOLEX-MICRO-FIT+_3206832-0201" value="MOLEX-MICRO_FIT+_">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Connector Header Through Hole 2 position "/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="206832-0201"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="as-digital" package="SO-18W" value="MCP23S08SO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD1" library="as-displays" package="OLED-128X64-I2C-V2" value="OLED-128X64-I2C-V2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="as-resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="as-switches" package="MULTIMEC-5GTH935RAS" value="5GTH935RAS">
<attribute name="DIGIKEY" value="679-3576-ND"/>
<attribute name="MANUFACTURER" value="MEC Switches"/>
<attribute name="MANUFACTURER_PARTNO" value="5GTH935RAS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="as-resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SW3" library="as-switches" package="MULTIMEC-5GTH935RAS" value="5GTH935RAS">
<attribute name="DIGIKEY" value="679-3576-ND"/>
<attribute name="MANUFACTURER" value="MEC Switches"/>
<attribute name="MANUFACTURER_PARTNO" value="5GTH935RAS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="as-resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SW4" library="as-switches" package="MULTIMEC-5GTH935RAS" value="5GTH935RAS">
<attribute name="DIGIKEY" value="679-3576-ND"/>
<attribute name="MANUFACTURER" value="MEC Switches"/>
<attribute name="MANUFACTURER_PARTNO" value="5GTH935RAS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="as-switches" package="E101J1ABE2" value="E101J1AQE2">
<attribute name="DIGIKEY" value="CKN2070-ND"/>
<attribute name="MANUFACTURER" value="C&amp;K"/>
<attribute name="MANUFACTURER_PARTNO" value="E101J1AQE2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="as-connectors" package="MOLEX-ULTRA-FIT_172286-1102" value="172286-1102">
<attribute name="DIGIKEY" value="WM11570-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="1722861102"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="as-electrics" package="MICROBUILDER_" value="CR1220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="as-digital" package="SO16W" value="DS3231/SO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="as-resistors" package="0603" value="20k">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD2002FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD2002F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="as-resistors" package="0603" value="20k">
<attribute name="DIGIKEY" value="2019-RK73H1JTTD2002FCT-ND"/>
<attribute name="MANUFACTURER" value="KOA Speer Electronics, Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="RK73H1JTTD2002F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="as-capacitors" package="RCL_C0603" value="100nF">
<attribute name="DIGIKEY" value="1276-CL10B104KB8WPNDCT-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURER_PARTNO" value="CL10B104KB8WPND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="as-resistors" package="0603" value="1k">
<attribute name="DIGIKEY" value="A129688CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F1K0"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="as-resistors" package="0603" value="10k">
<attribute name="DIGIKEY" value="A129700CT-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity Passive Product"/>
<attribute name="MANUFACTURER_PARTNO" value="CRGCQ0603F10K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="as-capacitors" package="RCL_C0603" value="680pF">
<attribute name="DIGIKEY" value="478-12730-1-ND"/>
<attribute name="MANUFACTURER" value="AVX Corporation"/>
<attribute name="MANUFACTURER_PARTNO" value="06035C681K4T2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="as-connectors" package="MOLEX-ULTRA-FIT_172299-1206" value="172299-1206">
<attribute name="DIGIKEY" value="WM11785-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="1722991206"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="as-diodes" package="SOD-323F" value="1N4148WS">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="as-diodes" package="SOD-323F" value="1N4148WS">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="as-diodes" package="SOD-323F" value="1N4148WS">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="as-connectors" package="MOLEX-ULTRA-FIT_172299-1206" value="172299-1206">
<attribute name="DIGIKEY" value="WM11785-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="1722991206"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="as-jumpers" package="JUMPER_2_NC_PASTE_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="10"/>
<contactref element="C35" pad="2"/>
<contactref element="R40" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="X1" pad="P$1"/>
<contactref element="X2" pad="P$1"/>
<contactref element="C41" pad="2"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="39"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="IC3" pad="28"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV1" pad="9"/>
<contactref element="LED1" pad="C"/>
<contactref element="R19" pad="1"/>
<contactref element="Q6" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="Q7" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="Q8" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="Q9" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="R42" pad="1"/>
<contactref element="C38" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="R36" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="R38" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="R60" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="9"/>
<contactref element="LCD1" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW4" pad="1"/>
<contactref element="IC5" pad="13"/>
<contactref element="B1" pad="-"/>
<contactref element="C56" pad="2"/>
<contactref element="IC5" pad="12"/>
<contactref element="IC5" pad="11"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC5" pad="9"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC5" pad="8"/>
<contactref element="C51" pad="2"/>
<contactref element="C52" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="20"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="C35" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="R44" pad="1"/>
<contactref element="IC3" pad="27"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC3" pad="38"/>
<contactref element="C40" pad="1"/>
<contactref element="SV1" pad="7"/>
<contactref element="SV1" pad="4"/>
<contactref element="L2" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="C38" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="R46" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R55" pad="2"/>
<contactref element="LCD1" pad="2"/>
<contactref element="R48" pad="2"/>
<contactref element="R49" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="C56" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="IC4" pad="18"/>
</signal>
<signal name="VIN">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VIN1A">
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="Q1" pad="7"/>
<contactref element="Q1" pad="6"/>
<contactref element="Q1" pad="8"/>
<contactref element="Q1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VDDA">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="REGN">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="28"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="ILM_HIZ">
<contactref element="U1" pad="6"/>
<contactref element="R7" pad="2"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C16" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$16">
<contactref element="R15" pad="1"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="/PROCHOT">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="11"/>
<contactref element="IC3" pad="43"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="13"/>
<contactref element="IC3" pad="19"/>
<contactref element="R47" pad="1"/>
<contactref element="LCD1" pad="3"/>
<contactref element="IC5" pad="16"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="12"/>
<contactref element="IC3" pad="20"/>
<contactref element="R46" pad="1"/>
<contactref element="LCD1" pad="4"/>
<contactref element="IC5" pad="15"/>
</signal>
<signal name="CHRG_OK">
<contactref element="R9" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="EN_OTG">
<contactref element="U1" pad="5"/>
<contactref element="R10" pad="2"/>
<contactref element="IC3" pad="25"/>
</signal>
<signal name="CMPOUT">
<contactref element="U1" pad="15"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="CMPIN">
<contactref element="U1" pad="14"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="7"/>
<contactref element="Q2" pad="6"/>
<contactref element="Q2" pad="8"/>
<contactref element="Q2" pad="5"/>
<contactref element="U1" pad="32"/>
<contactref element="C12" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="SW2">
<contactref element="Q3" pad="7"/>
<contactref element="Q3" pad="6"/>
<contactref element="Q3" pad="8"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q4" pad="1"/>
<contactref element="U1" pad="23"/>
<contactref element="C13" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="Q1" pad="4"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="29"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="Q4" pad="4"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$22">
<contactref element="Q3" pad="4"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="BTST1">
<contactref element="C12" pad="2"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="BTST2">
<contactref element="U1" pad="25"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="VSYS">
<contactref element="Q4" pad="8"/>
<contactref element="Q4" pad="6"/>
<contactref element="Q4" pad="7"/>
<contactref element="Q4" pad="5"/>
<contactref element="Q5" pad="3"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q5" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="C42" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="U4" pad="17"/>
<contactref element="R57" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="C53" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="CELL1">
<contactref element="JP7" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="CELL2">
<contactref element="JP6" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="CELL3">
<contactref element="JP5" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="VBATT">
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="Q10" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="VBATT_DRV">
<contactref element="C20" pad="1"/>
<contactref element="Q5" pad="7"/>
<contactref element="Q5" pad="5"/>
<contactref element="Q5" pad="6"/>
<contactref element="Q5" pad="8"/>
<contactref element="R17" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="/BATDRV">
<contactref element="U1" pad="21"/>
<contactref element="Q5" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="20"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="19"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="CELL_BATPRESZ">
<contactref element="U1" pad="18"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="IADPT">
<contactref element="U1" pad="8"/>
<contactref element="R13" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="PGND">
<contactref element="C8" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="IC2" pad="9"/>
<contactref element="Q14" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="TXCAN">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="RXCAN">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="CANH">
<contactref element="IC1" pad="7"/>
<contactref element="R39" pad="2"/>
<contactref element="X1" pad="P$4"/>
<contactref element="X2" pad="P$4"/>
</signal>
<signal name="CANL">
<contactref element="IC1" pad="6"/>
<contactref element="R39" pad="1"/>
<contactref element="X1" pad="P$3"/>
<contactref element="X2" pad="P$3"/>
</signal>
<signal name="RS">
<contactref element="R40" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$35">
<contactref element="Q14" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="IC2" pad="19"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC2" pad="16"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="14"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="17"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="8"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="/CS0">
<contactref element="IC3" pad="40"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="JTAG-TMS">
<contactref element="IC3" pad="22"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="JTAG-TDI">
<contactref element="SV1" pad="2"/>
<contactref element="IC3" pad="24"/>
</signal>
<signal name="JTAG-TDO">
<contactref element="SV1" pad="8"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="INT0">
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="JTAG-TCK">
<contactref element="SV1" pad="10"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="AREF1">
<contactref element="C39" pad="1"/>
<contactref element="IC3" pad="29"/>
</signal>
<signal name="/RESET">
<contactref element="R44" pad="2"/>
<contactref element="IC3" pad="4"/>
<contactref element="C41" pad="1"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="R45" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="CELL_4S_DIS_EN">
<contactref element="Q6" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="N$24">
<contactref element="Q10" pad="3"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="Q11" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="Q11" pad="3"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="Q12" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="Q8" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="Q12" pad="3"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="Q13" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="Q9" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="Q13" pad="3"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="CELL_1S_DIS_EN">
<contactref element="Q9" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="CELL_2S_DIS_EN">
<contactref element="Q8" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="CELL_3S_DIS_EN">
<contactref element="Q7" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="BOOST">
<contactref element="U2" pad="6"/>
<contactref element="C34" pad="1"/>
</signal>
<signal name="SW">
<contactref element="U2" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R42" pad="2"/>
<contactref element="R41" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="CELL4_ADC">
<contactref element="R31" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="IC3" pad="34"/>
</signal>
<signal name="CELL3_ADC">
<contactref element="R33" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="IC3" pad="35"/>
</signal>
<signal name="CELL2_ADC">
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="IC3" pad="36"/>
</signal>
<signal name="CELL1_ADC">
<contactref element="R37" pad="1"/>
<contactref element="R38" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="IC3" pad="37"/>
</signal>
<signal name="N$26">
<contactref element="X1" pad="P$2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="X2" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="J4" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C50" pad="1"/>
</signal>
<signal name="PGND5">
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="U3" pad="9"/>
<contactref element="J4" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP10" pad="2"/>
<contactref element="R59" pad="1"/>
<contactref element="C53" pad="2"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="EN_5V">
<contactref element="U3" pad="1"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="BOOT_5V">
<contactref element="U3" pad="7"/>
<contactref element="C45" pad="1"/>
</signal>
<signal name="SW_5V">
<contactref element="U3" pad="6"/>
<contactref element="C45" pad="2"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="PG_5V">
<contactref element="U3" pad="4"/>
<contactref element="IC3" pad="42"/>
</signal>
<signal name="N$7">
<contactref element="R53" pad="1"/>
<contactref element="R54" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C46" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R52" pad="1"/>
<contactref element="R53" pad="2"/>
<contactref element="R51" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C46" pad="1"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="AGND5">
<contactref element="R54" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="IC3" pad="44"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="CURRENT_SENSE">
<contactref element="IC3" pad="33"/>
<contactref element="R56" pad="1"/>
<contactref element="C52" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U4" pad="16"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="U4" pad="4"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="N$33">
<contactref element="U4" pad="13"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="VOUT0">
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="7"/>
<contactref element="J6" pad="1"/>
<contactref element="C55" pad="1"/>
</signal>
<signal name="VOUT1">
<contactref element="U4" pad="9"/>
<contactref element="U4" pad="11"/>
<contactref element="U4" pad="10"/>
<contactref element="J5" pad="1"/>
<contactref element="C54" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U4" pad="1"/>
<contactref element="R60" pad="2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$43">
<contactref element="U4" pad="15"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="N$44">
<contactref element="U4" pad="14"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="N$45">
<contactref element="U4" pad="3"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="/CS1">
<contactref element="IC4" pad="7"/>
<contactref element="IC3" pad="41"/>
</signal>
<signal name="N$25">
<contactref element="R55" pad="1"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="SWITCH3">
<contactref element="R50" pad="1"/>
<contactref element="SW4" pad="3"/>
<contactref element="IC3" pad="30"/>
</signal>
<signal name="SWITCH1">
<contactref element="R48" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="IC3" pad="32"/>
</signal>
<signal name="SWITCH2">
<contactref element="R49" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="IC3" pad="31"/>
</signal>
<signal name="BAL_CELL4">
<contactref element="R23" pad="2"/>
<contactref element="Q10" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="BAL_CELL3">
<contactref element="Q11" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="BAL_CELL2">
<contactref element="Q12" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="BAL_CELL1">
<contactref element="Q13" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="JP7" pad="2"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="IC5" pad="14"/>
<contactref element="B1" pad="+$1"/>
</signal>
<signal name="/INTRTC">
<contactref element="IC5" pad="3"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="N$46">
<contactref element="R57" pad="1"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="N$47">
<contactref element="R58" pad="1"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="SNS">
<contactref element="U4" pad="2"/>
<contactref element="R59" pad="2"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="PGND1">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="PGND_HIGH_CURRENT">
<contactref element="J1" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="JP11" pad="2"/>
<contactref element="U1" pad="PAD"/>
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$2"/>
<contactref element="U1" pad="P$3"/>
<contactref element="U1" pad="P$4"/>
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="P$5"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="5"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="VIN3V3">
<contactref element="D3" pad="C"/>
<contactref element="C32" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="22"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="BATT_PLUS">
<contactref element="JP4" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="SW1" pad="P$3"/>
</signal>
<signal name="BAL_PGND">
<contactref element="R30" pad="1"/>
<contactref element="JP8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
