<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<hole x="139" y="5" drill="3.1"/>
<hole x="139" y="85" drill="3.1"/>
<hole x="5" y="85" drill="3.1"/>
<hole x="5" y="5" drill="3.1"/>
<hole x="5" y="47" drill="3.1"/>
<hole x="80" y="5" drill="3.1"/>
<hole x="139" y="70" drill="3.1"/>
<hole x="95" y="85" drill="3.1"/>
<wire x1="0" y1="0" x2="0" y2="90" width="0.254" layer="20"/>
<wire x1="0" y1="90" x2="144" y2="90" width="0.254" layer="20"/>
<wire x1="144" y1="90" x2="144" y2="0" width="0.254" layer="20"/>
<wire x1="144" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>Batt Extension</text>
<text>Vin 12 - 24V</text>
<text>Vout0 (drive)</text>
<text>Vout1 (mow)</text>
<text>T-Mow Energy V1.1, © 2021, Anton Schegg</text>
<text>5V out
(Raspberry)</text>
<text>GND   +5V</text>
<text>CAN Termination: 120Ohm</text>
<text>GND</text>
<text>GND</text>
<text>CAN</text>
<text>CAN</text>
<text>CR1220
RTC Battery</text>
<text>MAIN SWITCH</text>
<hole x="95" y="5" drill="3.1"/>
<text>OFF</text>
<text>ON</text>
</plain>
<libraries>
<library name="as-resistors">
<packages>
<package name="2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="as-connectors">
<packages>
<package name="MOLEX-MICRO-FIT3_43650-0216">
<description>Micro-Fit 3.0 Vertical Header, 3.00mm Pitch, Single Row, 2 Circuits, with PCB Polarizing Peg, Gold, Glow Wire Capable, Black</description>
</package>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MOLEX-C-GRID-SL_70543-POS4">
<description>Molex C-Grid/SL - 70543 - Header, Shrouded, Thru Hole, Latch Holder
&lt;p&gt;&lt;a href='http://www.molex.com/pdm_docs/sd/705430001_sd.pdf'&gt;http://www.molex.com/pdm_docs/sd/705430001_sd.pdf&lt;/a&gt;</description>
</package>
<package name="MOLEX-MICRO-FIT+_3206832-0201">
</package>
<package name="MOLEX-ULTRA-FIT_172286-1102">
</package>
<package name="MOLEX-ULTRA-FIT_172299-1206">
</package>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="as-linear">
<packages>
<package name="WQFN32-4X4-TI-RSN">
</package>
<package name="HTSSOP16">
<description>Package LP, 16-Pin TSSOP with Exposed Thermal Pad</description>
</package>
</packages>
</library>
<library name="as-transistors">
<packages>
<package name="HSMT8">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="SOP-8">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="SOT95P230X110-3N">
</package>
</packages>
</library>
<library name="as-inductors">
<packages>
<package name="WE-LHMI_8040_PW5">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-LHMI SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8040
&lt;/b&gt;PW5 means the width of the pin is 5.0 mm</description>
</package>
<package name="WE-TPC_2828_OLD">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2828</description>
</package>
<package name="WE-XHMI_1090">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-XHMI SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1090</description>
</package>
</packages>
</library>
<library name="as-jumpers">
<packages>
<package name="SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SMT-JUMPER_2_NC_TRACE_SILK">
</package>
</packages>
</library>
<library name="as-digital">
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SO8">
</package>
<package name="TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
</packages>
</library>
<library name="as-crystals">
<packages>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="as-leds">
<packages>
<package name="LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="as-regulators">
<packages>
<package name="TPS56637RPAR">
</package>
<package name="SOT95P280X110-6N">
</package>
</packages>
</library>
<library name="as-diodes">
<packages>
<package name="SOD-323F">
<description>Diode, Small Outline Diode (SOD); 1.70 mm L X 1.30 mm W X 1.12 mm H body&lt;p&gt;&lt;i&gt;PCB Libraries Packages&lt;/i&gt;</description>
</package>
</packages>
</library>
<library name="as-displays">
<packages>
<package name="OLED-128X64-I2C-V2-VERTICAL">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;&lt;br /&gt;
Variant with I2C interface</description>
</package>
</packages>
</library>
<library name="as-switches">
<packages>
<package name="MULTIMEC-5GTH935RAS">
</package>
<package name="E101J1ABE2">
</package>
</packages>
</library>
<library name="as-electrics">
<packages>
<package name="MICROBUILDER_">
</package>
</packages>
</library>
<library name="gustl_RCL">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J4" library="as-connectors" package="MOLEX-MICRO-FIT3_43650-0216" value="MOLEX-MICRO-FIT-3_V_2">
<attribute name="DIGIKEY" value="WM1922-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="0436500216"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="as-linear" package="WQFN32-4X4-TI-RSN" value="BQ25703A">
<attribute name="DIGIKEY" value="296-46956-1-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="BQ25703ARSNT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="as-resistors" package="2010" value="0.01 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="gustl_RCL" package="R0603" value="4.99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="gustl_RCL" package="R0603" value="4.99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="gustl_RCL" package="C0603" value="33nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="gustl_RCL" package="C0603" value="33nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="gustl_RCL" package="R0603" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="gustl_RCL" package="R0603" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7_OPT" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gustl_RCL" package="C0603" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="gustl_RCL" package="R0603" value="40k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="gustl_RCL" package="C0603" value="1800pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="gustl_RCL" package="C0603" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="gustl_RCL" package="C0603" value="680pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="as-transistors" package="HSMT8" value="RQ3E100BNTB">
<attribute name="DIGIKEY" value="RQ3E100BNTBCT-ND"/>
<attribute name="MANUFACTURER" value="Rohm Semiconductor"/>
<attribute name="MANUFACTURER_PARTNO" value="RQ3E100BNTB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="gustl_RCL" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="gustl_RCL" package="C0603" value="47nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="gustl_RCL" package="C0603" value="47nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="as-inductors" package="WE-LHMI_8040_PW5" value="2u2H">
<attribute name="DIGIKEY" value="732-7208-1-ND"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MANUFACTURER_PARTNO" value="74437358022"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q10" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="as-transistors" package="SOP-8" value="MCQ4435-TP">
<attribute name="DIGIKEY" value="MCQ4435-TPMSCT-ND"/>
<attribute name="MANUFACTURER" value="Micro Commercial Co"/>
<attribute name="MANUFACTURER_PARTNO" value="MCQ4435-TP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="as-resistors" package="2010" value="0.01 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="gustl_RCL" package="R0603" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="gustl_RCL" package="R0603" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="gustl_RCL" package="R0603" value="40k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="gustl_RCL" package="R0603" value="137k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="gustl_RCL" package="C0603" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="as-digital" package="TSSOP20" value="MCP2515_TSOP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="as-digital" package="SO8" value="SN65HVD230D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q14" library="as-crystals" package="CTS406" value="16MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="gustl_RCL" package="C0603" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="gustl_RCL" package="C0603" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="gustl_RCL" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="gustl_RCL" package="R0603" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="as-digital" package="TQFP44" value="ATMEGA32A-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="gustl_RCL" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="as-connectors" package="MA05-2" value="Prog/Debug">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="gustl_RCL" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="as-leds" package="LED0603" value="green">
<attribute name="DIGIKEY" value="475-2709-1-ND"/>
<attribute name="MANUFACTURER" value="OSRAM Opto Semiconductors Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="LG L29K-G2J1-24-Z"/>
<attribute name="NAME"/>
<attribute name="SPANNUNG" value="1,7V"/>
<attribute name="STROM" value="2mA"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="gustl_RCL" package="R0603" value="820">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="as-connectors" package="MOLEX-C-GRID-SL_70543-POS4" value="MOLEX-C-GRID-SL_HEADER_POS470543"/>
<element name="X2" library="as-connectors" package="MOLEX-C-GRID-SL_70543-POS4" value="MOLEX-C-GRID-SL_HEADER_POS470543"/>
<element name="Q6" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="gustl_RCL" package="R0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q11" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="gustl_RCL" package="R0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q12" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="gustl_RCL" package="R0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q13" library="as-transistors" package="SOT23" value="DMP3056L-7">
<attribute name="DIGIKEY" value="DMP3056L-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PARTNO" value="DMP3056L-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q9" library="as-transistors" package="SOT95P230X110-3N" value="NX7002AK,215">
<attribute name="DIGIKEY" value="1727-1289-1-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="MANUFACTURER_PARTNO" value="NX7002AK,215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="gustl_RCL" package="R0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="as-regulators" package="SOT95P280X110-6N" value="TPS54308DDCR">
<attribute name="DIGIKEY" value="296-47880-1-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="TPS54308DDCR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="as-inductors" package="WE-TPC_2828_OLD" value="10uH">
<attribute name="DIGIKEY" value="732-2617-1-ND"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MANUFACTURER_PARTNO" value="744025100"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="gustl_RCL" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="gustl_RCL" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="gustl_RCL" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="gustl_RCL" package="R0603" value="5k36">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="gustl_RCL" package="R0603" value="1k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="gustl_RCL" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="gustl_RCL" package="R0603" value="1k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="gustl_RCL" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="gustl_RCL" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="gustl_RCL" package="R0603" value="1k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="gustl_RCL" package="R0603" value="5k36">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="gustl_RCL" package="R0603" value="3k57">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2_CAN_VCC" library="as-jumpers" package="SJW" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="as-regulators" package="TPS56637RPAR" value="TPS56637RPAR">
<attribute name="DIGIKEY" value="296-TPS56637RPARCT-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="TPS56637RPAR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="gustl_RCL" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="gustl_RCL" package="R0603" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="gustl_RCL" package="R0603" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="gustl_RCL" package="C0603" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="gustl_RCL" package="R0603" value="73k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="as-inductors" package="WE-XHMI_1090" value="3.3uH">
<attribute name="DIGIKEY" value="732-10709-1-ND"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MANUFACTURER_PARTNO" value="74439369033"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="gustl_RCL" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="gustl_RCL" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="gustl_RCL" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="gustl_RCL" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="gustl_RCL" package="R0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="gustl_RCL" package="R0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="gustl_RCL" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="as-diodes" package="SOD-323F" value="1N4148WS">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="as-linear" package="HTSSOP16" value="TPS2HB16AQPWPRQ1">
<attribute name="DIGIKEY" value="296-TPS2HB16AQPWPRQ1CT-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PARTNO" value="TPS2HB16AQPWPRQ1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="as-connectors" package="MOLEX-MICRO-FIT+_3206832-0201" value="MOLEX-MICRO_FIT+_">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Connector Header Through Hole 2 position "/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="206832-0201"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="as-connectors" package="MOLEX-MICRO-FIT+_3206832-0201" value="MOLEX-MICRO_FIT+_">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Connector Header Through Hole 2 position "/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="206832-0201"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="LCD1" library="as-displays" package="OLED-128X64-I2C-V2-VERTICAL" value="OLED-128X64-I2C-V2VERTICAL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="as-switches" package="MULTIMEC-5GTH935RAS" value="5GTH935RAS">
<attribute name="DIGIKEY" value="679-3576-ND"/>
<attribute name="MANUFACTURER" value="MEC Switches"/>
<attribute name="MANUFACTURER_PARTNO" value="5GTH935RAS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW3" library="as-switches" package="MULTIMEC-5GTH935RAS" value="5GTH935RAS">
<attribute name="DIGIKEY" value="679-3576-ND"/>
<attribute name="MANUFACTURER" value="MEC Switches"/>
<attribute name="MANUFACTURER_PARTNO" value="5GTH935RAS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW4" library="as-switches" package="MULTIMEC-5GTH935RAS" value="5GTH935RAS">
<attribute name="DIGIKEY" value="679-3576-ND"/>
<attribute name="MANUFACTURER" value="MEC Switches"/>
<attribute name="MANUFACTURER_PARTNO" value="5GTH935RAS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="as-switches" package="E101J1ABE2" value="E101J1AQE2">
<attribute name="DIGIKEY" value="CKN2070-ND"/>
<attribute name="MANUFACTURER" value="C&amp;K"/>
<attribute name="MANUFACTURER_PARTNO" value="E101J1AQE2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="as-connectors" package="MOLEX-ULTRA-FIT_172286-1102" value="172286-1102">
<attribute name="DIGIKEY" value="WM11570-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="1722861102"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="as-electrics" package="MICROBUILDER_" value="CR1220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="as-digital" package="SO16W" value="DS3231/SO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="gustl_RCL" package="R0603" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="gustl_RCL" package="R0603" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="gustl_RCL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="gustl_RCL" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="gustl_RCL" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="gustl_RCL" package="C0603" value="680pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="as-connectors" package="MOLEX-ULTRA-FIT_172299-1206" value="172299-1206">
<attribute name="DIGIKEY" value="WM11785-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="1722991206"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="as-diodes" package="SOD-323F" value="PMEG3005EJ,115">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="as-diodes" package="SOD-323F" value="PMEG3005EJ,115">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="as-diodes" package="SOD-323F" value="PMEG3005EJ,115">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4148WSFSTR-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="1N4148WS"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-323"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="as-connectors" package="MOLEX-ULTRA-FIT_172299-1206" value="172299-1206">
<attribute name="DIGIKEY" value="WM11785-ND"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="MANUFACTURER_PARTNO" value="1722991206"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="gustl_RCL" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="as-connectors" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD5_GND" library="as-connectors" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="PAD1_VIN" library="as-connectors" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="as-jumpers" package="SMT-JUMPER_2_NC_TRACE_SILK" value="CMPIN_GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD4_VBATT" library="as-connectors" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="PAD3_VSYS" library="as-connectors" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2_GND" library="as-connectors" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="PAD6_5V" library="as-connectors" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="PAD7_GND" library="as-connectors" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R7_OPT" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="10"/>
<contactref element="C35" pad="2"/>
<contactref element="R40" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="X1" pad="P$1"/>
<contactref element="X2" pad="P$1"/>
<contactref element="C41" pad="2"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="39"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="IC3" pad="28"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV1" pad="9"/>
<contactref element="LED1" pad="C"/>
<contactref element="R19" pad="1"/>
<contactref element="Q6" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="Q7" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="Q8" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="Q9" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="R42" pad="1"/>
<contactref element="C38" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="R36" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="R38" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="R60" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW4" pad="1"/>
<contactref element="IC5" pad="13"/>
<contactref element="B1" pad="-"/>
<contactref element="C56" pad="2"/>
<contactref element="IC5" pad="12"/>
<contactref element="IC5" pad="11"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC5" pad="9"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC5" pad="8"/>
<contactref element="C52" pad="2"/>
<contactref element="R59" pad="1"/>
<contactref element="C53" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="9"/>
<contactref element="R54" pad="1"/>
<contactref element="C47" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="5"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q3" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="PAD"/>
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$2"/>
<contactref element="U1" pad="P$3"/>
<contactref element="U1" pad="P$4"/>
<contactref element="U1" pad="P$5"/>
<contactref element="J1" pad="2"/>
<contactref element="LCD1" pad="2"/>
<contactref element="PAD5_GND" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="PAD7_GND" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="20"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="C35" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="R44" pad="1"/>
<contactref element="IC3" pad="27"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC3" pad="38"/>
<contactref element="C40" pad="1"/>
<contactref element="SV1" pad="7"/>
<contactref element="SV1" pad="4"/>
<contactref element="L2" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="C38" pad="1"/>
<contactref element="SJ2_CAN_VCC" pad="1"/>
<contactref element="R46" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R48" pad="2"/>
<contactref element="R49" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="C56" pad="1"/>
<contactref element="LCD1" pad="1"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="PAD1_VIN" pad="1"/>
</signal>
<signal name="VIN1A">
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="Q1" pad="7"/>
<contactref element="Q1" pad="6"/>
<contactref element="Q1" pad="8"/>
<contactref element="Q1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VDDA">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="REGN">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="28"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="ILM_HIZ">
<contactref element="U1" pad="6"/>
<contactref element="R7_OPT" pad="2"/>
<contactref element="R61" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C16" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$16">
<contactref element="R15" pad="1"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="13"/>
<contactref element="IC3" pad="19"/>
<contactref element="R47" pad="1"/>
<contactref element="IC5" pad="16"/>
<contactref element="LCD1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="12"/>
<contactref element="IC3" pad="20"/>
<contactref element="R46" pad="1"/>
<contactref element="IC5" pad="15"/>
<contactref element="LCD1" pad="4"/>
</signal>
<signal name="EN_OTG">
<contactref element="U1" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="CMPOUT">
<contactref element="U1" pad="15"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="CMPIN">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="7"/>
<contactref element="Q2" pad="6"/>
<contactref element="Q2" pad="8"/>
<contactref element="Q2" pad="5"/>
<contactref element="U1" pad="32"/>
<contactref element="C12" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="SW2">
<contactref element="Q3" pad="7"/>
<contactref element="Q3" pad="6"/>
<contactref element="Q3" pad="8"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q4" pad="1"/>
<contactref element="U1" pad="23"/>
<contactref element="C13" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="Q1" pad="4"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="29"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="Q4" pad="4"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$22">
<contactref element="Q3" pad="4"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="BTST1">
<contactref element="C12" pad="2"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="BTST2">
<contactref element="U1" pad="25"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="VSYS">
<contactref element="Q4" pad="8"/>
<contactref element="Q4" pad="6"/>
<contactref element="Q4" pad="7"/>
<contactref element="Q4" pad="5"/>
<contactref element="Q5" pad="3"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q5" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="C42" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="U4" pad="17"/>
<contactref element="R57" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="C53" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="U1" pad="22"/>
<contactref element="PAD3_VSYS" pad="1"/>
</signal>
<signal name="CELL1">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="Q13" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="CELL2">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="Q12" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="CELL3">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="Q11" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="VBATT">
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="D3" pad="A"/>
<contactref element="PAD4_VBATT" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="Q10" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="VBATT_DRV">
<contactref element="C20" pad="1"/>
<contactref element="Q5" pad="7"/>
<contactref element="Q5" pad="5"/>
<contactref element="Q5" pad="6"/>
<contactref element="Q5" pad="8"/>
<contactref element="R17" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="/BATDRV">
<contactref element="U1" pad="21"/>
<contactref element="Q5" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="20"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="19"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="CELL_BATPRESZ">
<contactref element="U1" pad="18"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="IADPT">
<contactref element="U1" pad="8"/>
<contactref element="R13" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="IC2" pad="9"/>
<contactref element="Q14" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="TXCAN">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="RXCAN">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="CANH">
<contactref element="IC1" pad="7"/>
<contactref element="R39" pad="2"/>
<contactref element="X1" pad="P$4"/>
<contactref element="X2" pad="P$4"/>
</signal>
<signal name="CANL">
<contactref element="IC1" pad="6"/>
<contactref element="R39" pad="1"/>
<contactref element="X1" pad="P$3"/>
<contactref element="X2" pad="P$3"/>
</signal>
<signal name="RS">
<contactref element="R40" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$35">
<contactref element="Q14" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="IC2" pad="19"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC2" pad="16"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="14"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="8"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="/CS0">
<contactref element="IC3" pad="40"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="JTAG-TMS">
<contactref element="IC3" pad="22"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="JTAG-TDI">
<contactref element="SV1" pad="2"/>
<contactref element="IC3" pad="24"/>
</signal>
<signal name="JTAG-TDO">
<contactref element="SV1" pad="8"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="INT0">
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="JTAG-TCK">
<contactref element="SV1" pad="10"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="AREF1">
<contactref element="C39" pad="1"/>
<contactref element="IC3" pad="29"/>
</signal>
<signal name="/RESET">
<contactref element="R44" pad="2"/>
<contactref element="IC3" pad="4"/>
<contactref element="C41" pad="1"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="R45" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="CELL_4S_DIS_EN">
<contactref element="Q6" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="N$24">
<contactref element="Q10" pad="3"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="Q11" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="Q11" pad="3"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="Q12" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="Q8" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="Q12" pad="3"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="Q13" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="Q9" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="Q13" pad="3"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="CELL_1S_DIS_EN">
<contactref element="Q9" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="CELL_2S_DIS_EN">
<contactref element="Q8" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="CELL_3S_DIS_EN">
<contactref element="Q7" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="BOOST">
<contactref element="U2" pad="6"/>
<contactref element="C34" pad="1"/>
</signal>
<signal name="SW">
<contactref element="U2" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R42" pad="2"/>
<contactref element="R41" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="CELL4_ADC">
<contactref element="R31" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="IC3" pad="34"/>
</signal>
<signal name="CELL3_ADC">
<contactref element="R33" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="IC3" pad="35"/>
</signal>
<signal name="CELL2_ADC">
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="IC3" pad="36"/>
</signal>
<signal name="CELL1_ADC">
<contactref element="R37" pad="1"/>
<contactref element="R38" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="IC3" pad="37"/>
</signal>
<signal name="N$26">
<contactref element="X1" pad="P$2"/>
<contactref element="SJ2_CAN_VCC" pad="2"/>
<contactref element="X2" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="J4" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="PAD6_5V" pad="1"/>
</signal>
<signal name="EN_5V">
<contactref element="U3" pad="1"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="BOOT_5V">
<contactref element="U3" pad="7"/>
<contactref element="C45" pad="1"/>
</signal>
<signal name="SW_5V">
<contactref element="U3" pad="6"/>
<contactref element="C45" pad="2"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="PG_5V">
<contactref element="U3" pad="4"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="N$7">
<contactref element="R53" pad="1"/>
<contactref element="R54" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C46" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R52" pad="1"/>
<contactref element="R53" pad="2"/>
<contactref element="R51" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C46" pad="1"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="IC3" pad="44"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="CURRENT_SENSE">
<contactref element="IC3" pad="33"/>
<contactref element="R56" pad="1"/>
<contactref element="C52" pad="1"/>
</signal>
<signal name="TPS_2HB16A_DIA_EN">
<contactref element="U4" pad="16"/>
<contactref element="IC3" pad="41"/>
</signal>
<signal name="EN_VOUT0">
<contactref element="U4" pad="4"/>
<contactref element="IC3" pad="25"/>
</signal>
<signal name="EN_VOUT1">
<contactref element="U4" pad="13"/>
<contactref element="IC3" pad="26"/>
</signal>
<signal name="VOUT0">
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="7"/>
<contactref element="J6" pad="1"/>
<contactref element="C55" pad="1"/>
</signal>
<signal name="VOUT1">
<contactref element="U4" pad="9"/>
<contactref element="U4" pad="11"/>
<contactref element="U4" pad="10"/>
<contactref element="J5" pad="1"/>
<contactref element="C54" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U4" pad="1"/>
<contactref element="R60" pad="2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="TPS_2HB16A_SEL2">
<contactref element="U4" pad="15"/>
<contactref element="IC3" pad="43"/>
</signal>
<signal name="TPS_2HB16A_SEL1">
<contactref element="U4" pad="14"/>
<contactref element="IC3" pad="42"/>
</signal>
<signal name="SWITCH3">
<contactref element="R50" pad="1"/>
<contactref element="SW4" pad="3"/>
<contactref element="IC3" pad="30"/>
</signal>
<signal name="SWITCH1">
<contactref element="R48" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="IC3" pad="32"/>
</signal>
<signal name="SWITCH2">
<contactref element="R49" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="IC3" pad="31"/>
</signal>
<signal name="N$42">
<contactref element="IC5" pad="14"/>
<contactref element="B1" pad="+$1"/>
</signal>
<signal name="/INTRTC">
<contactref element="IC5" pad="3"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="N$46">
<contactref element="R57" pad="1"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="N$47">
<contactref element="R58" pad="1"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="SNS">
<contactref element="U4" pad="2"/>
<contactref element="R59" pad="2"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="VIN3V3">
<contactref element="D3" pad="C"/>
<contactref element="C32" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="BATT_PLUS">
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="SW1" pad="P$3"/>
<contactref element="R23" pad="2"/>
<contactref element="Q10" pad="2"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="CHRG_OK">
<contactref element="PAD3" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="GND1">
<contactref element="PAD2_GND" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
