<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100.33" y2="0" width="0" layer="20"/>
<wire x1="100.33" y1="0" x2="100.33" y2="80.264" width="0" layer="20"/>
<wire x1="100.33" y1="80.264" x2="0" y2="80.254" width="0" layer="20"/>
<wire x1="0" y1="80.254" x2="0" y2="0" width="0" layer="20"/>
<hole x="3" y="3" drill="3"/>
<hole x="3" y="77" drill="3"/>
<hole x="97.79" y="77.47" drill="3"/>
<hole x="97.79" y="2.54" drill="3"/>
<hole x="82.55" y="31.115" drill="3"/>
<hole x="82.395" y="10.62" drill="3"/>
<hole x="81.915" y="52.07" drill="3"/>
<text>Univ_Steuer
V0.7</text>
<text>23.8.2021</text>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MKDSN1,5/2-5,08">
<description>&lt;b&gt;MKDSN 1,5/ 2-5,08&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 13,5 A&lt;br&gt;
Nennspannung: 250 V&lt;br&gt;
Rastermaß: 5,08 mm&lt;br&gt;
Polzahl: 2&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Montage: Löten&lt;br&gt;
Anschlussrichtung Leiter/Platine: 0 °&lt;br&gt;
Artikelnummer: 1729128&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1729128.pdf</description>
</package>
<package name="MKDSN1,5/8-5,08">
<description>&lt;b&gt;MKDSN 1,5/ 8-5,08&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 13,5 A&lt;br&gt;
Nennspannung: 250 V&lt;br&gt;
Rastermaß: 5,08 mm&lt;br&gt;
Polzahl: 8&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Montage: Löten&lt;br&gt;
Anschlussrichtung Leiter/Platine: 0 °&lt;br&gt;
Artikelnummer: 1729186&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1729186.pdf</description>
</package>
</packages>
</library>
<library name="Aqua_Power_12V">
<packages>
<package name="SO23">
</package>
<package name="D_PACK_TO252">
</package>
</packages>
</library>
<library name="con-phoenix-254">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 2.54 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
<package name="6POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-ml">
<description>&lt;b&gt;Harting  Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML6">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="IRLML6401">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="kzh20_lithium_batterie_holder">
<description>Lithium Battery Holder for CR2032</description>
<packages>
<package name="KZH20SMD">
</package>
</packages>
</library>
<library name="DS3231_SO16W">
<description>&lt;b&gt;IPC Standard SMD Packages&lt;/b&gt;&lt;p&gt;
This is a package-only library, based on the Surface Mount Design and Land Pattern Standard developed by the 
Institute for Interconnecting and Packaging electronic Circuits (IPC).&lt;p&gt;
Source:&lt;p&gt;
IPC-SM-782&lt;br&gt;
Revision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO28W">
<description>&lt;B&gt;28-Lead Plastic Small Outline (SO) &lt;/B&gt; Wide, 300 mil Body (SOIC)&lt;/B&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ftdichip">
<description>&lt;b&gt;FTDI (TM) CHIP&lt;/b&gt; Future Technology Devices International Ltd.&lt;p&gt;
http://www.ftdichip.com</description>
<packages>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt; SSOP-28&lt;p&gt;
http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
</library>
<library name="PESD12VL2BT">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-kycon">
<description>&lt;b&gt;Connector from KYCON, Inc&lt;/b&gt;&lt;p&gt;
1810 Little Orchard Street,&lt;br&gt;
San Jose,&lt;br&gt;
CA 95125 (408)494-0330&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/autor&gt;</description>
<packages>
<package name="KUSBVX-BS1N">
<description>&lt;b&gt;USB B-type Receptacle&lt;/b&gt; Vertical, 4 Position, Through Hole&lt;p&gt;
Source: Sibalco Kycon KUSBVX-BS1N-xxx.pdf</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
</packages>
</library>
<library name="MCP4728">
<packages>
<package name="MSOP10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="E5-10,5" value="2200u/16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Aqua_Power_12V" package="SO23" value="IRML2502">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Aqua_Power_12V" package="SO23" value="IRML2502">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Aqua_Power_12V" package="SO23" value="IRML2502">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="Aqua_Power_12V" package="SO23" value="IRML2502">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-phoenix-254" package="8POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="Aqua_Power_12V" package="D_PACK_TO252" value="IRLR2905">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="Aqua_Power_12V" package="D_PACK_TO252" value="IRLR2905">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="Aqua_Power_12V" package="D_PACK_TO252" value="IRLR2905">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="Aqua_Power_12V" package="D_PACK_TO252" value="IRLR2905">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-phoenix-508" package="MKDSN1,5/8-5,08" value="MKDSN1,5/8-5,08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="E5-10,5" value="2200u/16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="con-ml" package="ML6" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R100" library="rcl" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C100" library="rcl" package="E2-5" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C101" library="rcl" package="E2-5" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="kzh20_lithium_batterie_holder" package="KZH20SMD" value="2032">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="DS3231_SO16W" package="SO16W" value="DS3231">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="atmel" package="TQFP44" value="MEGA16-A">
<attribute name="OC_NEWARK" value="96K6515"/>
<attribute name="MPN" value="ATMEGA16-16AU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9171134"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="microchip" package="SO28W" value="MCP23S17SO">
<attribute name="OC_NEWARK" value="31K2950"/>
<attribute name="MPN" value="MCP23S17-E/SO"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$16" library="IRLML6401" package="SOT23" value="IRLML6401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$17" library="IRLML6401" package="SOT23" value="IRLML6401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$18" library="IRLML6401" package="SOT23" value="IRLML6401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="E5-10,5" value="2200u/16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X6" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X8" library="con-phoenix-254" package="6POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="ftdichip" package="SSOP28" value="FT232RL">
<attribute name="OC_NEWARK" value="91K9918"/>
<attribute name="MPN" value="FT232RL"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1146032"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="SML0603" value="Gelb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="led" package="SML0603" value="Grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="rcl" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="PESD12VL2BT" package="SOT23" value="PESD5V0L2BT_3P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$21" library="PESD12VL2BT" package="SOT23" value="PESD5V0L2BT_3P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$22" library="PESD12VL2BT" package="SOT23" value="PESD5V0L2BT_3P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C1206" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="pinhead" package="1X16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$24" library="IRLML6401" package="SOT23" value="IRLML6401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="R0603" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="E2-5" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="E2-5" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="con-kycon" package="KUSBVX-BS1N" value="KUSBVX-BS1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X9" library="con-kycon" package="KUSBVX-BS1N" value="KUSBVX-BS1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="maxim" package="SO16L" value="MAX232ECWE">
<attribute name="OC_NEWARK" value="67K4440"/>
<attribute name="MPN" value="MAX232ECWE+"/>
<attribute name="MF" value="MAXIM"/>
<attribute name="OC_FARNELL" value="9724435"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="MCP4728" package="MSOP10" value="MCP4728">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0603" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="rcl" package="R0805" value="10Uh">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value=""/>
<element name="SJ3" library="jumper" package="SJ" value=""/>
<element name="SJ4" library="jumper" package="SJ" value=""/>
<element name="SJ6" library="jumper" package="SJ" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="U$4" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="U$5" pad="3"/>
<contactref element="U$6" pad="3"/>
<contactref element="U$7" pad="3"/>
<contactref element="U$8" pad="3"/>
<contactref element="X3" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP4" pad="4"/>
<contactref element="SV2" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="C100" pad="-"/>
<contactref element="C5" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C101" pad="-"/>
<contactref element="C6" pad="1"/>
<contactref element="JP6" pad="6"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="U$11" pad="-"/>
<contactref element="U$13" pad="13"/>
<contactref element="IC2" pad="28"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="39"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="X8" pad="3"/>
<contactref element="X8" pad="5"/>
<contactref element="R20" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC3" pad="15"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="25"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="21"/>
<contactref element="C12" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="U$21" pad="2"/>
<contactref element="U$9" pad="2"/>
<contactref element="U$22" pad="2"/>
<contactref element="R35" pad="1"/>
<contactref element="C34" pad="2"/>
<contactref element="JP8" pad="10"/>
<contactref element="JP8" pad="16"/>
<contactref element="Q4" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="X6" pad="1"/>
<contactref element="C11" pad="-"/>
<contactref element="C14" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C21" pad="-"/>
<contactref element="C20" pad="-"/>
<contactref element="JP7" pad="8"/>
<contactref element="IC1" pad="26"/>
<contactref element="X7" pad="4"/>
<contactref element="X9" pad="4"/>
<contactref element="IC5" pad="15"/>
<contactref element="C16" pad="2"/>
<contactref element="JP5" pad="4"/>
<contactref element="U$10" pad="10"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP9" pad="4"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="10"/>
<contactref element="C23" pad="1"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="+12V">
<contactref element="X3" pad="2"/>
<contactref element="X4" pad="1"/>
<contactref element="X4" pad="3"/>
<contactref element="X4" pad="5"/>
<contactref element="X4" pad="7"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="3"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="X2" pad="6"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="X2" pad="4"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="X2" pad="2"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="1"/>
<contactref element="U$5" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="1"/>
<contactref element="U$6" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="1"/>
<contactref element="U$7" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R8" pad="1"/>
<contactref element="U$8" pad="1"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="X4" pad="2"/>
<contactref element="U$5" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="X4" pad="4"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="X4" pad="6"/>
<contactref element="U$7" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="X4" pad="8"/>
<contactref element="U$8" pad="4"/>
</signal>
<signal name="+15V">
<contactref element="X2" pad="5"/>
<contactref element="X2" pad="7"/>
<contactref element="X1" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="X2" pad="1"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="LP0">
<contactref element="R1" pad="2"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="LP1">
<contactref element="R2" pad="2"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="LP2">
<contactref element="R3" pad="2"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="LP3">
<contactref element="R4" pad="2"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="HP0">
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="HP1">
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="HP2">
<contactref element="R7" pad="2"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="HP3">
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="RS232_TX">
<contactref element="IC2" pad="10"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="RS232_RX">
<contactref element="IC2" pad="9"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="JP4" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="U$13" pad="15"/>
<contactref element="IC2" pad="20"/>
<contactref element="U$10" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="JP4" pad="3"/>
<contactref element="R18" pad="2"/>
<contactref element="U$13" pad="16"/>
<contactref element="IC2" pad="19"/>
<contactref element="U$10" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="SV2" pad="3"/>
<contactref element="JP6" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="MISO">
<contactref element="SV2" pad="1"/>
<contactref element="JP6" pad="3"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="SV2" pad="4"/>
<contactref element="JP6" pad="4"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="SS">
<contactref element="JP6" pad="5"/>
<contactref element="IC2" pad="44"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="+5V">
<contactref element="R100" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="C100" pad="+"/>
<contactref element="C5" pad="1"/>
<contactref element="C101" pad="+"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="U$13" pad="2"/>
<contactref element="IC2" pad="17"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="38"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP8" pad="11"/>
<contactref element="C20" pad="+"/>
<contactref element="C21" pad="+"/>
<contactref element="X7" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="U$10" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R39" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="R44" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="SJ3" pad="2"/>
<contactref element="SJ4" pad="2"/>
<contactref element="SJ6" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="29"/>
</signal>
<signal name="RESET">
<contactref element="SV2" pad="5"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="SV2" pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$500">
<contactref element="R100" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="U$11" pad="+"/>
<contactref element="U$13" pad="14"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$20">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$32">
<contactref element="JP6" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="C11" pad="+"/>
<contactref element="U$16" pad="2"/>
<contactref element="U$17" pad="2"/>
<contactref element="U$18" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="X6" pad="2"/>
<contactref element="U$24" pad="2"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="U$18" pad="3"/>
<contactref element="X8" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="U$17" pad="3"/>
<contactref element="X8" pad="4"/>
</signal>
<signal name="N$41">
<contactref element="U$16" pad="3"/>
<contactref element="X8" pad="6"/>
</signal>
<signal name="N$44">
<contactref element="R23" pad="2"/>
<contactref element="U$16" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="R24" pad="2"/>
<contactref element="U$17" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$46">
<contactref element="R25" pad="2"/>
<contactref element="U$18" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="LPHS0">
<contactref element="IC3" pad="4"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="LPHS1">
<contactref element="IC3" pad="3"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="LPHS2">
<contactref element="IC3" pad="2"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R26" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R27" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="R28" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="A7">
<contactref element="IC2" pad="30"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="A6">
<contactref element="IC2" pad="31"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="A5">
<contactref element="IC2" pad="32"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="A4">
<contactref element="IC2" pad="33"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="RS232_INT_TX">
<contactref element="IC2" pad="12"/>
<contactref element="IC5" pad="11"/>
</signal>
<signal name="RS232_INT_RX">
<contactref element="IC2" pad="11"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="5V_DISP">
<contactref element="C13" pad="1"/>
<contactref element="IC5" pad="16"/>
<contactref element="C22" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="A3">
<contactref element="IC2" pad="34"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="A2">
<contactref element="IC2" pad="35"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="A1">
<contactref element="IC2" pad="36"/>
<contactref element="JP8" pad="8"/>
</signal>
<signal name="A0">
<contactref element="IC2" pad="37"/>
<contactref element="JP8" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="C14" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="9"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="IC2" pad="26"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="IC2" pad="25"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="N$60">
<contactref element="LED8" pad="C"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$61">
<contactref element="LED9" pad="C"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$62">
<contactref element="LED8" pad="A"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$63">
<contactref element="LED9" pad="A"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="IC1" pad="17"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="R40" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$64">
<contactref element="U$21" pad="3"/>
<contactref element="IC1" pad="16"/>
<contactref element="X9" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="U$9" pad="3"/>
<contactref element="IC1" pad="15"/>
<contactref element="X9" pad="3"/>
</signal>
<signal name="N$98">
<contactref element="C34" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="X9" pad="M1"/>
</signal>
<signal name="N$6">
<contactref element="U$13" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="IC2" pad="40"/>
<contactref element="JP8" pad="12"/>
</signal>
<signal name="N$48">
<contactref element="IC2" pad="41"/>
<contactref element="JP8" pad="13"/>
</signal>
<signal name="N$49">
<contactref element="IC2" pad="42"/>
<contactref element="JP8" pad="14"/>
</signal>
<signal name="N$50">
<contactref element="IC2" pad="43"/>
<contactref element="JP8" pad="15"/>
</signal>
<signal name="N$57">
<contactref element="U$24" pad="3"/>
<contactref element="X8" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="R36" pad="2"/>
<contactref element="U$24" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="LPHS3">
<contactref element="IC3" pad="1"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="+5V/1">
<contactref element="U$22" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="U$21" pad="1"/>
<contactref element="U$9" pad="1"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="4"/>
<contactref element="C18" pad="1"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="Q4" pad="1"/>
<contactref element="R37" pad="1"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$43">
</signal>
<signal name="N$56">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$79">
</signal>
<signal name="N$80">
</signal>
<signal name="N$81">
</signal>
<signal name="N$82">
</signal>
<signal name="N$83">
</signal>
<signal name="N$84">
</signal>
<signal name="N$85">
</signal>
<signal name="N$86">
</signal>
<signal name="N$87">
</signal>
<signal name="N$88">
</signal>
<signal name="N$89">
</signal>
<signal name="N$90">
</signal>
<signal name="N$93">
</signal>
<signal name="N$95">
</signal>
<signal name="N$96">
</signal>
<signal name="N$97">
</signal>
<signal name="N$99">
</signal>
<signal name="N$100">
</signal>
<signal name="N$101">
</signal>
<signal name="N$102">
</signal>
<signal name="N$103">
</signal>
<signal name="N$104">
</signal>
<signal name="N$109">
</signal>
<signal name="N$110">
</signal>
<signal name="N$111">
</signal>
<signal name="N$112">
</signal>
<signal name="N$113">
</signal>
<signal name="N$114">
</signal>
<signal name="N$115">
</signal>
<signal name="N$116">
</signal>
<signal name="N$117">
</signal>
<signal name="N$118">
</signal>
<signal name="N$119">
</signal>
<signal name="N$120">
</signal>
<signal name="N$121">
</signal>
<signal name="N$122">
</signal>
<signal name="N$123">
</signal>
<signal name="N$124">
</signal>
<signal name="N$125">
</signal>
<signal name="N$126">
</signal>
<signal name="N$127">
</signal>
<signal name="N$128">
</signal>
<signal name="N$129">
</signal>
<signal name="N$130">
</signal>
<signal name="N$135">
</signal>
<signal name="N$136">
</signal>
<signal name="N$137">
</signal>
<signal name="N$138">
</signal>
<signal name="N$139">
</signal>
<signal name="N$140">
</signal>
<signal name="N$141">
</signal>
<signal name="N$142">
</signal>
<signal name="N$143">
</signal>
<signal name="N$144">
</signal>
<signal name="N$145">
</signal>
<signal name="N$146">
</signal>
<signal name="N$147">
</signal>
<signal name="N$148">
</signal>
<signal name="N$149">
</signal>
<signal name="N$150">
</signal>
<signal name="N$151">
</signal>
<signal name="N$152">
</signal>
<signal name="N$153">
</signal>
<signal name="N$154">
</signal>
<signal name="N$159">
</signal>
<signal name="N$160">
</signal>
<signal name="N$161">
</signal>
<signal name="N$162">
</signal>
<signal name="N$163">
</signal>
<signal name="N$164">
</signal>
<signal name="N$165">
</signal>
<signal name="N$166">
</signal>
<signal name="N$167">
</signal>
<signal name="N$168">
</signal>
<signal name="N$169">
</signal>
<signal name="N$170">
</signal>
<signal name="N$171">
</signal>
<signal name="N$172">
</signal>
<signal name="N$173">
</signal>
<signal name="N$174">
</signal>
<signal name="N$175">
</signal>
<signal name="N$176">
</signal>
<signal name="N$177">
</signal>
<signal name="N$180">
</signal>
<signal name="N$181">
</signal>
<signal name="N$182">
</signal>
<signal name="N$183">
</signal>
<signal name="N$184">
</signal>
<signal name="N$185">
</signal>
<signal name="N$186">
</signal>
<signal name="N$187">
</signal>
<signal name="N$188">
</signal>
<signal name="N$189">
</signal>
<signal name="N$190">
</signal>
<signal name="N$191">
</signal>
<signal name="N$192">
</signal>
<signal name="N$105">
</signal>
<signal name="N$194">
<contactref element="IC3" pad="28"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="N$195">
<contactref element="IC3" pad="25"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="N$196">
<contactref element="IC3" pad="24"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="N$197">
<contactref element="IC3" pad="23"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="N$198">
<contactref element="IC3" pad="22"/>
<contactref element="JP7" pad="6"/>
</signal>
<signal name="N$199">
<contactref element="IC3" pad="21"/>
<contactref element="JP7" pad="7"/>
</signal>
<signal name="N$106">
<contactref element="X9" pad="1"/>
<contactref element="R40" pad="2"/>
<contactref element="U$22" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="IC5" pad="13"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$36">
<contactref element="IC5" pad="14"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="IC5" pad="2"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$107">
<contactref element="IC5" pad="6"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="IC5" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$131">
<contactref element="IC5" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$132">
<contactref element="C15" pad="1"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="N$133">
<contactref element="C15" pad="2"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="N$134">
<contactref element="U$10" pad="9"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$155">
<contactref element="U$10" pad="8"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$156">
<contactref element="U$10" pad="7"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$157">
<contactref element="U$10" pad="6"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="#LDAC">
<contactref element="U$10" pad="4"/>
<contactref element="R39" pad="2"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="RDY/#BSY">
<contactref element="U$10" pad="5"/>
<contactref element="R30" pad="2"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="N$54">
<contactref element="IC2" pad="27"/>
<contactref element="R44" pad="1"/>
<contactref element="C23" pad="2"/>
</signal>
<signal name="#DTR">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="#CTS">
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
