<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.24" y2="0" width="0" layer="20"/>
<wire x1="15.24" y1="0" x2="15.24" y2="19.05" width="0" layer="20"/>
<wire x1="15.24" y1="19.05" x2="14.478" y2="19.812" width="0" layer="20"/>
<wire x1="14.478" y1="19.812" x2="14.478" y2="21.844" width="0" layer="20"/>
<wire x1="14.478" y1="21.844" x2="15.24" y2="22.606" width="0" layer="20"/>
<wire x1="15.24" y1="22.606" x2="15.24" y2="50.8" width="0" layer="20"/>
<wire x1="15.24" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="0" width="0" layer="20"/>
<text>MAX10
cdpga h3
Buheitel
2022/3 A</text>
</plain>
<libraries>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE06-2W">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gustl_RCL">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="L0805">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0402">
<description>&lt;b&gt;Chip RESISTOR 0402 EIA (1005 Metric)&lt;/b&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="L0402">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="gustl_MP2162A">
<packages>
<package name="QFN_8_2X1P5_MPS">
</package>
</packages>
</library>
<library name="gustl_U262-161N-4BVC11">
<packages>
<package name="U262-161N-4BVC11">
</package>
</packages>
</library>
<library name="gustl_SMDLED">
<packages>
<package name="SMDLED0402">
</package>
</packages>
</library>
<library name="gustl_93LC56BT">
<packages>
<package name="SOT95P270X145-6N">
</package>
</packages>
</library>
<library name="gustl_FTDI">
<description>&lt;html&gt;
&lt;head&gt;
&lt;/head&gt;
&lt;body&gt;
&lt;h2&gt;&lt;b&gt;USB-Controllers from Future Technology Devices International Ltd.&lt;/b&gt;&lt;/h2&gt;
&lt;h2 align=center&gt;&lt;a href="http://www.ftdichip.com/"&gt;www.ftdichip.com&lt;/a&gt;&lt;/h2&gt;
&lt;p align=right&gt; Version 4.00 17&lt;supth&lt;/sup&gt; July 2010&lt;/p&gt;
&lt;p&gt;Based on the source of the libraries ftdi3.lbr and ft2232c.lbr.&lt;/p&gt;
&lt;p&gt;With new FTxxxR Types. Old AM Types (first generation) are not included.&lt;/p&gt;
&lt;P&gt;Updated to make consistent symbol style, and other updates like same prefix for all devices, and improve this page.&lt;/P&gt;
&lt;p&gt;Includes the following controller:&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;FT232BL , FT245BL (2nd generation)&lt;/li&gt;
  &lt;li&gt;FT2232C (3rd generation)&lt;/li&gt;
  &lt;li&gt;FT232RL , FT232RQ, FT245RL, FT245RQ (4th generation)&lt;/li&gt;
  &lt;li&gt;FT2232C&lt;/li&gt;
  &lt;li&gt;FT2232D (4th generation)&lt;/li&gt;
  &lt;li&gt;FT2232H  USB 2.0 64 pin device&lt;/li&gt;
  &lt;li&gt;Viniculum host controller chip&lt;/li&gt;
&lt;/ul&gt;
&lt;P&gt;Originally by B.Redemann, www.b-redemann.de&lt;/P&gt;
&lt;P&gt;Updated Paul Carpenter, &lt;B&gt;PC Services&lt;/B&gt; &lt;a href="http://www.pcserviceselectronics.co.uk/"&gt;www.pcserviceselectronics.co.uk&lt;/a&gt;&lt;/P&gt;
&lt;/body&gt;
&lt;/html&gt;</description>
<packages>
<package name="LQFP64">
<description>&lt;b&gt;LQFP-64 package&lt;/b&gt;&lt;p&gt;
10x10 mm case, 0.5 mm lead pitch</description>
</package>
</packages>
</library>
<library name="gustl_SN74HC595">
<packages>
<package name="X1QFN_16">
</package>
</packages>
</library>
<library name="gustl_cdpga_h3">
<packages>
<package name="CDPGA_H3">
</package>
</packages>
</library>
<library name="gustl_SRV05-4">
<packages>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
</packages>
</library>
<library name="gustl_CM1213A-02SR">
<packages>
<package name="SOT143-R">
<description>&lt;b&gt;SOT143 / SOT143B Reflow soldering&lt;/b&gt;&lt;p&gt;
Source:  Philips SC01_Mounting_1996.pdf / BAS70_1PS7XSB70_SER_8.pdf</description>
</package>
</packages>
</library>
<library name="gustl_NX3225">
<packages>
<package name="NX3225">
</package>
</packages>
</library>
<library name="gustl_AD7689">
<packages>
<package name="QFN20_4X4">
<description>&lt;b&gt;QFN 4x4 mm&lt;/b&gt;&lt;p&gt;
Source: http://www.hittite.com/product_info/product_specs/dividersdetectors/hmc394lp4.pdf</description>
</package>
</packages>
</library>
<library name="resistor-dil">
<description>&lt;b&gt;Resistors in DIL Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4X0402ARV341">
<description>&lt;b&gt;Array chip resistor&lt;/b&gt; size 4 × 0402&lt;p&gt;
Source: http://docs-europe.electrocomponents.com/webdocs/0114/0900766b80114d99.pdf</description>
</package>
</packages>
</library>
<library name="gustl_TPS60151">
<packages>
<package name="WSON_6_2MM_X_2MM">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LGA-14">
<description>&lt;h3&gt;14-Pin LGA (3 x 5 x 1 mm) (1:1 footprint)&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL345.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 14&lt;/li&gt;
&lt;li&gt;Area: 3.0 x 5.0 x 1.0 mm&lt;/li&gt;
&lt;li&gt;Pitch: 0.8 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;ADXL345&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="BTN_CK_KSS">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WS2812B">
<description>&lt;h3&gt;WS2812B&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Size: 5.0 x 5.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"&gt;WS2812B&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;WS2812B&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="gustl_Single_Buffer_74LVC1G17">
<description>SINGLE SCHMITT-TRIGGER BUFFER</description>
<packages>
<package name="SC70-5">
<description>&lt;b&gt;SMT SC70-5&lt;/b&gt;&lt;p&gt;
SOT353 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV8" library="con-lsta" package="FE06-2W" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="gustl_RCL" package="C0805" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C117" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L6" library="gustl_RCL" package="L0805" value="1u_2.xA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="gustl_RCL" package="R0402" value="200k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="gustl_RCL" package="R0402" value="44k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C119" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C129" library="gustl_RCL" package="C0603" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="gustl_MP2162A" package="QFN_8_2X1P5_MPS" value="MP2162GQH-Z">
<attribute name="COPYRIGHT" value="Copyright (C) 2021 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MP2162GQH-Z"/>
<attribute name="MFR_NAME" value="Monolithic Power Systems"/>
</element>
<element name="C6" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="gustl_U262-161N-4BVC11" package="U262-161N-4BVC11" value="U262-161N-4BVC11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="gustl_RCL" package="R0402" value="5.1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="gustl_RCL" package="R0402" value="5.1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="gustl_RCL" package="R0402" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="gustl_RCL" package="R0402" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="LED1" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="Q1" library="gustl_NX3225" package="NX3225" value="NX3225"/>
<element name="C13" library="gustl_RCL" package="C0402" value="27p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="gustl_RCL" package="C0402" value="27p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="gustl_RCL" package="R0402" value="12k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R76" library="gustl_RCL" package="R0402" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="gustl_RCL" package="L0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="gustl_RCL" package="L0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C99" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="gustl_93LC56BT" package="SOT95P270X145-6N" value="93LC56BT-I/OT">
<attribute name="MPN" value="93LC56BT-I/OT"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="30H4760"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="gustl_RCL" package="R0402" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="gustl_RCL" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="IC1" library="gustl_FTDI" package="LQFP64" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="gustl_RCL" package="L0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="gustl_RCL" package="C0402" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="gustl_RCL" package="C0603" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="gustl_RCL" package="C0402" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="gustl_cdpga_h3" package="CDPGA_H3" value="CDPGA_H3">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="U$9" library="gustl_SRV05-4" package="SOT23-6" value="SRV05-4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="gustl_SRV05-4" package="SOT23-6" value="SRV05-4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="gustl_CM1213A-02SR" package="SOT143-R" value="CM1213A-02SR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="gustl_RCL" package="C0805" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="gustl_AD7689" package="QFN20_4X4" value="AD7689">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$20" library="gustl_SN74HC595" package="X1QFN_16" value="SN74HC595B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$22" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$23" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$24" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$25" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$26" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$27" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$28" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$29" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="RN1" library="resistor-dil" package="4X0402ARV341" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-dil" package="4X0402ARV341" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U$30" library="gustl_SN74HC595" package="X1QFN_16" value="SN74HC595B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$31" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$32" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$33" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$34" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$35" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$36" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$37" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="U$38" library="gustl_SMDLED" package="SMDLED0402" value="SMDLED"/>
<element name="RN3" library="resistor-dil" package="4X0402ARV341" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="RN4" library="resistor-dil" package="4X0402ARV341" value="4.7k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="gustl_TPS60151" package="WSON_6_2MM_X_2MM" value="TPS60151">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gustl_RCL" package="C0603" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="gustl_RCL" package="L0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gustl_RCL" package="C0402" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="gustl_RCL" package="C0402" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Sensors" package="LGA-14" value="ADXL345">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09097"/>
<attribute name="SF_ID" value="SEN-09045"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="gustl_RCL" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="gustl_RCL" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="gustl_RCL" package="C0402" value="470n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="adafruit" package="BTN_CK_KSS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="gustl_RCL" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="gustl_RCL" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="gustl_RCL" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="gustl_Single_Buffer_74LVC1G17" package="SC70-5" value="74LVC1G17SE-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="gustl_RCL" package="C0603" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="gustl_RCL" package="C0603" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="gustl_RCL" package="C0402" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="gustl_RCL" package="C0805" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C117" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="C119" pad="2"/>
<contactref element="C129" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="51"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="35"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="25"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R39" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="10"/>
<contactref element="U$7" pad="SHIELD_1"/>
<contactref element="U$7" pad="SHIELD_2"/>
<contactref element="U$7" pad="B1A12"/>
<contactref element="U$7" pad="SHIELD_3"/>
<contactref element="U$7" pad="A1B12"/>
<contactref element="U$7" pad="SHIELD_4"/>
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C99" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="Q1" pad="4"/>
<contactref element="C23" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="U$11" pad="1"/>
<contactref element="C39" pad="2"/>
<contactref element="U$8" pad="P$15"/>
<contactref element="C18" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U$3" pad="5" route="any" routetag="G$1.GND"/>
<contactref element="U$3" pad="EXP" route="any" routetag="G$1.GND"/>
<contactref element="U$3" pad="4" route="any" routetag="G$1.GND"/>
<contactref element="U$3" pad="10"/>
<contactref element="U$25" pad="C-"/>
<contactref element="U$26" pad="C-"/>
<contactref element="U$27" pad="C-"/>
<contactref element="U$28" pad="C-"/>
<contactref element="U$29" pad="C-"/>
<contactref element="U$22" pad="C-"/>
<contactref element="U$23" pad="C-"/>
<contactref element="U$24" pad="C-"/>
<contactref element="U$34" pad="C-"/>
<contactref element="U$35" pad="C-"/>
<contactref element="U$36" pad="C-"/>
<contactref element="U$37" pad="C-"/>
<contactref element="U$38" pad="C-"/>
<contactref element="U$31" pad="C-"/>
<contactref element="U$32" pad="C-"/>
<contactref element="U$33" pad="C-"/>
<contactref element="U$20" pad="13"/>
<contactref element="U$20" pad="8"/>
<contactref element="U$20" pad="EXP"/>
<contactref element="U$30" pad="13"/>
<contactref element="U$30" pad="8"/>
<contactref element="U$30" pad="EXP"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="PAD"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C8" pad="2"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="C19" pad="2"/>
<contactref element="U$9" pad="2"/>
<contactref element="U$10" pad="2"/>
<contactref element="D1" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="C24" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="SV8" pad="3"/>
<contactref element="SV8" pad="4"/>
<contactref element="C34" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C37" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U$4" pad="6"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="L4" pad="2"/>
<contactref element="IC1" pad="42"/>
<contactref element="IC1" pad="56"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="50"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="LED1" pad="A+"/>
<contactref element="LED5" pad="A+"/>
<contactref element="R76" pad="2"/>
<contactref element="LED2" pad="A+"/>
<contactref element="L6" pad="1"/>
<contactref element="C119" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C129" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U$8" pad="P$9"/>
<contactref element="C39" pad="1"/>
<contactref element="U$3" pad="15"/>
<contactref element="U$20" pad="10"/>
<contactref element="U$20" pad="16"/>
<contactref element="U$30" pad="10"/>
<contactref element="U$30" pad="16"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="12"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="C57" pad="1"/>
<contactref element="SV8" pad="2"/>
<contactref element="SV8" pad="1"/>
<contactref element="U$9" pad="5"/>
<contactref element="U$10" pad="5"/>
<contactref element="C24" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="PMOD_3">
<contactref element="SV8" pad="5"/>
<contactref element="U$3" pad="19"/>
<contactref element="U$10" pad="4"/>
<contactref element="U$8" pad="P$8"/>
</signal>
<signal name="PMOD_2">
<contactref element="SV8" pad="7"/>
<contactref element="U$3" pad="18"/>
<contactref element="U$10" pad="1"/>
<contactref element="U$8" pad="P$4"/>
</signal>
<signal name="PMOD_1">
<contactref element="SV8" pad="9"/>
<contactref element="U$3" pad="17"/>
<contactref element="U$9" pad="1"/>
<contactref element="U$8" pad="P$6"/>
</signal>
<signal name="PMOD_0">
<contactref element="SV8" pad="11"/>
<contactref element="U$3" pad="16"/>
<contactref element="U$9" pad="6"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="PMOD_4">
<contactref element="SV8" pad="12"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$9" pad="4"/>
<contactref element="U$8" pad="P$2"/>
</signal>
<signal name="PMOD_5">
<contactref element="SV8" pad="10"/>
<contactref element="U$3" pad="7"/>
<contactref element="U$9" pad="3"/>
<contactref element="U$8" pad="P$5"/>
</signal>
<signal name="PMOD_6">
<contactref element="SV8" pad="8"/>
<contactref element="U$3" pad="8"/>
<contactref element="U$10" pad="3"/>
<contactref element="U$8" pad="P$3"/>
</signal>
<signal name="PMOD_7">
<contactref element="SV8" pad="6"/>
<contactref element="U$3" pad="9"/>
<contactref element="U$10" pad="6"/>
<contactref element="U$8" pad="P$7"/>
</signal>
<signal name="N$49">
<contactref element="L6" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$51">
<contactref element="R6" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="R7" pad="2"/>
<contactref element="LED1" pad="C-"/>
</signal>
<signal name="USB-">
<contactref element="U$7" pad="A7"/>
<contactref element="U$7" pad="B7"/>
<contactref element="IC1" pad="7"/>
<contactref element="U$11" pad="2"/>
</signal>
<signal name="1.8V_FT2232H">
<contactref element="IC1" pad="49"/>
<contactref element="C25" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C99" pad="1"/>
<contactref element="IC1" pad="64"/>
<contactref element="IC1" pad="37"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$20">
<contactref element="U$7" pad="B5"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="U$7" pad="A5"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="USB+">
<contactref element="U$7" pad="B6"/>
<contactref element="U$7" pad="A6"/>
<contactref element="IC1" pad="8"/>
<contactref element="U$11" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="R14" pad="1"/>
<contactref element="LED2" pad="C-"/>
</signal>
<signal name="N$35">
<contactref element="R14" pad="2"/>
<contactref element="IC1" pad="60"/>
</signal>
<signal name="N$36">
<contactref element="IC1" pad="14"/>
<contactref element="R76" pad="1"/>
</signal>
<signal name="EEDATA">
<contactref element="U$4" pad="3"/>
<contactref element="R13" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="IC1" pad="61"/>
</signal>
<signal name="EECLK">
<contactref element="U$4" pad="4"/>
<contactref element="R10" pad="2"/>
<contactref element="IC1" pad="62"/>
</signal>
<signal name="EECS">
<contactref element="U$4" pad="5"/>
<contactref element="IC1" pad="63"/>
</signal>
<signal name="N$37">
<contactref element="U$4" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="9"/>
<contactref element="L4" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C31" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="IC1" pad="4"/>
<contactref element="L3" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C29" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="IC1" pad="54"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="R8" pad="2"/>
<contactref element="LED5" pad="C-"/>
</signal>
<signal name="N$45">
<contactref element="R8" pad="1"/>
<contactref element="IC1" pad="55"/>
</signal>
<signal name="TCK">
<contactref element="IC1" pad="16"/>
<contactref element="R4" pad="1"/>
<contactref element="U$8" pad="P$18"/>
</signal>
<signal name="TDI">
<contactref element="IC1" pad="17"/>
<contactref element="R5" pad="1"/>
<contactref element="U$8" pad="P$19"/>
</signal>
<signal name="TDO">
<contactref element="IC1" pad="18"/>
<contactref element="R15" pad="1"/>
<contactref element="U$8" pad="P$20"/>
</signal>
<signal name="TXD">
<contactref element="IC1" pad="38"/>
<contactref element="U$8" pad="P$22"/>
</signal>
<signal name="N$4">
<contactref element="U$7" pad="B4A9"/>
<contactref element="U$7" pad="A4B9"/>
<contactref element="L5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$11" pad="4"/>
</signal>
<signal name="5V_USB">
<contactref element="L5" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="C117" pad="1"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="3"/>
<contactref element="Q1" pad="3"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="TMS">
<contactref element="IC1" pad="19"/>
<contactref element="R16" pad="1"/>
<contactref element="U$8" pad="P$17"/>
</signal>
<signal name="RXD">
<contactref element="IC1" pad="39"/>
<contactref element="U$8" pad="P$21"/>
</signal>
<signal name="5V">
<contactref element="C17" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U$3" pad="20"/>
<contactref element="U$3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C10" pad="1"/>
<contactref element="U$3" pad="3"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="2"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U$29" pad="A+"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="U$22" pad="A+"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$23" pad="A+"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="U$24" pad="A+"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$42">
<contactref element="U$25" pad="A+"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="U$26" pad="A+"/>
<contactref element="RN2" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="U$27" pad="A+"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="U$28" pad="A+"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="LED8">
<contactref element="U$20" pad="7"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="LED1">
<contactref element="U$20" pad="15"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="LED2">
<contactref element="U$20" pad="1"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="LED3">
<contactref element="U$20" pad="2"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="LED4">
<contactref element="U$20" pad="3"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="LED5">
<contactref element="U$20" pad="4"/>
<contactref element="RN2" pad="8"/>
</signal>
<signal name="LED6">
<contactref element="U$20" pad="5"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="LED7">
<contactref element="U$20" pad="6"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="N$82">
<contactref element="U$38" pad="A+"/>
<contactref element="RN4" pad="4"/>
</signal>
<signal name="N$86">
<contactref element="U$31" pad="A+"/>
<contactref element="RN3" pad="1"/>
</signal>
<signal name="N$87">
<contactref element="U$32" pad="A+"/>
<contactref element="RN3" pad="2"/>
</signal>
<signal name="N$88">
<contactref element="U$33" pad="A+"/>
<contactref element="RN3" pad="3"/>
</signal>
<signal name="N$89">
<contactref element="U$34" pad="A+"/>
<contactref element="RN3" pad="4"/>
</signal>
<signal name="N$93">
<contactref element="U$35" pad="A+"/>
<contactref element="RN4" pad="1"/>
</signal>
<signal name="N$98">
<contactref element="U$36" pad="A+"/>
<contactref element="RN4" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="U$37" pad="A+"/>
<contactref element="RN4" pad="3"/>
</signal>
<signal name="LED16">
<contactref element="U$30" pad="7"/>
<contactref element="RN4" pad="5"/>
</signal>
<signal name="LED9">
<contactref element="U$30" pad="15"/>
<contactref element="RN3" pad="8"/>
</signal>
<signal name="LED10">
<contactref element="U$30" pad="1"/>
<contactref element="RN3" pad="7"/>
</signal>
<signal name="LED11">
<contactref element="U$30" pad="2"/>
<contactref element="RN3" pad="6"/>
</signal>
<signal name="LED12">
<contactref element="U$30" pad="3"/>
<contactref element="RN3" pad="5"/>
</signal>
<signal name="LED13">
<contactref element="U$30" pad="4"/>
<contactref element="RN4" pad="8"/>
</signal>
<signal name="LED14">
<contactref element="U$30" pad="5"/>
<contactref element="RN4" pad="7"/>
</signal>
<signal name="LED15">
<contactref element="U$30" pad="6"/>
<contactref element="RN4" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="U$20" pad="9"/>
<contactref element="U$30" pad="14"/>
</signal>
<signal name="SR_SER_3.3V">
<contactref element="U$20" pad="14"/>
<contactref element="U$8" pad="P$10"/>
</signal>
<signal name="SR_RCLK_3.3V">
<contactref element="U$20" pad="12"/>
<contactref element="U$30" pad="12"/>
<contactref element="U$8" pad="P$11"/>
</signal>
<signal name="SR_SRCLK_3.3V">
<contactref element="U$20" pad="11"/>
<contactref element="U$30" pad="11"/>
<contactref element="U$8" pad="P$12"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="U$2" pad="3"/>
<contactref element="L1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="ACCEL_SDA">
<contactref element="U1" pad="13"/>
<contactref element="R1" pad="1"/>
<contactref element="U$8" pad="P$14"/>
</signal>
<signal name="ACCEL_SCL">
<contactref element="U1" pad="14"/>
<contactref element="R2" pad="1"/>
<contactref element="U$8" pad="P$13"/>
</signal>
<signal name="BTN">
<contactref element="SW1" pad="P$1"/>
<contactref element="C19" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U$8" pad="P$16"/>
</signal>
<signal name="ADC_CNV">
<contactref element="U$3" pad="11"/>
<contactref element="U$8" pad="P$28"/>
</signal>
<signal name="ADC_SCK">
<contactref element="U$3" pad="13"/>
<contactref element="U$8" pad="P$26"/>
</signal>
<signal name="ADC_MOSI">
<contactref element="U$3" pad="12"/>
<contactref element="U$8" pad="P$27"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="WS2812B">
<contactref element="U$1" pad="2"/>
<contactref element="U$8" pad="P$23"/>
</signal>
<signal name="ADC_MISO">
<contactref element="U$3" pad="14"/>
<contactref element="U$8" pad="P$24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
