<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="DIL14">
</package>
</packages>
<symbols>
<symbol name="TL497-ST">
<pin name="AN"/>
<pin name="CAT"/>
<pin name="COL" direction="out"/>
<pin name="COMP"/>
<pin name="EMIT" direction="out"/>
<pin name="FREQ"/>
<pin name="GND" direction="in"/>
<pin name="ILIM"/>
<pin name="INH"/>
<pin name="SUBST" direction="in"/>
<pin name="VCC" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TL497" prefix="IC" uservalue="yes">
<description>TL497 from Atari ST Computer</description>
<gates>
<gate name="G$1" symbol="TL497-ST"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="AN" pad="7"/>
<connect gate="G$1" pin="CAT" pad="6"/>
<connect gate="G$1" pin="COL" pad="10"/>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="EMIT" pad="8"/>
<connect gate="G$1" pin="FREQ" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ILIM" pad="13"/>
<connect gate="G$1" pin="INH" pad="2"/>
<connect gate="G$1" pin="SUBST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
