{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["AVR128-DA","AVR128-DB","AVR64-DD-32-28","AVR16|32-DD-28-32","AVR4808|4809-28-32-40-48"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"AVR128-DA","index":0,"n_rows":1090,"n_cols":30,"rows_kept":1090,"flags":["formulas_cached_only"]}
["AVR128-DA-28/32/48/64","[ 04 – 2023 ]"]
["Peripherals and Architecture"]
[]
[]
["Table 8-1. Peripheral Address Map",{"$nulls":20},"Table","8-3. Interrupt Vector Mapping"]
[{"$nulls":21},"***********************************************************************************************************************************************************************"]
["Base Address ","Name"," Description","Offset","Name","Bit 7","Bit 6"," Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0",null,"Pin 28","Pin 32","Pin 48","Pin 64",{"$nulls":3},"Vector","Program",{"$nulls":3},"28-Pin","32-Pin","48-Pin","64-Pin"]
[{"$nulls":21},"Number","Address","Peripheral","Description"]
["0x0000","VPORTA","Virtual Port A","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},0,"0x00","RESET","Reset",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},1,"0x02","NMI","Non-Maskable Interrupt available for CRCSCAN",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},2,"0x04","BOD VLM","Voltage Level Monitor Interrupt",null,"X","X","X","X"]
[{"$nulls":21},3,"0x06","RTC CNT","Real-Time Counter Overflow or Compare Match Interrupt",null,"X","X","X","X"]
["0x0004","VPORTB","Virtual Port B","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},4,"0x08","RTC PIT","Real-Time Counter Periodic Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},5,"0x0A","CCL CCL","Configurable Custom Logic Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},6,"0x0C","PORTA PORT","PORTA External interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},7,"0x0E","TCA0_OVF ","Normal: Timer/Counter Type A Overflow Interrupt ",null,"X","X","X","X"]
[{"$nulls":21},7,"0x0E","TCA0 LUNF","Split: Timer/Counter Type A Low Underflow Interrupt",null,"X","X","X","X"]
["0x0008","VPORTC","Virtual Port C","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},8,"0x10","TCA0 HUNF","Normal: Unused",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},8,"0x10","TCA0 HUNF","Split: Timer/Counter Type A High Underflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},9,"0x12","TCA0 CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},9,"0x12","TCA0 LCMP0","Split: Timer/Counter Type A Low Compare 0 Interrupt",null,"X","X","X","X"]
[{"$nulls":21},10,"0x14","TCA0 CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"X","X","X","X"]
["0x000C","VPORTD","Virtual Port D","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},10,"0x14","TCA0 LCMP1","Split: Timer/Counter Type A Low Compare 1 Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},11,"0x16","TCA0 CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},11,"0x16","TCA0 LCMP2","Split: Timer/Counter Type A Low Compare 2 Interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},12,"0x18","TCB0 INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":21},13,"0x1A","TCB1 INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X","X","X"]
["0x0010","VPORTE","Virtual Port E","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},14,"0x1C","TCD0 OVF","Timer Counter Type D Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},15,"0x1E","TCD0 TRIG","Timer Counter Type D Trigger Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},16,"0x20","TWI0 TWIS","Two-Wire Interface Client Interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},17,"0x22","TWI0 TWIM","Two-Wire Interface Host Interrupt",null,"X","X","X","X"]
[{"$nulls":21},18,"0x24","SPI0 INT","Serial Peripheral Interface Interrupt",null,"X","X","X","X"]
["0x0014","VPORTF","Virtual Port F","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},19,"0x26","USART0 RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},20,"0x28","USART0 DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},21,"0x2A","USART0 TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},22,"0x2C","PORTD PORT","PORTD External Interrupt",null,"X","X","X","X"]
[{"$nulls":21},23,"0x2E","AC0 AC","Analog Comparator Interrupt",null,"X","X","X","X"]
["0x0018","VPORTG","Virtual Port G","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":3},24,"0x30","ADC0 RESRDY","Analog-to-Digital Converter Result Ready Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":3},25,"0x32","ADC0 WCMP","Analog-to-Digital Converter Window Compare Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":3},26,"0x34","ZCD0 ZCD","Zero-Cross Interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":3},27,"0x36","PTC PTC","Peripheral Touch Controller Interrupt",null,"X","X","X","X"]
[{"$nulls":16}," ",{"$nulls":4},28,"0x38","AC1 AC","Analog Comparator Interrupt",null,"X","X","X","X"]
["0x001C","GPR","General Purpose Registers","0x00","GPR0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},29,"0x3A","PORTC PORT","PORTC External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","GPR1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},30,"0x3C","TCB2 INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","GPR2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},31,"0x3E","USART1 RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
["ref",null,null,"0x03","GPR3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},32,"0x40","USART1 DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":21},33,"0x42","USART1 TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
["0x0030","CPU","CPU","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},34,"0x44","PORTF PORT","PORTF External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},35,"0x46","NVMCTRL EE","Nonvolatile Memory Controller EEPROM Ready Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},36,"0x48","SPI1 INT","Serial Peripheral Interface Interrupt",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},37,"0x4A","USART2 RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CCP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},38,"0x4C","USART2 DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},39,"0x4E","USART2 TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},40,"0x50","AC2 AC","Analog Comparator Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},41,"0x52","TCB3 INT","Timer Counter Type B Capture/Overflow Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},42,"0x54","TWI1 TWIS","Two-Wire Interface Client Interrupt",null,"-","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},43,"0x56","TWI1 TWIM","Two-Wire Interface Host Interrupt",null,"-","X","X","X"]
[{"$nulls":3},"0x0B","RAMPZ","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},44,"0x58","PORTB PORT","PORTB External Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},45,"0x5A","PORTE PORT","PORTE External Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","SP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},46,"0x5C","TCA1_OVF ","Normal: Timer/Counter Type A Overflow Interrupt ",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X",{"$nulls":3},46,"0x5C","TCA1 LUNF","Split: Timer/Counter Type A Low Underflow Interrupt",null,"-","-","X","X"]
["ref",null,null,"0x0F","SREG","I","T","H","S","V","N","Z","C",null,"X","X","X","X",{"$nulls":3},47,"0x5E","TCA1 HUNF","Normal: Unused",null,"-","-","X","X"]
[{"$nulls":21},47,"0x5E","TCA1 HUNF","Split: Timer/Counter Type A High Underflow Interrupt",null,"-","-","X","X"]
["0x0040","RSTCTRL","Reset Controller","0x00","RSTFR","-","-","UPDIRF","SWRF","WDRF","EXTRF","BORF","PORF",{"$nulls":8},48,"0x60","TCA1 CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"-","-","X","X"]
["ref",null,null,"0x01","SWRR","-","-","-","-","-","-","-","SWRST",{"$nulls":8},48,"0x60","TCA1 LCMP0","Split: Timer/Counter Type A Low Compare 0 Interrupt",null,"-","-","X","X"]
[{"$nulls":21},49,"0x62","TCA1 CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"-","-","X","X"]
["0x0050","SLPCTRL","Sleep Controller","0x00","CTRLA","-","-","-","-","SMODE[2]","SMODE[1]","SMODE[0]","SEN",null,"X","X","X","X",{"$nulls":3},49,"0x62","TCA1 LCMP1","Split: Timer/Counter Type A Low Compare 1 Interrupt",null,"-","-","X","X"]
["ref",null,null,"0x01","VREGCTRL","-","-","HTLLEN","-","-","PMODE[2]","PMODE[1]","PMODE[0]",null,"X","X","X","X",{"$nulls":3},50,"0x64","TCA1 CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"-","-","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},50,"0x64","TCA1 LCMP2","Split: Timer/Counter Type A Low Compare 2 Interrupt",null,"-","-","X","X"]
["0x0060","CLKCTRL","Clock Controller","0x00","MCLKCTRLA","CLKOUT","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X",{"$nulls":3},51,"0x66","ZCD1 ZCD","Zero-Cross Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x01","MCLKCTRLB","-","-","-","PDIV[3]","PDIV[2]","PDIV[1]","PDIV[0]","PEN",null,"X","X","X","X",{"$nulls":3},52,"0x68","USART3 RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x02","MCLKLOCK","-","-","-","-","-","-","-","LOCKEN",null,"X","X","X","X",{"$nulls":3},53,"0x6A","USART3 DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x03","MCLKSTATUS","-","-","PLLS","EXTS","XOSC32KS","OSC32KS","OSCHFS","SOSC",null,"X","X","X","X",{"$nulls":3},54,"0x6C","USART3 TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},55,"0x6E","USART4 RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},56,"0x70","USART4 DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},57,"0x72","USART4 TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},58,"0x74","PORTG PORT","PORTG External Interrupt",null,"-","-","-","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},59,"0x76","ZCD2","ZCD Zero-Cross Interrupt ",null,"-","-","-","X"]
[{"$nulls":3},"0x08","OSCHFCTRLA","RUNSTDBY",null,"FRQSEL[3]","FRQSEL[2]","FRQSEL[1]","FRQSEL[0]",null,"AUTOTUNE",null,"X","X","X","X",{"$nulls":3},60,"0x78","TCB4 INT","Timer Counter Type B Capture/Overflow Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"0x09","OSCHFTUNE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},61,"0x7A","USART5 RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","-","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},62,"0x7C","USART5 DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},63,"0x7E","USART5 TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","PLLCTRLA","RUNSTDBY","SOURCE","-","-","-","-","MULFAC[1]","MULFAC[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x11","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x18","OSC32KCTRLA","RUNSTDBY","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x19","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1B","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
["ref",null,null,"0x1C","XOSC32KCTRLA","RUNSTDBY","-","CSUT[1]","CSUT[0]","-","SEL","LPMODE","ENABLE",null,"X","X","X","X"]
[]
["…"]
[]
["0x0080","BOD","Brown-out Detector","0x00","CTRLA","-","-","-","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","LVL[2]","LVL[1]","LVL[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","VLMCTRLA","-","-","-","-","-","-","VLMLVL[1]","VLMLVL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTCTRL","-","-","-","-","-","VLMCFG[1]","VLMCFG[0]","VLMIE",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTFLAGS","-","-","-","-","-","-","-","VLMIF",null,"X","X","X","X"]
["ref",null,null,"0x0B","STATUS","-","-","-","-","-","-","-","VLMS",null,"X","X","X","X"]
[]
["0x00A0","VREF","Voltage Reference","0x00","ADC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DAC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ref",null,null,"0x04","ACREF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X","X","X"]
[]
["0x0100","WDT","Watchdog Timer","0x00","CTRLA","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X","X","X"]
["ref",null,null,"0x01","STATUS","LOCK","-","-","-","-","-","-","SYNCBUSY",null,"X","X","X","X"]
[]
["0x0110","CPUINT","Interrupt Controller","0x00","CTRLA","-","IVSEL","CVT","-","-","-","-","LVL0RR",null,"X","X","X","X"]
[{"$nulls":3},"0x01","STATUS","NMIEX","-","-","-","-","-","LVL1EX","LVL0EX",null,"X","X","X","X"]
[{"$nulls":3},"0x02","LVL0PRI","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x03","LVL1VEC","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0120","CRCSCAN","Cyclic Redundancy Check Memory Scan","0x00","CTRLA","RESET","-","-","-","-","-","NMIEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","SRC[1:0]","SRC[1:0]",null,"X","X","X","X"]
["ref",null,null,"0x02","STATUS","-","-","-","-","-","-","OK","BUSY",null,"X","X","X","X"]
[]
["…","…"]
[]
["0x0140","RTC","Real-Time Counter","0x00","CTRLA","RUNSTDBY","PRESCALER[3]","PRESCALER[2]","PRESCALER[1]","PRESCALER[0]","CORREN","-","RTCEN",null,"X","X","X","X"]
[{"$nulls":3},"0x01","STATUS","-","-","-","-","CMPBUSY","PERBUSY","CNTBUSY","CTRLABUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","CMP","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","-","-","-","-","-","-","CMP","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CALIB","SIGN","ERROR[6]","ERROR[5]","ERROR[4]","ERROR[3]","ERROR[2]","ERROR[1]","ERROR[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CLKSEL","-","-","-","-","-","-","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PER]","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","PITCTRLA","-","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]","-","-","PITEN",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PITSTATUS","-","-","-","-","-","-","-","CTRLBUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PITINTCTRL","-","-","-","-","-","-","-","PI",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PITINTFLAGS","-","-","-","-","-","-","-","PI",null,"X","X","X","X"]
[{"$nulls":3},"0x14","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ref",null,null,"0x15","PITDBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[]
["0x01C0","CCL","Configurable Custom Logic","0x00","CTRLA","-","RUNSTDBY","-","-","-","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","SEQCTRL0","-","-","-","-","SEQSEL0[3]","SEQSEL0[2]","SEQSEL0[1]","SEQSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","SEQCTRL1","-","-","-","-","SEQSEL1[3]","SEQSEL1[2]","SEQSEL1[1]","SEQSEL1[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","SEQCTRL2","-","-","-","-","SEQSEL2[3]","SEQSEL2[2]","SEQSEL2[1]","SEQSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL0","INTMODE3[1]","INTMODE3[0]","INTMODE2[1]","INTMODE2[0]","INTMODE1[1]","INTMODE1[0]","INTMODE0[1]","INTMODE0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL1","-","-","-","-","INTMODE5[1]","INTMODE5[0]","INTMODE4[1]","INTMODE4[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","INTFLAGS","-","-","INT5","INT4","INT3","INT2","INT1","INT0",null,"X","X","X","X"]
[{"$nulls":3},"0x08","LUT0CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x09","LUT0CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","LUT0CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","TRUTH0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","LUT1CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","LUT1CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL0[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","LUT1CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TRUTH1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x10","LUT2CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x11","LUT2CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","LUT2CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","TRUTH2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","LUT3CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x15","LUT3CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","LUT3CTRLC",{"$nulls":4},"INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x17","TRUTH3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x18","LUT4CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x19","LUT4CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1A","LUT4CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1B","TRUTH4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1C","LUT5CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x1D","LUT5CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1E","LUT5CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
["ref",null,null,"0x1F","TRUTH5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0200","EVSYS","Event System","0x00","SWEVENTA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","SWEVENTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","CHANNEL0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","CHANNEL1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","CHANNEL2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","CHANNEL3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","CHANNEL4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","CHANNEL5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","CHANNEL6","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x17","CHANNEL7","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x18","CHANNEL8","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x19","CHANNEL9","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","USERCCLLUT0A","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"..."," …",{"$nulls":9},"X","X","X","X"]
["ref",null,null,"0x4A","USERTCD0INPUTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0400","PORTA","Port A Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0420","PORTB","Port B Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[]
["0x0440","PORTC","Port C Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0460","PORTD","Port D Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0480","PORTE","Port E Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[]
["0x04A0","PORTF","Port F Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x04C0","PORTG","Port G Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"-","-","-","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"-","-","-","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","-","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
["ref",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[]
["0x05E0","PORTMUX","Port Multiplexer","0x00","EVSYSROUTEA","-","EVOUTG","EVOUTF","EVOUTE","EVOUTD","EVOUTC","EVOUTB","EVOUTA",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CCLROUTEA","-","-","LUT5","LUT4","LUT3","LUT2","LUT1","LUT0",null,"X","X","X","X"]
[{"$nulls":3},"0x02","USARTROUTEA","USART3[1]","USART3[0]","USART2[1]","USART2[0]","USART1[1]","USART1[0]","USART0[1]","USART0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","USARTROUTEB","-","-","-","-","USART5[1]","USART5[0]","USART4[1]","USART4[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","SPIROUTEA","-","-","-","-","SPI1[1:0]","SPI1[1:0]","SPI0[1:0]","SPI0[1:0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","TWIROUTEA","-","-","-","-","TWI1[1:0]","TWI1[1:0]","TWI0[1:0]","TWI0[1:0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","TCAROUTEA","-","-","TCA1[2]","TCA1[1]","TCA1[0]","TCA0[2]","TCA0[1]","TCA0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","TCBROUTEA","-","-","-","TCB4","TCB3","TCB2","TCB1","TCB0",null,"X","X","X","X"]
[{"$nulls":3},"0x08","TCDROUTEA","-","-","-","-","-","TCD0[2]","TCD0[1]","TCD0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","ACROUTEA","-","-","-","-","-","AC2","AC1","AC0",null,"X","X","X","X"]
["ref",null,null,"0x0A","ZCDROUTEA","-","-","-","-","-","ZCD2","ZCD1","ZCD0",null,"X","X","X","X"]
[]
["0x0600","ADC0","Analog to-Digital Converter 0","0x00","CTRLA","RUNSTDBY","-","CONVMODE","LEFTADJ","RESSEL[1:0]","RESSEL[1:0]","FREERUN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","SAMPNUM[2]","SAMPNUM[1]","SAMPNUM[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","PRESC[3]","PRESC[2]","PRESC[1]","PRESC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","INITDLY[2]","INITDLY[1]","INITDLY[0]","-","SAMPDLY[3]","SAMPDLY[2]","SAMPDLY[1]","SAMPDLY[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLE","-","-","-","-","-","WINCM[2]","WINCM[1]","WINCM[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","SAMPCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","MUXPOS"," ","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","MUXNEG"," ","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","COMMAND","-","-","-","-","-","-","SPCONV","STCONV",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","EVCTRL","-","-","-","-","-","-",null,"STARTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x10","RES","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","WINLT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","WINHT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0680","AC0","Analog Comparator 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WINSEL[1]","WINSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X","X","X"]
["ref",null,null,"0x07","STATUS","WINSTATE[1]","WINSTATE[0]","-","CMPSTATE","-","-","-","CMPIF",null,"X","X","X","X"]
[]
["0x0688","AC1","Analog Comparator 1","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WINSEL[1]","WINSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X","X","X"]
["ref",null,null,"0x07","STATUS","WINSTATE[1]","WINSTATE[0]","-","CMPSTATE","-","-","-","CMPIF",null,"X","X","X","X"]
[]
["0x0690","AC2","Analog Comparator 2","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WINSEL[1]","WINSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X","X","X"]
["ref",null,null,"0x07","STATUS","WINSTATE[1]","WINSTATE[0]","-","CMPSTATE","-","-","-","CMPIF",null,"X","X","X","X"]
[]
["0x06A0","DAC0","Digital-to-Analog converter","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","-","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DATA","[1]","[0]","-","-","-","-","-","-",null,"X","X","X","X"]
["ref",{"$nulls":3}," ","[9]","[8]","[7]","[6]","[5]","[4]","[3]","[2]",null,"X","X","X","X"]
[]
["0x06C0","ZCD0","Zero-Cross Detector 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",null,"X","X","X","X"]
["ref",null,null,"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",null,"X","X","X","X"]
[]
["0x06C8","ZCD1","Zero-Cross Detector 1","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",null,"-","-","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",null,"-","-","X","X"]
["ref",null,null,"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",null,"-","-","X","X"]
[]
["0x06D0","ZCD2","Zero-Cross Detector 2","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",null,"-","-","-","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"-","-","-","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",null,"-","-","-","X"]
["ref",null,null,"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",null,"-","-","-","X"]
[]
["0x07C0","PTC","Peripheral Touch Controller",{"$nulls":11},"X","X","X","X"]
["ref"]
[]
["0x0800","USART0","Universal Sync. and Async RX TX 0","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0820","USART1","Universal Sync. and Async RX TX 1","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0840","USART2","Universal Sync. and Async RX TX 2","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0860","USART3","Universal Sync. and Async RX TX 3","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"-","-","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"-","-","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"-","-","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["ref",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[]
["0x0880","USART4","Universal Sync. and Async RX TX 4","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"-","-","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"-","-","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"-","-","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["ref",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[]
["0x08A0","USART5","Universal Sync. and Async RX TX 5","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"-","-","-","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"-","-","-","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"-","-","-","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"-","-","-","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"-","-","-","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"-","-","-","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","-","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"-","-","-","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","-","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"-","-","-","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
["ref",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[]
["0x0900","TWI0","Two-Wire Interface 0","0x00","CTRLA","-","INPUTLVL","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","INPUTLVL","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1:0]","BUSSTATE[1:0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,"X","X","X","X"]
[{"$nulls":14}," "," "," "," "]
["0x0920","TWI1","Two-Wire Interface 1","0x00","CTRLA","-","INPUTLVL","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,"-","X","X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","INPUTLVL","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,"-","X","X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","X","X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,"-","X","X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1]","BUSSTATE[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,"-","X","X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,"-","X","X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","X","X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","X","X","X"]
["ref",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,"-","X","X","X"]
[]
["0x0940","SPI0","Serial Peripheral Interface 0","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X","X","X"]
["ref",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0960","SPI1","Serial Peripheral Interface 1","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X","X","X"]
["ref",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0A00","TCA0 – [ Normal Mode ]","Timer/Counter Type A - instance 0 – [ Normal Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x09","EVCTRL","EVACTB[2]","EVACTB[1]","EVACTB[0]","CNTBEI","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0A00","TCA0 – [ Split Mode ]","Timer/Counter Type A - instance 0 – [ Split Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0A40","TCA1 – [ Normal Mode ]","Timer/Counter Type A - instance 1 – [ Normal Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"-","-","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",null,"-","-","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"-","-","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"-","-","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"-","-","X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"-","-","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x09","EVCTRL","EVACTB[2]","EVACTB[1]","EVACTB[0]","CNTBEI","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["ref",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[]
["0x0A40","TCA1 - [ Split Mode ]","Timer/Counter Type A – instance 1 – [ Split Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"-","-","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",null,"-","-","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",null,"-","-","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"-","-","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":14},"-","-","X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["ref",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[]
["0x0B00","TCB0","Timer/Counter Type B - instance 0","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0B10","TCB1","Timer/Counter Type B - instance 1","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0B20","TCB2","Timer/Counter Type B - instance 2","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0B30","TCB3","Timer/Counter Type B - instance 3","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"-","-","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"-","-","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"-","-","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"-","-","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"-","-","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["ref",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[]
["0x0B40","TCB4","Timer/Counter Type B - instance 4","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"-","-","-","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"-","-","-","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"-","-","-","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"-","-","-","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"-","-","-","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"-","-","-","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"-","-","-","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","-","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","-","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
["ref",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","-","X"]
[{"$nulls":17}," "]
["0x0B80","TCD0","Timer/Counter Type D - instance 0","0x00","CTRLA","-","CLKSEL[1]","CLKSEL[0]","CNTPRES[1]","CNTPRES[0]","SYNCPRES[1]","SYNCPRES[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WGMODE[1]","WGMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","CMPDSEL","CMPCSEL","-","-","FIFTY","-","AUPDATE","CMPOVR",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","CMPBVAL[3]","CMPBVAL[2]","CMPBVAL[1]","CMPBVAL[0]","CMPAVAL[3]","CMPAVAL[2]","CMPAVAL[1]","CMPAVAL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLE","DISEOC",null,null,"SCAPTUREB","SCAPTUREA","RESTART","SYNC","SYNCEOC",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","EVCTRLA","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X","X","X"]
[{"$nulls":3},"0x09","EVCTRLB","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","STATUS","PWMACTB","PWMACTA","-","-","-","-","CMDRDY","ENRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","INPUTCTRLA","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","INPUTCTRLB","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[3]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","FAULTCTRL","CMPDEN","CMPCEN","CMPBEN","CMPAEN","CMPD","CMPC","CMPB","CMPA",null,"X","X","X","X"]
[{"$nulls":3},"0x13","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x14","DLYCTRL","-","-","DLYPRESC[1]","DLYPRESC[0]","DLYTRIG[1]","DLYTRIG[0]","DLYSEL[1]","DLYSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","DLYVAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x16","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x18","DITCTRL","-","-","-","-","-","-","DITHERSEL[1]","DITHERSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x19","DITVAL","-","-","-","-","DITHER[3]","DITHER[2]","DITHER[1]","DITHER[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1E","DBGCTRL","-","-","-","-","-","FAULTDET","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x21","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","CAPTUREA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x24","CAPTUREB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x27","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x28","CMPASET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","CMPACLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","CMPBSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["ref",null,null,"0x2E","CMPBCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0F00","SYSCFG","System Configuration","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ref",null,null,"0x01","REVID","MAJOR[3]","MAJOR[2]","MAJOR[1]","MAJOR[0]","MINOR[3]","MINOR[2]","MINOR[1]","MINOR[0]",null,"X","X","X","X"]
[]
["0x1000","NVMCTRL","Nonvolatile Memory Controller","0x00","CTRLA","-","CMD[6]","CMD[5]","CMD[4]","CMD[3]","CMD[2]","CMD[1]","CMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","FLMAPLOCK","-","FLMAP[1]","FLMAP[0]","-","APPDATAWP","BOOTRP","APPCODEWP",null,"X","X","X","X"]
[{"$nulls":3},"0x02","STATUS","-","ERROR[2]","ERROR[1]","ERROR[0]","-","-","EEBUSY","FBUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTCTRL","-","-","-","-","-","-","-","EEREADY",null,"X","X","X","X"]
[{"$nulls":3},"0x04","INTFLAGS","-","-","-","-","-","-","-","EEREADY",null,"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x06","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","ADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["ref",{"$nulls":3}," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
[]
["0x1040","LOCK","Lock Bits","0x00","KEY","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3}," "," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3}," "," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
["ref",null,null," "," ","[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X","X","X"]
[]
["0x1050","FUSE","Configuration and User Fuses","0x00","WDTCFG","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","BODCFG","LVL[2]","LVL[1]","LVL[0]","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","OSCCFG","-","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","SYSCFG0","CRCSRC[1]","CRCSRC[0]","CRCSEL","-","RSTPINCFG[1]","RSTPINCFG[0]","-","EESAVE",null,"X","X","X","X"]
[{"$nulls":3},"0x06","SYSCFG1","-","-","-","-","-","SUT[2]","SUT[1]","SUT[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CODESIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x08","BOOTSIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x1080","USERROW","User Row","0x00",null,"[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":5},"[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
["ref",{"$nulls":4},"[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X","X","X"]
[]
["0x1100","SIGROW","Signature Row  – [ READ ONLY  ]","0x00","DEVICEID0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DEVICEID1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DEVICEID2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TEMPSENSE0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","TEMPSENSE1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","SERNUM0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"...","…","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ref",null,null,"0x1F","SERNUM15","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["WITHOUT ANY WARRANTY"]
[]
[]
["AVR128DA is used as a reference, differences in other types are mentioned there"]
[]
["Features"]
[]
["• AVR® CPU"]
["  – Running at up to 24 MHz"]
["  – Single-cycle I/O access"]
["  – Two-level interrupt controller"]
["  – Two-cycle hardware multiplier"]
["  – Supply voltage range: 1.8V to 5.5V"]
[]
["• Memories"]
["  – 128 KB In-System self-programmable Flash memory"]
["  – 512B EEPROM"]
["  – 16 KB SRAM"]
["  – 32B of user row in nonvolatile memory that can keep data during chip-erase and be programmed "]
["     while the device is locked"]
["  – Write/erase endurance"]
["    • Flash 10,000 cycles"]
["    • EEPROM 100,000 cycles"]
["  – Data retention: 40 years at 55°C"]
[]
["• System"]
["  – Power-on Reset (POR) circuit"]
["  – Brown-out Detector (BOD)"]
["  – Clock options"]
["    • High-Precision internal high-frequency Oscillator with selectable frequency up to 24 MHz (OSCHF)"]
["      – Auto-tuning for improved internal oscillator accuracy"]
["    • Internal PLL up to 48 MHz for high-frequency operation of Timer/Counter type D (PLL)"]
["    • 32.768 kHz Ultra-Low Power internal oscillator (OSC32K)"]
["    • 32.768 kHz external crystal oscillator (XOSC32K)"]
["    • External clock input"]
["  – Single-pin Unified Program and Debug Interface (UPDI)"]
["  – Three sleep modes"]
["    • Idle with all peripherals running for immediate wake-up"]
["    • Standby with a configurable operation of selected peripherals"]
["    • Power-Down with full data retention"]
[]
["  • Peripherals"]
["    – Up to two 16-bit Timer/Counter type A (TCA) with a dedicated period register and three PWM channels"]
["    – Up to five 16-bit Timer/Counter type B (TCB) with input capture and simple PWM functionality"]
["    – One 12-bit Timer/Counter type D (TCD) optimized for power control"]
["    – One 16-bit Real-Time Counter (RTC) running from an external crystal or internal oscillator"]
["    – Up to six USART with fractional baud rate generator, auto-baud, and start-of-frame detection"]
["    – Two host/client Serial Peripheral Interface (SPI)"]
["    – Up to two Two-Wire Interface (TWI) with dual address match"]
["      • Independent host and client operation (Dual mode)"]
["      • Philips I2C compatible"]
["      • Standard mode (Sm, 100 kHz)"]
["      • Fast mode (Fm, 400 kHz)"]
["      • Fast mode plus (Fm+, 1 MHz) (1)"]
["  – Event System for CPU independent and predictable inter-peripheral signaling"]
["  – Configurable Custom Logic (CCL) with up to six programmable Look-up Tables (LUT)"]
["  – One 12-bit differential 130 ksps Analog-to-Digital Converter (ADC)"]
["  – Three Analog Comparators (ACs) with window compare functions"]
["  – One 10-bit Digital-to-Analog Converter (DAC)"]
["  – Up to three Zero-Cross Detectors (ZCD)"]
["  – Multiple voltage references (VREF)"]
["    • 1.024V"]
["    • 2.048V"]
["    • 2.500V"]
["    • 4.096V"]
["  – Peripheral Touch Controller (PTC) with Driven Shield+ and Boost Mode technologies "]
["     for capacitive touch buttons, sliders, wheels and 2D surface"]
["    • Up to 46 self-capacitance and 529 mutual capacitance channels"]
["  – Automated Cyclic Redundancy Check (CRC) Flash memory scan"]
["  – Watchdog Timer (WDT) with Window mode, with a separate on-chip oscillator"]
["  – External interrupt on all general purpose pins"]
[]
["• I/O and Packages:"]
["  – Up to 55 programmable I/O pins"]
["  – 28-pin SPDIP, SSOP and SOIC"]
["  – 32-pin VQFN 5x5 mm and TQFP 7x7 mm"]
["  – 48-pin VQFN 6x6 mm and TQFP 7x7 mm"]
["  – 64-pin VQFN 9x9 mm and TQFP 10x10 mm"]
[]
["• Temperature Ranges:"]
["  – Industrial: -40°C to +85°C"]
["  – Extended: -40°C to +125°C"]
[]
["  Note: "]
["  1. I2C Fm+ is only supported for VDD above 2.7V."]

{"sheet":"AVR128-DB","index":1,"n_rows":1117,"n_cols":31,"rows_kept":1117,"flags":["formulas_cached_only"]}
["AVR128-DB-28/32/48/64","[ 04 -2023 ]"]
["Peripherals and Architecture"]
[]
[]
["Table 8-1. Peripheral Address Map",{"$nulls":21},"Table","  8-3. Interrupt Vector Mapping"]
[{"$nulls":22},"**********************************************************************************************************************************************************************"]
["Base Address ","Name"," Description","Offset","Name","Bit 7","Bit 6"," Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0",null,"Pin 28","Pin 32","Pin 48","Pin 64",{"$nulls":4},"Vector","Program",{"$nulls":3},"28-Pin","32-Pin","48-Pin","64-Pin"]
[{"$nulls":22},"Number","Address","Peripheral","Description"]
["0x0000","VPORTA","Virtual Port A","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},0,"0x00","RESET","Reset",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},1,"0x02","NMI","Non-Maskable Interrupt available for CRCSCAN, CFD",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},2,"0x04","BOD_VLM","Voltage Level Monitor Interrupt",null,"X","X","X","X"]
[{"$nulls":22},3,"0x06","CLKCTRL_CFD","External_crystal_oscillator/clock_source_failure_Interrupt",null,"X","X","X","X"]
["0x0004","VPORTB","Virtual Port B","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},4,"0x08","MVIO_MVIO","Multi-Voltage_Input/Output_Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},5,"0x0A","RTC_CNT","Real-Time Counter Overflow or Compare Match Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},6,"0x0C","RTC_PIT","Real-Time Counter Periodic Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},7,"0x0E","CCL_CCL","Configurable Custom Logic Interrupt",null,"X","X","X","X"]
[{"$nulls":22},8,"0x10","PORTA_PORT","PORTA External interrupt",null,"X","X","X","X"]
["0x0008","VPORTC","Virtual Port C","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},9,"0x12","TCA0_OVF","OVF Normal: Timer/Counter Type A Overflow Interrupt ",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},9,"0x12","TCA0_LUNF","Split:     Timer/Counter Type A Low Underflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},10,"0x14","TCA0_HUNF","Normal: Unused",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},10,"0x14","TCA0_HUNF","Split:     Timer/Counter Type A High Underflow Interrupt",null,"X","X","X","X"]
[{"$nulls":22},11,"0x16","TCA0_CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"X","X","X","X"]
["0x000C","VPORTD","Virtual Port D","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},11,"0x16","TCA0_LCMP0","Split:     Timer/Counter Type A Low Compare 0 Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},12,"0x18","TCA0_CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},12,"0x18","TCA0_LCMP1","Split:     Timer/Counter Type A Low Compare 1 Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},13,"0x1A","TCA0_CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"X","X","X","X"]
[{"$nulls":22},13,"0x1A","TCA0_LCMP2","Split: Timer/Counter Type A Low Compare 2 Interrupt",null,"X","X","X","X"]
["0x0010","VPORTE","Virtual Port E","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},14,"0x1C","TCB0_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},15,"0x1E","TCB1_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},16,"0x20","TCD0_OVF","Timer Counter Type D Overflow Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":4},17,"0x22","TCD0_TRIG","Timer Counter Type D Trigger Interrupt",null,"X","X","X","X"]
[{"$nulls":22},18,"0x24","TWI0_TWIS","Two-Wire Interface Client Interrupt",null,"X","X","X","X"]
["0x0014","VPORTF","Virtual Port F","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},19,"0x26","TWI0_TWIM","Two-Wire Interface Host Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},20,"0x28","SPI0_INT","Serial Peripheral Interface Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},21,"0x2A","USART0_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},22,"0x2C","USART0_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":22},23,"0x2E","USART0_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
["0x0018","VPORTG","Virtual Port G","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":4},24,"0x30","PORTD_PORT","PORTD External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":4},25,"0x32","AC0_AC","Analog Comparator Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":4},26,"0x34","ADC0_RESRDY","Analog-to-Digital Converter Result Ready Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":4},27,"0x36","ADC0_WCMP","Analog-to-Digital Converter Window Compare Interrupt",null,"X","X","X","X"]
[{"$nulls":16}," ",{"$nulls":5},28,"0x38","ZCD0_ZCD","Zero-Cross Interrupt",null,"X","X","X","X"]
["0x001C","GPR","General Purpose Registers","0x00","GPR0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},29,"0x3A","AC1_AC","Analog Comparator Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","GPR1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},30,"0x3C","PORTC_PORT","PORTC External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","GPR2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},31,"0x3E","TCB2_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","GPR3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},32,"0x40","USART1_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":22},33,"0x42","USART1_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
["…",null,"Reserved",{"$nulls":19},34,"0x44","USART1_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":22},35,"0x46","PORTF_PORT","PORTF External Interrupt",null,"X","X","X","X"]
["0x0030","CPU","CPU","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},36,"0x48","NVMCTRL_EE","Nonvolatile Memory Controller EEPROM Ready Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},37,"0x4A","SPI1_INT","Serial Peripheral Interface Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},38,"0x4C","USART2_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":4},39,"0x4E","USART2_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CCP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},40,"0x50","USART2_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":4},41,"0x52","AC2_AC","Analog Comparator Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},42,"0x54","TWI1_TWIS","Two-Wire Interface Client Interrupt",null,"-","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},43,"0x56","TWI1_TWIM","Two-Wire Interface Host Interrupt",null,"-","X","X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},44,"0x58","TCB3_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"-","-","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":4},45,"0x5A","PORTB_PORT","PORTB External Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","RAMPZ","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},46,"0x5C","PORTE_PORT","PORTE External Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},47,"0x5E","TCA1_OVF","Normal: Timer/Counter Type A Overflow Interrupt ",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","SP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},47,"0x5E","TCA1_LUNF","Split:     Timer/Counter Type A Low Underflow Interrupt",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X",{"$nulls":4},48,"0x60","TCA1_HUNF","Normal: Unused",null,"-","-","X","X"]
["ok",null,null,"0x0F","SREG","I","T","H","S","V","N","Z","C",null,"X","X","X","X",{"$nulls":4},48,"0x60","TCA1_HUNF","Split:     Timer/Counter Type A High Underflow Interrupt",null,"-","-","X","X"]
[{"$nulls":22},49,"0x62","TCA1_CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"-","-","X","X"]
["0x0040","RSTCTRL","Reset Controller","0x00","RSTFR","-","-","UPDIRF","SWRF","WDRF","EXTRF","BORF","PORF",null,"X","X","X","X",{"$nulls":4},49,"0x62","TCA1_LCMP0","Split:     Timer/Counter Type A Low Compare 0 Interrupt",null,"-","-","X","X"]
["ok",null,null,"0x01","SWRR","-","-","-","-","-","-","-","SWRST",null,"X","X","X","X",{"$nulls":4},50,"0x64","TCA1_CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"-","-","X","X"]
[" ",{"$nulls":21},50,"0x64","TCA1_LCMP1","Split:     Timer/Counter Type A Low Compare 1 Interrupt",null,"-","-","X","X"]
["0x0050","SLPCTRL","Sleep Controller","0x00","CTRLA","-","-","-","-","SMODE[2]","SMODE[1]","SMODE[0]","SEN",null,"X","X","X","X",{"$nulls":4},51,"0x66","TCA1_CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"-","-","X","X"]
["ok",null,null,"0x01","VREGCTRL","-","-","HTLLEN","-","-","PMODE[2]","PMODE[1]","PMODE[0]",null,"X","X","X","X",{"$nulls":4},51,"0x66","TCA1_LCMP2","Split:     Timer/Counter Type A Low Compare 2 Interrupt",null,"-","-","X","X"]
[" ",{"$nulls":13},"X","X","X","X",{"$nulls":4},52,"0x68","ZCD1_ZCD","Zero-Cross Interrupt",null,"-","-","X","X"]
["0x0060","CLKCTRL","Clock Controller","0x00","MCLKCTRLA","CLKOUT","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X",{"$nulls":4},53,"0x6A","USART3_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x01","MCLKCTRLB","-","-","-","PDIV[3]","PDIV[2]","PDIV[1]","PDIV[0]","PEN",null,"X","X","X","X",{"$nulls":4},54,"0x6C","USART3_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","X","X"]
["add",null,null,"0x02","MCLKCTRLC"," ","-","-","-","CFDSRC[1]","CFDSRC[0]","CFDTST","CFDEN",null,"X","X","X","X",{"$nulls":4},55,"0x6E","USART3_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x03","MCLKINTCTRL","INTTYPE","-","-","-","-","-","-","CFD",null,"X","X","X","X",{"$nulls":4},56,"0x70","USART4_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","X","X"]
["add",null,null,"0x04","MCLKINTFLAGS","-","-","-","-","-","-","-","CFD",null,"X","X","X","X",{"$nulls":4},57,"0x72","USART4_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","X","X"]
["add",null,null,"0x05","MCLKSTATUS","-","-","PLLS","EXTS","XOSC32KS","OSC32KS","OSCHFS","SOSC",{"$nulls":9},58,"0x74","USART4_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":22},59,"0x76","PORTG_PORT","PORTG External Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},60,"0x78","ZCD2","ZCD Zero-Cross Interrupt ",null,"-","-","-","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":4},61,"0x7A","TCB4_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"-","-","-","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":4},62,"0x7C","USART5_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"0x08","OSCHFCTRLA","RUNSTDBY","-","FRQSEL[3]","FRQSEL[2]","FRQSEL[1]","FRQSEL[0]","-","AUTOTUNE",null,"X","X","X","T",{"$nulls":4},63,"0x7E","USART5_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"0x09","OSCHFTUNE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":4},64,"0x80","USART5_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","-","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":5},"modified"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","PLLCTRLA","RUNSTDBY","SOURCE","-","-","-","-","MULFAC[1]","MULFAC[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x11","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x18","OSC32KCTRLA","RUNSTDBY","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x19","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1B","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1C","XOSC32KCTRLA","RUNSTDBY","-","CSUT[1]","CSUT[0]","-","SEL","LPMODE","ENABLE",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[]
["add",null,null,"0x20","XOSCHFCTRLA","RUNSTDBY","-","CSUTHF[1]","CSUTHF[0]","FRQRANGE[1]","FRQRANGE[0]","SELHF","ENABLE",null,"X","X","X","X"]
[" "]
["0x00A0","BOD","Brown-Out Reset Detector","0x00","CTRLA","-","-","-","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","LVL[2]","LVL[1]","LVL[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","VLMCTRLA","-","-","-","-","-","-","VLMLVL[1]","VLMLVL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTCTRL","-","-","-","-","-","VLMCFG[1]","VLMCFG[0]","VLMIE",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTFLAGS","-","-","-","-","-","-","-","VLMIF",null,"X","X","X","X"]
["mod addr, name",null,null,"0x0B","STATUS","-","-","-","-","-","-","-","VLMS",null,"X","X","X","X"]
[]
["0x00B0","VREF","Voltage Reference","0x00","ADC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DAC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["mod addr",null,null,"0x04","ACREF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X","X","X"]
[]
["0x00C0","MVIO","Multi-Voltage I/O","0x00","INTCTRL",{"$nulls":7},"VDDIO2IE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","INTFLAGS",{"$nulls":7},"VDDIO2IF",null,"X","X","X","X"]
["new",null,null,"0x02","STATUS",{"$nulls":7},"VDDIO2",null,"X","X","X","X"]
[]
["…","Reserved"]
[]
["0x0100","WDT","Watchdog Timer","0x00","CTRLA","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X","X","X"]
["ok",null,null,"0x01","STATUS","LOCK","-","-","-","-","-","-","SYNCBUSY",null,"X","X","X","X"]
[]
["0x0110","CPUINT","Interrupt Controller","0x00","CTRLA","-","IVSEL","CVT","-","-","-","-","LVL0RR",null,"X","X","X","X"]
[{"$nulls":3},"0x01","STATUS","NMIEX","-","-","-","-","-","LVL1EX","LVL0EX",null,"X","X","X","X"]
[{"$nulls":3},"0x02","LVL0PRI","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x03","LVL1VEC","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0120","CRCSCAN","Cyclic Redundancy Check Memory Scan","0x00","CTRLA","RESET","-","-","-","-","-","NMIEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","SRC[1:0]","SRC[1:0]",null,"X","X","X","X"]
["ok",null,null,"0x02","STATUS","-","-","-","-","-","-","OK","BUSY",null,"X","X","X","X"]
[]
["…","Reserved"]
[]
["0x0140","RTC","Real-Time Counter","0x00","CTRLA","RUNSTDBY","PRESCALER[3]","PRESCALER[2]","PRESCALER[1]","PRESCALER[0]","CORREN","-","RTCEN",null,"X","X","X","X"]
[{"$nulls":3},"0x01","STATUS","-","-","-","-","CMPBUSY","PERBUSY","CNTBUSY","CTRLABUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","CMP","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","-","-","-","-","-","-","CMP","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CALIB","SIGN","ERROR[6]","ERROR[5]","ERROR[4]","ERROR[3]","ERROR[2]","ERROR[1]","ERROR[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CLKSEL","-","-","-","-","-","-","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PER]","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","PITCTRLA","-","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]","-","-","PITEN",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PITSTATUS","-","-","-","-","-","-","-","CTRLBUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PITINTCTRL","-","-","-","-","-","-","-","PI",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PITINTFLAGS","-","-","-","-","-","-","-","PI",null,"X","X","X","X"]
[{"$nulls":3},"0x14","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ok",null,null,"0x15","PITDBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[]
["…","Reserved"]
[]
["0x01C0","CCL","Configurable Custom Logic","0x00","CTRLA","-","RUNSTDBY","-","-","-","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","SEQCTRL0","-","-","-","-","SEQSEL0[3]","SEQSEL0[2]","SEQSEL0[1]","SEQSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","SEQCTRL1","-","-","-","-","SEQSEL1[3]","SEQSEL1[2]","SEQSEL1[1]","SEQSEL1[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","SEQCTRL2","-","-","-","-","SEQSEL2[3]","SEQSEL2[2]","SEQSEL2[1]","SEQSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL0","INTMODE3[1]","INTMODE3[0]","INTMODE2[1]","INTMODE2[0]","INTMODE1[1]","INTMODE1[0]","INTMODE0[1]","INTMODE0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL1","-","-","-","-","INTMODE5[1]","INTMODE5[0]","INTMODE4[1]","INTMODE4[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","INTFLAGS","-","-","INT5","INT4","INT3","INT2","INT1","INT0",null,"X","X","X","X"]
[{"$nulls":3},"0x08","LUT0CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x09","LUT0CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","LUT0CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","TRUTH0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","LUT1CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","LUT1CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL0[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","LUT1CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TRUTH1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x10","LUT2CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x11","LUT2CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","LUT2CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","TRUTH2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","LUT3CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x15","LUT3CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","LUT3CTRLC",{"$nulls":4},"INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x17","TRUTH3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x18","LUT4CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x19","LUT4CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1A","LUT4CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1B","TRUTH4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1C","LUT5CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x1D","LUT5CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1E","LUT5CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
["ok",null,null,"0x1F","TRUTH5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0200","EVSYS","Event System","0x00","SWEVENTA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","SWEVENTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","CHANNEL0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","CHANNEL1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","CHANNEL2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","CHANNEL3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","CHANNEL4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","CHANNEL5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","CHANNEL6","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x17","CHANNEL7","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x18","CHANNEL8","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x19","CHANNEL9","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","USERCCLLUT0A","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"...","…",{"$nulls":6},"-","-",null,"X","X","X","X"]
["mod",null,null,"0x55","USEROPAMP2DRIVE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0400","PORTA","Port A Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0420","PORTB","Port B Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
[]
["0x0440","PORTC","Port C Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0460","PORTD","Port D Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0480","PORTE","Port E Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":3},"X","X"]
[]
["0x04A0","PORTF","Port F Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x04C0","PORTG","Port G Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",{"$nulls":4},"X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",{"$nulls":4},"X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
["add INLVL","mod",null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",{"$nulls":4},"X"]
[]
["0x05E0","PORTMUX","Port Multiplexer","0x00","EVSYSROUTEA","-","EVOUTG","EVOUTF","EVOUTE","EVOUTD","EVOUTC","EVOUTB","EVOUTA",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CCLROUTEA","-","-","LUT5","LUT4","LUT3","LUT2","LUT1","LUT0",null,"X","X","X","X"]
[{"$nulls":3},"0x02","USARTROUTEA","USART3[1]","USART3[0]","USART2[1]","USART2[0]","USART1[1]","USART1[0]","USART0[1]","USART0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","USARTROUTEB","-","-","-","-","USART5[1]","USART5[0]","USART4[1]","USART4[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","SPIROUTEA","-","-","-","-","SPI1[1]","SPI1[0]","SPI0[1]","SPI0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","TWIROUTEA","-","-","-","-","TWI1[1]","TWI1[0]","TWI0[1]","TWI0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","TCAROUTEA","-","-","TCA1[2]","TCA1[1]","TCA1[0]","TCA0[2]","TCA0[1]","TCA0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","TCBROUTEA","-","-","-","TCB4","TCB3","TCB2","TCB1","TCB0",null,"X","X","X","X"]
[{"$nulls":3},"0x08","TCDROUTEA","-","-","-","-","-","TCD0[2]","TCD0[1]","TCD0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","ACROUTEA","-","-","-","-","-","AC2","AC1","AC0",null,"X","X","X","X"]
["ok",null,null,"0x0A","ZCDROUTEA","-","-","-","-","-","ZCD2","ZCD1","ZCD0",null,"X","X","X","X"]
[]
["…","…"]
[]
["0x0600","ADC0","Analog to-Digital Converter 0","0x00","CTRLA","RUNSTDBY","-","CONVMODE","LEFTADJ","RESSEL[1]","RESSEL[0]","FREERUN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","SAMPNUM[2]","SAMPNUM[1]","SAMPNUM[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","PRESC[3]","PRESC[2]","PRESC[1]","PRESC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","INITDLY[2]","INITDLY[1]","INITDLY[0]","-","SAMPDLY[3]","SAMPDLY[2]","SAMPDLY[1]","SAMPDLY[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLE","-","-","-","-","-","WINCM[2]","WINCM[1]","WINCM[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","SAMPCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","MUXPOS","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","MUXNEG","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","COMMAND","-","-","-","-","-","-","SPCONV","STCONV",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","EVCTRL","-","-","-","-","-","-",null,"STARTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x10","RES","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","WINLT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","WINHT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["…","…"]
[]
["0x0680","AC0","Analog Comparator 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WINSEL[1]","WINSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X","X","X"]
["0k",null,null,"0x07","STATUS","WINSTATE[1]","WINSTATE[0]","-","CMPSTATE","-","-","-","CMPIF",null,"X","X","X","X"]
[]
["0x0688","AC1","Analog Comparator 1","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WINSEL[1]","WINSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X","X","X"]
["ok",null,null,"0x07","STATUS","WINSTATE[1]","WINSTATE[0]","-","CMPSTATE","-","-","-","CMPIF",null,"X","X","X","X"]
[]
["0x0690","AC2","Analog Comparator 2","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WINSEL[1]","WINSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X","X","X"]
["ok",null,null,"0x07","STATUS","WINSTATE[1]","WINSTATE[0]","-","CMPSTATE","-","-","-","CMPIF",null,"X","X","X","X"]
[]
["0x06A0","DAC0","Digital-to-Analog converter","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","-","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DATA","[1]","[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":4}," ","[9]","[8]","[7]","[6]","[5]","[4]","[3]","[2]",null,"X","X","X","X"]
[]
["0x06C0","ZCD0","Zero-Cross Detector 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",null,"X","X","X","X"]
[]
["0x06C8","ZCD1","Zero-Cross Detector 1","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",{"$nulls":3},"X","X"]
[]
["0x06D0","ZCD2","Zero-Cross Detector 2","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",{"$nulls":4},"X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",{"$nulls":4},"X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",{"$nulls":4},"X"]
[]
["0x07C0","PTC","Peripheral Touch Controller",{"$nulls":11},"X","X","X","X"]
[]
["…","…"]
[]
["0x0800","USART0","Universal Sync. and Async RX TX 0","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0820","USART1","Universal Sync. and Async RX TX 1","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[0]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0840","USART2","Universal Sync. and Async RX TX 2","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0860","USART3","Universal Sync. and Async RX TX 3","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[0]","CMODE[0]","-","-","-","UDORD","UCPHA","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[]
["0x0880","USART4","Universal Sync. and Async RX TX 4","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
["pok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[]
["0x08A0","USART5","Universal Sync. and Async RX TX 4","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",{"$nulls":4},"X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",{"$nulls":4},"X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",{"$nulls":4},"X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",{"$nulls":4},"X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",{"$nulls":4},"X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",{"$nulls":4},"X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",{"$nulls":4},"X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":4},"X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",{"$nulls":4},"X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[]
["0x0900","TWI0","Two-Wire Interface 0","0x00","CTRLA","-","INPUTLVL","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","INPUTLVL","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1]","BUSSTATE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,"X","X","X","X"]
[{"$nulls":14}," "," "," "," "]
["0x0920","TWI1","Two-Wire Interface 1","0x00","CTRLA","-","INPUTLVL","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,null,"X","X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","INPUTLVL","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,null,"X","X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,null,"X","X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,null,"X","X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1]","BUSSTATE[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,null,"X","X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,null,"X","X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,null,"X","X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,null,"X","X","X"]
["ok",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,null,"X","X","X"]
[]
["0x0940","SPI0","Serial Peripheral Interface 0","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X","X","X"]
["ok",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0960","SPI1","Serial Peripheral Interface 1","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X","X","X"]
["ok",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0A00","TCA0 – [ Normal Mode ]","Timer/Counter Type A - instance 0 – [ Normal Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x09","EVCTRL","EVACTB[2]","EVACTB[1]","EVACTB[0]","CNTBEI","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0A00","TCA0 – [ Split Mode ]","Timer/Counter Type A - instance 0 – [ Split Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0A40","TCA1 – [ Normal Mode ]","Timer/Counter Type A - instance 1 – [ Normal Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x09","EVCTRL","EVACTB[2]","EVACTB[1]","EVACTB[0]","CNTBEI","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
["ok",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[]
["0x0A40","TCA1 - [ Split Mode ]","Timer/Counter Type A – instance 1 – [ Split Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":16},"X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
["ok",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[]
["0x0B00","TCB0","Timer/Counter Type B - instance 0","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0B10","TCB1","Timer/Counter Type B - instance 1","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0B20","TCB2","Timer/Counter Type B - instance 2","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0B30","TCB3","Timer/Counter Type B - instance 3","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":3},"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":3},"X","X"]
[]
["0x0B40","TCB4","Timer/Counter Type B - instance 4","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",{"$nulls":4},"X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",{"$nulls":4},"X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",{"$nulls":4},"X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",{"$nulls":4},"X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",{"$nulls":4},"X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",{"$nulls":4},"X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",{"$nulls":4},"X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",{"$nulls":4},"X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":4},"X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",{"$nulls":4},"X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",{"$nulls":4},"X"]
[{"$nulls":17}," "]
["0x0B80","TCD0","Timer/Counter Type D - instance 0","0x00","CTRLA","-","CLKSEL[1]","CLKSEL[0]","CNTPRES[1]","CNTPRES[0]","SYNCPRES[1]","SYNCPRES[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WGMODE[1]","WGMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","CMPDSEL","CMPCSEL","-","-","FIFTY","-","AUPDATE","CMPOVR",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","CMPBVAL[3]","CMPBVAL[2]","CMPBVAL[1]","CMPBVAL[0]","CMPAVAL[3]","CMPAVAL[2]","CMPAVAL[1]","CMPAVAL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLE","DISEOC","-","-","SCAPTUREB","SCAPTUREA","RESTART","SYNC","SYNCEOC",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","EVCTRLA","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X","X","X"]
[{"$nulls":3},"0x09","EVCTRLB","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","STATUS","PWMACTB","PWMACTA","-","-","-","-","CMDRDY","ENRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","INPUTCTRLA","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","INPUTCTRLB","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[3]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","FAULTCTRL","CMPDEN","CMPCEN","CMPBEN","CMPAEN","CMPD","CMPC","CMPB","CMPA",null,"X","X","X","X"]
[{"$nulls":3},"0x13","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x14","DLYCTRL","-","-","DLYPRESC[1]","DLYPRESC[0]","DLYTRIG[1]","DLYTRIG[0]","DLYSEL[1]","DLYSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","DLYVAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x16","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x18","DITCTRL","-","-","-","-","-","-","DITHERSEL[1]","DITHERSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x19","DITVAL","-","-","-","-","DITHER[3]","DITHER[2]","DITHER[1]","DITHER[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1E","DBGCTRL","-","-","-","-","-","FAULTDET","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x21","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","CAPTUREA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x24","CAPTUREB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x27","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x28","CMPASET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","CMPACLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","CMPBSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["ok",null,null,"0x2E","CMPBCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0F00","SYSCFG","System Configuration","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ok",null,null,"0x01","REVID","MAJOR[3]","MAJOR[2]","MAJOR[1]","MAJOR[0]","MINOR[3]","MINOR[2]","MINOR[1]","MINOR[0]",null,"X","X","X","X"]
[]
["0x1000","NVMCTRL","Nonvolatile Memory Controller","0x00","CTRLA","-","CMD[6]","CMD[5]","CMD[4]","CMD[3]","CMD[2]","CMD[1]","CMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","FLMAPLOCK","-","FLMAP[1]","FLMAP[0]","-","APPDATAWP","BOOTRP","APPCODEWP",null,"X","X","X","X"]
[{"$nulls":3},"0x02","STATUS","-","ERROR[2]","ERROR[1]","ERROR[0]","-","-","EEBUSY","FBUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTCTRL","-","-","-","-","-","-","-","EEREADY",null,"X","X","X","X"]
[{"$nulls":3},"0x04","INTFLAGS","-","-","-","-","-","-","-","EEREADY",null,"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x06","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","ADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["ok",{"$nulls":3}," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
[]
["0x1040","LOCK","Lock Bits","0x00","KEY","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3}," "," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3}," "," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
["ok",null,null," "," ","[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X","X","X"]
[]
["0x1050","FUSE","Configuration and User Fuses","0x00","WDTCFG","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","BODCFG","LVL[2]","LVL[1]","LVL[0]","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","OSCCFG","-","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","SYSCFG0","CRCSRC[1]","CRCSRC[0]","CRCSEL","-","RSTPINCFG[1]","RSTPINCFG[0]","-","EESAVE",null,"X","X","X","X"]
[{"$nulls":3},"0x06","SYSCFG1","-","-","-","-","-","SUT[2]","SUT[1]","SUT[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CODESIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x08","BOOTSIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x1080","USERROW","User Row","0x00",null,"[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":5},"[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
[{"$nulls":5},"[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X","X","X"]
[]
["0x1100","SIGROW","Signature Row  – [ READ ONLY  ]","0x00","DEVICEID0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DEVICEID1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DEVICEID2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TEMPSENSE0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","TEMPSENSE1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","SERNUM0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"...","…","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","SERNUM15","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["WITHOUT ANY WARRANTY"]
[]
[]
["Features"]
[]
["• AVR® CPU"]
["  – Running at up to 24 MHz"]
["  – Single-cycle I/O register access",{"$nulls":13},-28,-32,-48,"64-Pin"]
["  – Two-level interrupt controller"]
["  – Two-cycle hardware multiplier"]
["  – Supply voltage range: 1.8V to 5.5V"]
[]
["• Memories"]
["  – 128 KB In-System self-programmable Flash memory"]
["  – 512B EEPROM"]
["  – 16 KB SRAM"]
["  – 32B of user row in nonvolatile memory that can keep data during chip-erase and be programmed "]
["     while the device is locked"]
["  – Write/erase endurance"]
["    • Flash: 1000 cycles"]
["    • EEPROM: 100,000 cycles"]
["  – Data retention: 40 Years at 55°C"]
[]
["• System"]
["  – Power-on Reset (POR) circuit"]
["  – Brown-out Detector (BOD) with user-programmable levels"]
["  – Voltage Level Monitor (VLM) with interrupt at a programmable level above the BOD level"]
["  – Clock failure detection"]
["  – Clock options"]
["     • High-precision internal oscillator with selectable frequency up to 24 MHz (OSCHF)"]
["      – Auto-tuning for improved internal oscillator accuracy"]
["     • Internal PLL up to 48 MHz for high-frequency operation of Timer/Counter type D (PLL)"]
["     • Internal ultra-low power 32.768 kHz oscillator (OSC32K)"]
["     • External 32.768 kHz crystal oscillator (XOSC32K)"]
["     • External clock input"]
["     • External high-frequency crystal oscillator (XOSCHF) with clock failure detection"]
["  – Single pin Unified Program and Debug Interface (UPDI)"]
["  – Three sleep modes"]
["      • Idle with all peripherals running for immediate wake-up"]
["      • Standby with a configurable operation of selected peripherals"]
["      • Power-Down with full data retention"]
[]
["• Peripherals"]
["  – Up to two 16-bit Timer/Counters type A (TCA) with three compare channels for PWM and waveform generation"]
["  – Up to five 16-bit Timer/Counters type B (TCB) with input capture for capture and signal measurements"]
["  – One 12-bit PWM Timer/Counter type D (TCD) optimized for power control"]
["  – One 16-bit Real-Time Counter (RTC) that can run from external crystal or internal oscillator"]
["  – Up to six USARTs"]
["     • Operation modes: RS-485, LIN client, host SPI, and IrDA"]
["     • Fractional baud rate generator, auto-baud, and start-of-frame detection"]
["  – Two SPIs with host/client operation modes"]
["  – Up to two Two-Wire Interface (TWI) with dual address match"]
["     • Independent host and client operation Dual mode)"]
["     • Phillips I2C compatible"]
["     • Standard mode (Sm, 100 kHz)"]
["     • Fast mode (Fm, 400 kHz)"]
["     • Fast mode plus (Fm+, 1 MHz)(1)"]
["  – Event System for CPU-independent and predictable inter-peripherals signaling"]
["  – Configurable Custom Logic (CCL) with up to six programmable Look-up Tables (LUTs)"]
["  – One 12-bit 130 ksps differential Analog-to-Digital Converter (ADC)"]
["  – Three Analog Comparators (ACs) with window compare functions"]
["  – One 10-bit Digital-to-Analog Converter (DAC)"]
["  – Up to three Zero-Cross Detectors (ZCDs)"]
["  – Analog Signal Conditioning (OPAMP) peripheral with up to three op amps, each with an internal resistor ladder "]
["     that allows for many useful configurations with no external components"]
["  – Multiple voltage references (VREF)"]
["     • 1.024V"]
["     • 2.048V"]
["     • 2.500V"]
["     • 4.096V"]
["     • External Voltage Reference (VREFA)"]
["     • Supply Voltage (VDD)"]
["  – Automated Cyclic Redundancy Check (CRC) Flash program memory scan"]
["  – Watchdog Timer (WDT) with Window mode, and separate on-chip oscillator"]
["  – External interrupt on all general purpose pins"]
[]
["• I/O and Packages"]
["  – Multi-Voltage I/O (MVIO) on I/O port C"]
["  – Selectable input voltage threshold"]
["  – Up to 55/54 programmable I/O pins"]
["  – 28-pin SSOP, SOIC and SPDIP"]
["  – 32-pin VQFN 5x5 mm and TQFP 7x7 mm"]
["  – 48-pin VQFN 5x5 mm and TQFP 7x7 mm"]
["  – 64-pin VQFN 9x9 mm and TQFP 10x10 mm"]
[]
["• Temperature Ranges"]
["  – Industrial: -40°C to 85°C"]
["  – Extended: -40°C to 125°C"]
[]
["  Note: "]
["  1. I2C Fm+ is only supported for supply voltage VDD above 2.7 VDC."]

{"sheet":"AVR64-DD-32-28","index":2,"n_rows":750,"n_cols":25,"rows_kept":750,"flags":["formulas_cached_only"]}
["AVR64-DD-28-32","[ 04 -2023 ]"]
["Peripherals and Architecture"]
[]
[]
["Table 9-1. Peripheral Address Map",{"$nulls":17},"Table","  8-3. Interrupt Vector Mapping"]
[{"$nulls":18},"*************************************************************************************************************************************************************************"]
["Base Address","Name","Description","Offset","Name","Bit 7","Bit 6"," Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0",null,"28-Pin","32-Pin",null,null,"Vector","Program",{"$nulls":3},"28-Pin","32-Pin"]
[{"$nulls":18},"Number","Address","Peripheral","Description"]
["0x0000","VPORTA","Virtual Port A","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,0,"0x00","RESET","Reset",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,1,"0x02","NMI","Non-Maskable Interrupt available for CRCSCAN, CFD",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,2,"0x04","BOD_VLM","Voltage Level Monitor Interrupt",null,"X","X"]
[{"$nulls":18},3,"0x06","CLKCTRL_CFD","External_crystal_oscillator/clock_source_failure_Interrupt",null,"X","X"]
["0x0008","VPORTC","Virtual Port C","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,4,"0x08","MVIO_MVIO","Multi-Voltage_Input/Output_Interrupt",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,5,"0x0A","RTC_CNT","Real-Time Counter Overflow or Compare Match Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,6,"0x0C","RTC_PIT","Real-Time Counter Periodic Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,7,"0x0E","CCL_CCL","Configurable Custom Logic Interrupt",null,"X","X"]
[{"$nulls":18},8,"0x10","PORTA_PORT","PORTA External interrupt",null,"X","X"]
["0x000C","VPORTD","Virtual Port D","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,9,"0x12","TCA0_OVF","OVF Normal: Timer/Counter Type A Overflow Interrupt ",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,9,"0x12","TCA0_LUNF","Split:     Timer/Counter Type A Low Underflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,10,"0x14","TCA0_HUNF","Normal: Unused",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,10,"0x14","TCA0_HUNF","Split:     Timer/Counter Type A High Underflow Interrupt",null,"X","X"]
[{"$nulls":18},11,"0x16","TCA0_CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"X","X"]
["0x0014 ","VPORTF","Virtual Port F","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,11,"0x16","TCA0_LCMP0","Split:     Timer/Counter Type A Low Compare 0 Interrupt",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,12,"0x18","TCA0_CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,12,"0x18","TCA0_LCMP1","Split:     Timer/Counter Type A Low Compare 1 Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,13,"0x1A","TCA0_CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"X","X"]
[{"$nulls":18},13,"0x1A","TCA0_LCMP2","Split: Timer/Counter Type A Low Compare 2 Interrupt",null,"X","X"]
[{"$nulls":18},14,"0x1C","TCB0_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X"]
["0x001C","GPR","General Purpose Registers","0x00","GPIOR0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,15,"0x1E","TCB1_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x01","GPIOR1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,16,"0x20","TCD0_OVF","Timer Counter Type D Overflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","GPIOR2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,17,"0x22","TCD0_TRIG","Timer Counter Type D Trigger Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","GPIOR3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,18,"0x24","TWI0_TWIS","Two-Wire Interface Client Interrupt",null,"X","X"]
[{"$nulls":18},19,"0x26","TWI0_TWIM","Two-Wire Interface Host Interrupt",null,"X","X"]
["0x0030","CPU","CPU","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,20,"0x28","SPI0_INT","Serial Peripheral Interface Interrupt",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,21,"0x2A","USART0_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,22,"0x2C","USART0_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X"]
[{"$nulls":14},"X","X",null,null,23,"0x2E","USART0_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x04","CCP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,24,"0x30","PORTD_PORT","PORTD External Interrupt",null,"X","X"]
[{"$nulls":14},"X","X",null,null,25,"0x32","AC0_AC","Analog Comparator Interrupt",null,"X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,26,"0x34","ADC0_RESRDY","Analog-to-Digital Converter Result Ready Interrupt",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,27,"0x36","ADC0_WCMP","Analog-to-Digital Converter Window Compare Interrupt",null,"X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,28,"0x38","ZCD3_ZCD","Zero-Cross Interrupt",null,"X","X"]
[{"$nulls":14},"X","X",null,null,29,"0x3C","PORTC_PORT","PORTC External Interrupt",null,"X","X"]
[{"$nulls":3},"0x0B","RAMPZ","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,30,"0x3E","TCB2_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,31,"0x40","USART1_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x0D","SP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,32,"0x42","USART1_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X",null,null,33,"0x44","USART1_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x0F","SREG","I","T","H","S","V","N","Z","C",null,"X","X",null,null,34,"0x46","PORTF_PORT","PORTF External Interrupt",null,"X","X"]
[{"$nulls":18},35,"0x48","NVMCTRL_EE","Nonvolatile Memory Controller EEPROM Ready Interrupt",null,"X","X"]
["0x0040","RSTCTRL","Reset Controller","0x00","RSTFR","-","-","UPDIRF","SWRF","WDRF","EXTRF","BORF","PORF",null,"X","X",null,null," "]
[{"$nulls":3},"0x01","SWRR","-","-","-","-","-","-","-","SWRST",null,"X","X",{"$nulls":3},"modified"]
[{"$nulls":14}," "," ",{"$nulls":3},"reduced"]
["0x0050","SLPCTRL","Sleep Controller","0x00","CTRLA","-","-","-","-","SMODE[2]","SMODE[1]","SMODE[0]","SEN",null,"X","X"]
[{"$nulls":3},"0x01","VREGCTRL","-","-","HTLLEN","-","-","PMODE[2]","PMODE[1]","PMODE[0]",null,"X","X"]
[]
["0x0060","CLKCTRL","Clock Controller","0x00","MCLKCTRLA","CLKOUT","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X"]
[{"$nulls":3},"0x01","MCLKCTRLB","-","-","-","PDIV[3]","PDIV[2]","PDIV[1]","PDIV[0]","PEN",null,"X","X"]
["add",null,null,"0x02","MCLKCTRLC"," ","-","-","-","CFDSRC[1]","CFDSRC[0]","CFDTST","CFDEN",null,"X","X"]
[{"$nulls":3},"0x03","MCLKINTCTRL","INTTYPE","-","-","-","-","-","-","CFD",null,"X","X"]
["add",null,null,"0x04","MCLKINTFLAGS","-","-","-","-","-","-","-","CFD",null,"X","X"]
["add",null,null,"0x05","MCLKSTATUS","-","-","PLLS","EXTS","XOSC32KS","OSC32KS","OSCHFS","SOSC",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","OSCHFCTRLA","RUNSTDBY","-","FRQSEL[3]","FRQSEL[2]","FRQSEL[1]","FRQSEL[0]","-","AUTOTUNE",null,"X","X"]
[{"$nulls":3},"0x09","OSCHFTUNE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","PLLCTRLA","RUNSTDBY","SOURCE","-","-","-","-","MULFAC[1]","MULFAC[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x11","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x18","OSC32KCTRLA","RUNSTDBY","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x19","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1B","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1C","XOSC32KCTRLA","RUNSTDBY","-","CSUT[1]","CSUT[0]","-","SEL","LPMODE","ENABLE",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
["add",null,null,"0x20","XOSCHFCTRLA","RUNSTDBY","-","CSUTHF[1]","CSUTHF[0]","FRQRANGE[1]","FRQRANGE[0]","SELHF","ENABLE",null,"X","X"]
[{"$nulls":14},"  "," "]
["0x00A0","BOD","Brown-Out Reset Detector","0x00","CTRLA","-","-","-","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","LVL[2]","LVL[1]","LVL[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","VLMCTRLA","-","-","-","-","-","-","VLMLVL[1]","VLMLVL[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTCTRL","-","-","-","-","-","VLMCFG[1]","VLMCFG[0]","VLMIE",null,"X","X"]
[{"$nulls":3},"0x0A","INTFLAGS","-","-","-","-","-","-","-","VLMIF",null,"X","X"]
["mod addr, name",null,null,"0x0B","STATUS","-","-","-","-","-","-","-","VLMS",null,"X","X"]
[{"$nulls":14}," "," "]
["0x00B0","VREF","Voltage Reference","0x00","ADC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x02","DAC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["mod addr",null,null,"0x04","ACREF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X"]
[]
["0x00C0","MVIO","Multi-Voltage I/O Controller","0x00","INTCTRL","-","-","-","-","-","-","-","VDDIO2IE",null,"X","X"]
[{"$nulls":3},"0x01","INTFLAGS","-","-","-","-","-","-","-","VDDIO2IF",null,"X","X"]
["new",null,null,"0x02","STATUS","-","-","-","-","-","-","-","VDDIO2S",null,"X","X"]
[]
["…","Reserved"]
[]
["0x0100","WDT","Watchdog Timer","0x00","CTRLA","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X"]
["ok",null,null,"0x01","STATUS","LOCK","-","-","-","-","-","-","SYNCBUSY",null,"X","X"]
[]
["0x0110","CPUINT","Interrupt Controller","0x00","CTRLA","-","IVSEL","CVT","-","-","-","-","LVL0RR",null,"X","X"]
[{"$nulls":3},"0x01","STATUS","NMIEX","-","-","-","-","-","LVL1EX","LVL0EX",null,"X","X"]
[{"$nulls":3},"0x02","LVL0PRI","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x03","LVL1VEC","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0120","CRCSCAN","Cyclic Redundancy Check Memory Scan","0x00","CTRLA","RESET","-","-","-","-","-","NMIEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","SRC[1:0]","SRC[1:0]",null,"X","X"]
["ok",null,null,"0x02","STATUS","-","-","-","-","-","-","OK","BUSY",null,"X","X"]
[]
["…","Reserved"]
[]
["0x0140","RTC","Real-Time Counter","0x00","CTRLA","RUNSTDBY","PRESCALER[3]","PRESCALER[2]","PRESCALER[1]","PRESCALER[0]","CORREN","-","RTCEN",null,"X","X"]
[{"$nulls":3},"0x01","STATUS","-","-","-","-","CMPBUSY","PERBUSY","CNTBUSY","CTRLABUSY",null,"X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","CMP","OVF",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","-","-","-","-","-","-","CMP","OVF",null,"X","X"]
[{"$nulls":3},"0x04","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x06","CALIB","SIGN","ERROR[6]","ERROR[5]","ERROR[4]","ERROR[3]","ERROR[2]","ERROR[1]","ERROR[0]",null,"X","X"]
[{"$nulls":3},"0x07","CLKSEL","-","-","-","-","-","-","CLKSEL[1]","CLKSEL[0]",null,"X","X"]
[{"$nulls":3},"0x08","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0A","PER]","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0E","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","PITCTRLA","-","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]","-","-","PITEN",null,"X","X"]
[{"$nulls":3},"0x11","PITSTATUS","-","-","-","-","-","-","-","CTRLBUSY",null,"X","X"]
[{"$nulls":3},"0x12","PITINTCTRL","-","-","-","-","-","-","-","PI",null,"X","X"]
[{"$nulls":3},"0x13","PITINTFLAGS","-","-","-","-","-","-","-","PI",null,"X","X"]
[{"$nulls":3},"0x14","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["ok",null,null,"0x15","PITDBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[]
["…","Reserved"]
[]
["0x01C0","CCL","Configurable Custom Logic","0x00","CTRLA","-","RUNSTDBY","-","-","-","-","-","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","SEQCTRL0","-","-","-","-","SEQSEL0[3]","SEQSEL0[2]","SEQSEL0[1]","SEQSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x02","SEQCTRL1","-","-","-","-","SEQSEL1[3]","SEQSEL1[2]","SEQSEL1[1]","SEQSEL1[0]",null,"X","X"]
["unused",null,null,"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL0","INTMODE3[1]","INTMODE3[0]","INTMODE2[1]","INTMODE2[0]","INTMODE1[1]","INTMODE1[0]","INTMODE0[1]","INTMODE0[0]",null,"X","X"]
["unused",null,null,"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["reduced",null,null,"0x07","INTFLAGS","-","-","-","-","INT3","INT2","INT1","INT0",null,"X","X"]
[{"$nulls":3},"0x08","LUT0CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x09","LUT0CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x0A","LUT0CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
[{"$nulls":3},"0x0B","TRUTH0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0C","LUT1CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x0D","LUT1CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL0[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x0E","LUT1CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
[{"$nulls":3},"0x0F","TRUTH1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x10","LUT2CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x11","LUT2CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x12","LUT2CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
[{"$nulls":3},"0x13","TRUTH2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x14","LUT3CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x15","LUT3CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x16","LUT3CTRLC",{"$nulls":4},"INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
["mod reduced, 4,5 omitted",null,null,"0x17","TRUTH3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0200","EVSYS","Event System","0x00","SWEVENTA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","SWEVENTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","CHANNEL0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x11","CHANNEL1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x12","CHANNEL2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x13","CHANNEL3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x14","CHANNEL4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x15","CHANNEL5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
["omitted ch 6..9",null,null,"0x16","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x20","USERCCLLUT0A","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"...","…",{"$nulls":6},"-","-",null,"X","X"]
["mod reduced","new USERTCD0INPUTB",null,"0x38","USERTCD0INPUTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0400","PORTA","Port A Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["0x0440","PORTC","Port C Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["0x0460","PORTD","Port D Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["0x04A0","PORTF","Port F Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["0x05E0","PORTMUX","Port Multiplexer","0x00","EVSYSROUTEA","-","-","EVOUTF","-","EVOUTD","-","-","EVOUTA",null,"X","X"]
[{"$nulls":3},"0x01","CCLROUTEA","-","-","-","-","-","LUT2","LUT1","LUT0",null,"X","X"]
[{"$nulls":3},"0x02","USARTROUTEA","-","-","-","USART1[1]","USART1[0]","USART0[2]","USART0[1]","USART0[0]",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved",{"$nulls":3},"-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x05","SPIROUTEA","-","-","-","-","-","-","SPI0[1]","SPI0[0]",null,"X","X"]
[{"$nulls":3},"0x06","TWIROUTEA","-","-","-","-","-","-","TWI0[1]","TWI0[0]",null,"X","X"]
[{"$nulls":3},"0x07","TCAROUTEA","-","-","-","-","-","TCA0[2]","TCA0[1]","TCA0[0]",null,"X","X"]
[{"$nulls":3},"0x08","TCBROUTEA","-","-","-","-","-","-","TCB1","TCB0",null,"X","X"]
["reduced",null,"-USARTROUTEB, -ACROUTEA, -ZCDROUTEA","0x09","TCDROUTEA","-","-","-","-","-","TCD0[2]","TCD0[1]","TCD0[0]",null,"X","X"]
[]
["0x0600","ADC0","Analog to-Digital Converter 0","0x00","CTRLA","RUNSTDBY","-","CONVMODE","LEFTADJ","RESSEL[1]","RESSEL[0]","FREERUN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","SAMPNUM[2]","SAMPNUM[1]","SAMPNUM[0]",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","PRESC[3]","PRESC[2]","PRESC[1]","PRESC[0]",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","INITDLY[2]","INITDLY[1]","INITDLY[0]","-","SAMPDLY[3]","SAMPDLY[2]","SAMPDLY[1]","SAMPDLY[0]",null,"X","X"]
[{"$nulls":3},"0x04","CTRLE","-","-","-","-","-","WINCM[2]","WINCM[1]","WINCM[0]",null,"X","X"]
[{"$nulls":3},"0x05","SAMPCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","MUXPOS","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","MUXNEG","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","COMMAND","-","-","-","-","-","-","SPCONV","STCONV",null,"X","X"]
[{"$nulls":3},"0x0B","EVCTRL","-","-","-","-","-","-","-","STARTEI",null,"X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x10","RES","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x12","WINLT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x14","WINHT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0680","AC0","Analog Comparator 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X"]
["reduced -CTRLB -Winstate[1:0] ",null,null,"0x07","STATUS","-","-","-","CMPSTATE","-","-","-","CMPIF",null,"X","X"]
[]
["0x06A0","DAC0","Digital-to-Analog converter 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","-","-","-","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x02","DATA","[1]","[0]","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":4}," ","[9]","[8]","[7]","[6]","[5]","[4]","[3]","[2]",null,"X","X"]
[]
["0x06D8","ZCD3 ","Zero-Cross Detector 3","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",null,"X","X"]
["addr",null,null,"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",null,"X","X"]
[]
["0x0800","USART0","Universal Sync. and Async RX TX 0","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0820","USART1","Universal Sync. and Async RX TX 1","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0900","TWI0","Two-Wire Interface 0","0x00","CTRLA","-","INPUTLVL","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,"X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","INPUTLVL","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,"X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1]","BUSSTATE[0]",null,"X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,"X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,"X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,"X","X"]
[]
["0x0940","SPI0","Serial Peripheral Interface 0","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X"]
["ok",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0A00","TCA0 – [ Normal Mode ]","Timer/Counter Type A - instance 0 – [ Normal Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x09","EVCTRL","EVACTB[2]","EVACTB[1]","EVACTB[0]","CNTBEI","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",null,"X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0A00","TCA0 – [ Split Mode ]","Timer/Counter Type A - instance 0 – [ Split Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0B00","TCB0","Timer/Counter Type B - instance 0","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0B10","TCB1","Timer/Counter Type B - instance 1","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0B20","TCB2","Timer/Counter Type B - instance 2","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0B80","TCD0","Timer/Counter Type D - instance 0","0x00","CTRLA","-","CLKSEL[1]","CLKSEL[0]","CNTPRES[1]","CNTPRES[0]","SYNCPRES[1]","SYNCPRES[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WGMODE[1]","WGMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","CMPDSEL","CMPCSEL","-","-","FIFTY","-","AUPDATE","CMPOVR",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","CMPBVAL[3]","CMPBVAL[2]","CMPBVAL[1]","CMPBVAL[0]","CMPAVAL[3]","CMPAVAL[2]","CMPAVAL[1]","CMPAVAL[0]",null,"X","X"]
[{"$nulls":3},"0x04","CTRLE","DISEOC","-","-","SCAPTUREB","SCAPTUREA","RESTART","SYNC","SYNCEOC",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","EVCTRLA","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X"]
[{"$nulls":3},"0x09","EVCTRLB","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0B","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X"]
[{"$nulls":3},"0x0E","STATUS","PWMACTB","PWMACTA","-","-","-","-","CMDRDY","ENRDY",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x10","INPUTCTRLA","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x11","INPUTCTRLB","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[3]",null,"X","X"]
[{"$nulls":3},"0x12","FAULTCTRL","CMPDEN","CMPCEN","CMPBEN","CMPAEN","CMPD","CMPC","CMPB","CMPA",null,"X","X"]
[{"$nulls":3},"0x13","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x14","DLYCTRL","-","-","DLYPRESC[1]","DLYPRESC[0]","DLYTRIG[1]","DLYTRIG[0]","DLYSEL[1]","DLYSEL[0]",null,"X","X"]
[{"$nulls":3},"0x15","DLYVAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
[{"$nulls":3},"0x16","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x18","DITCTRL","-","-","-","-","-","-","DITHERSEL[1]","DITHERSEL[0]",null,"X","X"]
[{"$nulls":3},"0x19","DITVAL","-","-","-","-","DITHER[3]","DITHER[2]","DITHER[1]","DITHER[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1E","DBGCTRL","-","-","-","-","-","FAULTDET","-","DBGRUN",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x21","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x22","CAPTUREA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x24","CAPTUREB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x26","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x27","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x28","CMPASET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2A","CMPACLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2C","CMPBSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
["ok",null,null,"0x2E","CMPBCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0F00","SYSCFG","System Configuration","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["ok",null,null,"0x01","REVID","MAJOR[3]","MAJOR[2]","MAJOR[1]","MAJOR[0]","MINOR[3]","MINOR[2]","MINOR[1]","MINOR[0]",null,"X","X"]
[]
["0x1000","NVMCTRL","Nonvolatile Memory Controller","0x00","CTRLA","-","CMD[6]","CMD[5]","CMD[4]","CMD[3]","CMD[2]","CMD[1]","CMD[0]",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","FLMAPLOCK","-","FLMAP[1]","FLMAP[0]","-","APPDATAWP","BOOTRP","APPCODEWP",null,"X","X"]
[{"$nulls":3},"0x02","STATUS","-","ERROR[2]","ERROR[1]","ERROR[0]","-","-","EEBUSY","FBUSY",null,"X","X"]
[{"$nulls":3},"0x03","INTCTRL","-","-","-","-","-","-","-","EEREADY",null,"X","X"]
[{"$nulls":3},"0x04","INTFLAGS","-","-","-","-","-","-","-","EEREADY",null,"X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x06","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"X","X"]
[{"$nulls":3},"0x08","ADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
["ok",{"$nulls":3}," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X"]
[]
["0x1040","LOCK","Lock Bits","0x00","KEY","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3}," "," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3}," "," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X"]
["ok",null,null," "," ","[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X"]
[]
["0x1050","FUSE","Configuration and User Fuses","0x00","WDTCFG","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X"]
[{"$nulls":3},"0x01","BODCFG","LVL[2]","LVL[1]","LVL[0]","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X"]
[{"$nulls":3},"0x02","OSCCFG","-","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x05","SYSCFG0","CRCSRC[1]","CRCSRC[0]","CRCSEL","-","RSTPINCFG[1]","RSTPINCFG[0]","-","EESAVE",null,"X","X"]
[{"$nulls":3},"0x06","SYSCFG1","-","-","-","-","-","SUT[2]","SUT[1]","SUT[0]",null,"X","X"]
[{"$nulls":3},"0x07","CODESIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x08","BOOTSIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x1080","USERROW","User Row","0x00",null,"[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":5},"[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X"]
["ok",{"$nulls":4},"[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X"]
[]
["0x1100","SIGROW","Signature Row – [ READ ONLY  ]","0x00","DEVICEID0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DEVICEID1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DEVICEID2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","TEMPSENSE0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x06","TEMPSENSE1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","SERNUM0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"...","…","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x1F","SERNUM15","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["WITHOUT ANY WARRANTY"]
[]
[]
["Features"]
[]
["• AVR® CPU"]
["  – Running at up to 24 MHz"]
["  – Single-cycle I/O access"]
["  – Two-level interrupt controller"]
["  – Two-cycle hardware multiplier  "]
["  – Supply voltage range: 1.8V to 5.5V"]
[]
["• Memories"]
["  – 64 KB in-system self-programmable Flash memory"]
["  – 256B EEPROM"]
["  – 8 KB SRAM"]
["  – 32B of user row in nonvolatile memory that can keep data during chip erase and can be programmed while the device is locked"]
["  – Write/erase endurance"]
["     • Flash 1,000 cycles"]
["     • Flash 1,000 cycles"]
["  – Data retention: 40 years at 55°C"]
[]
["• System"]
["  – Power-on Reset (POR) circuit"]
["  – Brown-out Detector (BOD)"]
["  – Clock options"]
["     • High-precision internal high-frequency oscillator with selectable frequency up to 24 MHz (OSCHF)"]
["       – Auto-tuning for improved internal oscillator accuracy"]
["     • Internal PLL up to 48 MHz for high-frequency operation of Timer/Counter type D (PLL)"]
["     • 32.768 kHz ultra-low power internal oscillator (OSC32K)"]
["     • 32.768 kHz external crystal oscillator (XOSC32K)"]
["     • External clock input"]
["     • External high-frequency crystal oscillator (XOSCHF) with Clock Failure Detection"]
["  – Single-pin Unified Program and Debug Interface (UPDI)"]
["  – Three sleep modes"]
["     • Idle with all peripherals running for immediate wake-up"]
["     • Standby with a configurable operation of selected peripherals"]
["     • Power-Down with full data retention"]
["  – Automated Cyclic Redundancy Check (CRC) Flash memory scan"]
["  – Watchdog Timer (WDT) with Window mode, with a separate on-chip oscillator"]
["  – External interrupt on all general purpose pins"]
[]
["• Peripherals"]
["  – One 16-bit Timer/Counter type A (TCA) with three compare channels for PWM and waveform generation"]
["  – Three 16-bit Timer/Counter type B (TCB) with input capture and signal measurements"]
["  – One 12-bit PWM Timer/Counter type D (TCD) optimized for power control"]
["  – One 16-bit Real-Time Counter (RTC) that can run from an external crystal or internal oscillator"]
["  – Two USARTs"]
["     • Operation modes: RS-485, LIN client, host SPI, and IrDA"]
["     • Fractional baud rate generator, auto-baud, and start-of-frame detection"]
["  – One SPI with host/client operation modes"]
["  – One Two-Wire Interface (TWI) with dual address match"]
["     • Simultaneous host/client operation (Dual mode)"]
["     • Philips I2C compatible"]
["     • Standard mode (Sm, 100 kHz)"]
["     • Fast mode (Fm, 400 kHz)"]
["     • Fast mode Plus (Fm+, 1 MHz) (1)"]
["  – Event System for CPU independent and predictable inter-peripheral signaling"]
["  – Configurable Custom Logic (CCL) with four programmable Look-up Tables (LUTs)"]
["  – One 12-bit differential 130 ksps Analog-to-Digital Converter (ADC)"]
["  – One 10-bit Digital-to-Analog Converter (DAC)"]
["  – One Analog Comparator (AC)"]
["  – One Zero-Cross Detector (ZCD)"]
["  – Internal 1.024V, 2.048V, 2.500V and 4.096V voltage references, and external reference option (VREF)"]
[]
["  • I/O and Packages:"]
["    – Multi-Voltage I/O (MVIO) on I/O port C"]
["    – Selectable input voltage threshold"]
["    – Up to 27/26 programmable I/O pins"]
["    – 32-pin VQFN 5x5 mm and TQFP 7x7 mm"]
["    – 28-pin SPDIP, SSOP, SOIC and VQFN"]
[]
["  • Temperature Ranges:"]
["    – Industrial: -40°C to +85°C"]
["    – Extended: -40°C to +125°C"]
[]
["  Note: "]
["  1. I2C Fm+ is only supported for 2.7V and above."]

{"sheet":"AVR16|32-DD-28-32","index":3,"n_rows":781,"n_cols":25,"rows_kept":781,"flags":["formulas_cached_only"]}
["AVR16|32-DD-28-32"," [ 04-2023 ]"]
["Peripherals and Architecture"]
[]
[]
["Table 9-1. Peripheral Address Map",{"$nulls":17},"Table","  8-3. Interrupt Vector Mapping"]
[{"$nulls":18},"***********************************************************************************************************************************************************************"]
["Base Address","Name","Description","Offset","Name","Bit 7","Bit 6"," Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0",null,"28-Pin","32-Pin",null,null,"Vector","Program",{"$nulls":3},"28-Pin","32-Pin"]
[{"$nulls":18},"Number","Address","Peripheral","Description"]
["0x0000","VPORTA","Virtual Port A","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,0,"0x00","RESET","Reset",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,1,"0x02","NMI","Non-Maskable Interrupt available for CRCSCAN, CFD",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,2,"0x04","BOD_VLM","Voltage Level Monitor Interrupt",null,"X","X"]
[{"$nulls":18},3,"0x06","CLKCTRL_CFD","External_crystal_oscillator/clock_source_failure_Interrupt",null,"X","X"]
["0x0008","VPORTC","Virtual Port C","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,4,"0x08","MVIO_MVIO","Multi-Voltage_Input/Output_Interrupt",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,5,"0x0A","RTC_CNT","Real-Time Counter Overflow or Compare Match Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,6,"0x0C","RTC_PIT","Real-Time Counter Periodic Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,7,"0x0E","CCL_CCL","Configurable Custom Logic Interrupt",null,"X","X"]
[{"$nulls":18},8,"0x10","PORTA_PORT","PORTA External interrupt",null,"X","X"]
["0x000C","VPORTD","Virtual Port D","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,9,"0x12","TCA0_OVF","OVF Normal: Timer/Counter Type A Overflow Interrupt ",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,9,"0x12","TCA0_LUNF","Split:     Timer/Counter Type A Low Underflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,10,"0x14","TCA0_HUNF","Normal: Unused",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,10,"0x14","TCA0_HUNF","Split:     Timer/Counter Type A High Underflow Interrupt",null,"X","X"]
[{"$nulls":18},11,"0x16","TCA0_CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"X","X"]
["0x0014 ","VPORTF","Virtual Port F","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,11,"0x16","TCA0_LCMP0","Split:     Timer/Counter Type A Low Compare 0 Interrupt",null,"X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,12,"0x18","TCA0_CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,12,"0x18","TCA0_LCMP1","Split:     Timer/Counter Type A Low Compare 1 Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,13,"0x1A","TCA0_CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"X","X"]
[{"$nulls":18},13,"0x1A","TCA0_LCMP2","Split: Timer/Counter Type A Low Compare 2 Interrupt",null,"X","X"]
[{"$nulls":18},14,"0x1C","TCB0_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X"]
["0x001C","GPR","General Purpose Registers","0x00","GPIOR0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,15,"0x1E","TCB1_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x01","GPIOR1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,16,"0x20","TCD0_OVF","Timer Counter Type D Overflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x02","GPIOR2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,17,"0x22","TCD0_TRIG","Timer Counter Type D Trigger Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","GPIOR3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,18,"0x24","TWI0_TWIS","Two-Wire Interface Client Interrupt",null,"X","X"]
[{"$nulls":18},19,"0x26","TWI0_TWIM","Two-Wire Interface Host Interrupt",null,"X","X"]
["0x0030","CPU","CPU","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,20,"0x28","SPI0_INT","Serial Peripheral Interface Interrupt",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,21,"0x2A","USART0_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,22,"0x2C","USART0_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X"]
[{"$nulls":14},"X","X",null,null,23,"0x2E","USART0_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x04","CCP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,24,"0x30","PORTD_PORT","PORTD External Interrupt",null,"X","X"]
[{"$nulls":14},"X","X",null,null,25,"0x32","AC0_AC","Analog Comparator Interrupt",null,"X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,26,"0x34","ADC0_RESRDY","Analog-to-Digital Converter Result Ready Interrupt",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,27,"0x36","ADC0_WCMP","Analog-to-Digital Converter Window Compare Interrupt",null,"X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,28,"0x38","ZCD3_ZCD","Zero-Cross Interrupt",null,"X","X"]
[{"$nulls":14},"X","X",null,null,29,"0x3C","PORTC_PORT","PORTC External Interrupt",null,"X","X"]
[{"$nulls":3},"0x0B","RAMPZ","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,30,"0x3E","TCB2_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X",null,null,31,"0x40","USART1_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x0D","SP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X",null,null,32,"0x42","USART1_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X",null,null,33,"0x44","USART1_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X"]
[{"$nulls":3},"0x0F","SREG","I","T","H","S","V","N","Z","C",null,"X","X",null,null,34,"0x46","PORTF_PORT","PORTF External Interrupt",null,"X","X"]
[{"$nulls":18},35,"0x48","NVMCTRL_EE","Nonvolatile Memory Controller EEPROM Ready Interrupt",null,"X","X"]
[{"$nulls":18}," "]
["0x0040","RSTCTRL","Reset Controller","0x00","RSTFR","-","-","UPDIRF","SWRF","WDRF","EXTRF","BORF","PORF",null,"X","X",{"$nulls":3},"modified"]
[{"$nulls":3},"0x01","SWRR","-","-","-","-","-","-","-","SWRST",null,"X","X",{"$nulls":3},"reduced"]
[{"$nulls":14}," "," "]
["0x0050","SLPCTRL","Sleep Controller","0x00","CTRLA","-","-","-","-","SMODE[2]","SMODE[1]","SMODE[0]","SEN",null,"X","X"]
[{"$nulls":3},"0x01","VREGCTRL","-","-","HTLLEN","-","-","PMODE[2]","PMODE[1]","PMODE[0]",null,"X","X"]
[]
["0x0060","CLKCTRL","Clock Controller","0x00","MCLKCTRLA","CLKOUT","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X"]
[{"$nulls":3},"0x01","MCLKCTRLB","-","-","-","PDIV[3]","PDIV[2]","PDIV[1]","PDIV[0]","PEN",null,"X","X"]
["add",null,null,"0x02","MCLKCTRLC"," ","-","-","-","CFDSRC[1]","CFDSRC[0]","CFDTST","CFDEN",null,"X","X"]
[{"$nulls":3},"0x03","MCLKINTCTRL","INTTYPE","-","-","-","-","-","-","CFD",null,"X","X"]
["add",null,null,"0x04","MCLKINTFLAGS","-","-","-","-","-","-","-","CFD",null,"X","X"]
["add",null,null,"0x05","MCLKSTATUS","-","-","PLLS","EXTS","XOSC32KS","OSC32KS","OSCHFS","SOSC",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","OSCHFCTRLA","RUNSTDBY","-","FRQSEL[3]","FRQSEL[2]","FRQSEL[1]","FRQSEL[0]","-","AUTOTUNE",null,"X","X"]
[{"$nulls":3},"0x09","OSCHFTUNE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","PLLCTRLA","RUNSTDBY","SOURCE","-","-","-","-","MULFAC[1]","MULFAC[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x11","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x18","OSC32KCTRLA","RUNSTDBY","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x19","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1B","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1C","XOSC32KCTRLA","RUNSTDBY","-","CSUT[1]","CSUT[0]","-","SEL","LPMODE","ENABLE",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
["add",null,null,"0x20","XOSCHFCTRLA","RUNSTDBY","-","CSUTHF[1]","CSUTHF[0]","FRQRANGE[1]","FRQRANGE[0]","SELHF","ENABLE",null,"X","X"]
[]
["0x00A0","BOD","Brown-Out Reset Detector","0x00","CTRLA","-","-","-","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","LVL[2]","LVL[1]","LVL[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","VLMCTRLA","-","-","-","-","-","-","VLMLVL[1]","VLMLVL[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTCTRL","-","-","-","-","-","VLMCFG[1]","VLMCFG[0]","VLMIE",null,"X","X"]
[{"$nulls":3},"0x0A","INTFLAGS","-","-","-","-","-","-","-","VLMIF",null,"X","X"]
["mod addr, name",null,null,"0x0B","STATUS","-","-","-","-","-","-","-","VLMS",null,"X","X"]
[]
["0x00B0","VREF","Voltage Reference","0x00","ADC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x02","DAC0REF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["mod addr",null,null,"0x04","ACREF","ALWAYSON","-","-","-","-","REFSEL[2]","REFSEL[1]","REFSEL[0]",null,"X","X"]
[]
["0x00C0","MVIO","Multi-Voltage I/O Controller","0x00","INTCTRL","-","-","-","-","-","-","-","VDDIO2IE",null,"X","X"]
[{"$nulls":3},"0x01","INTFLAGS","-","-","-","-","-","-","-","VDDIO2IF",null,"X","X"]
["new",null,null,"0x02","STATUS","-","-","-","-","-","-","-","VDDIO2S",null,"X","X"]
[]
["…","Reserved"]
[]
["0x0100","WDT","Watchdog Timer","0x00","CTRLA","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X"]
["ok",null,null,"0x01","STATUS","LOCK","-","-","-","-","-","-","SYNCBUSY",null,"X","X"]
[]
["…"]
[]
["0x0110","CPUINT","Interrupt Controller","0x00","CTRLA","-","IVSEL","CVT","-","-","-","-","LVL0RR",null,"X","X"]
[{"$nulls":3},"0x01","STATUS","NMIEX","-","-","-","-","-","LVL1EX","LVL0EX",null,"X","X"]
[{"$nulls":3},"0x02","LVL0PRI","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x03","LVL1VEC","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0120","CRCSCAN","Cyclic Redundancy Check Memory Scan","0x00","CTRLA","RESET","-","-","-","-","-","NMIEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","SRC[1:0]","SRC[1:0]",null,"X","X"]
["ok",null,null,"0x02","STATUS","-","-","-","-","-","-","OK","BUSY",null,"X","X"]
[]
["…"]
[]
["0x0140","RTC","Real-Time Counter","0x00","CTRLA","RUNSTDBY","PRESCALER[3]","PRESCALER[2]","PRESCALER[1]","PRESCALER[0]","CORREN","-","RTCEN",null,"X","X"]
[{"$nulls":3},"0x01","STATUS","-","-","-","-","CMPBUSY","PERBUSY","CNTBUSY","CTRLABUSY",null,"X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","CMP","OVF",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","-","-","-","-","-","-","CMP","OVF",null,"X","X"]
[{"$nulls":3},"0x04","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x06","CALIB","SIGN","ERROR[6]","ERROR[5]","ERROR[4]","ERROR[3]","ERROR[2]","ERROR[1]","ERROR[0]",null,"X","X"]
[{"$nulls":3},"0x07","CLKSEL","-","-","-","-","-","-","CLKSEL[1]","CLKSEL[0]",null,"X","X"]
[{"$nulls":3},"0x08","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0A","PER]","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0E","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","PITCTRLA","-","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]","-","-","PITEN",null,"X","X"]
[{"$nulls":3},"0x11","PITSTATUS","-","-","-","-","-","-","-","CTRLBUSY",null,"X","X"]
[{"$nulls":3},"0x12","PITINTCTRL","-","-","-","-","-","-","-","PI",null,"X","X"]
[{"$nulls":3},"0x13","PITINTFLAGS","-","-","-","-","-","-","-","PI",null,"X","X"]
[{"$nulls":3},"0x14","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["ok",null,null,"0x15","PITDBGCTRL","-","-","-","-","-","-","-","DBGRUN"]
[]
["…","Reserved"]
[]
["0x01C0","CCL","Configurable Custom Logic","0x00","CTRLA","-","RUNSTDBY","-","-","-","-","-","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","SEQCTRL0","-","-","-","-","SEQSEL0[3]","SEQSEL0[2]","SEQSEL0[1]","SEQSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x02","SEQCTRL1","-","-","-","-","SEQSEL1[3]","SEQSEL1[2]","SEQSEL1[1]","SEQSEL1[0]",null,"X","X"]
["unused",null,null,"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL0","INTMODE3[1]","INTMODE3[0]","INTMODE2[1]","INTMODE2[0]","INTMODE1[1]","INTMODE1[0]","INTMODE0[1]","INTMODE0[0]",null,"X","X"]
["unused",null,null,"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["reduced",null,null,"0x07","INTFLAGS","-","-","-","-","INT3","INT2","INT1","INT0",null,"X","X"]
[{"$nulls":3},"0x08","LUT0CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x09","LUT0CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x0A","LUT0CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
[{"$nulls":3},"0x0B","TRUTH0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0C","LUT1CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x0D","LUT1CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL0[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x0E","LUT1CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
[{"$nulls":3},"0x0F","TRUTH1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x10","LUT2CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x11","LUT2CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x12","LUT2CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
[{"$nulls":3},"0x13","TRUTH2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x14","LUT3CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x15","LUT3CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X"]
[{"$nulls":3},"0x16","LUT3CTRLC",{"$nulls":4},"INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X"]
["mod reduced, 4,5 omitted",null,null,"0x17","TRUTH3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0200","EVSYS","Event System","0x00","SWEVENTA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","SWEVENTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","CHANNEL0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x11","CHANNEL1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x12","CHANNEL2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x13","CHANNEL3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x14","CHANNEL4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x15","CHANNEL5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
["omitted ch 6..9",null,null,"0x16","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x20","USERCCLLUT0A","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"...","…",{"$nulls":6},"-","-",null,"X","X"]
["mod reduced","new USERTCD0INPUTB",null,"0x38","USERTCD0INPUTB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0400","PORTA","Port A Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["…"]
[]
["0x0440","PORTC","Port C Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["…"]
[]
["0x0460","PORTD","Port D Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["…"]
[]
["0x04A0","PORTF","Port F Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X"]
["add INLVL",null,null,"0x0B","PINCONFIG","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["add INLVL",null,null,"0x10","PIN0CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x11","PIN1CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x12","PIN2CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x13","PIN3CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x14","PIN4CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x15","PIN5CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x16","PIN6CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
["add INLVL",null,null,"0x17","PIN7CTRL","INVEN","INLVL","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X"]
[]
["…"]
[]
["0x05E0","PORTMUX","Port Multiplexer","0x00","EVSYSROUTEA","-","-","EVOUTF","-","EVOUTD","-","-","EVOUTA",null,"X","X"]
[{"$nulls":3},"0x01","CCLROUTEA","-","-","-","-","-","LUT2","LUT1","LUT0",null,"X","X"]
[{"$nulls":3},"0x02","USARTROUTEA","-","-","-","USART1[1]","USART1[0]","USART0[2]","USART0[1]","USART0[0]",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved",{"$nulls":3},"-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x05","SPIROUTEA","-","-","-","-","-","SPI0[2]","SPI0[1]","SPI0[0]",null,"X","X"]
[{"$nulls":3},"0x06","TWIROUTEA","-","-","-","-","-","-","TWI0[1]","TWI0[0]",null,"X","X"]
[{"$nulls":3},"0x07","TCAROUTEA","-","-","-","-","-","TCA0[2]","TCA0[1]","TCA0[0]",null,"X","X"]
[{"$nulls":3},"0x08","TCBROUTEA","-","-","-","-","-","-","TCB1","TCB0",null,"X","X"]
["reduced",null,"-USARTROUTEB, -ACROUTEA, -ZCDROUTEA","0x09","TCDROUTEA","-","-","-","-","-","TCD0[2]","TCD0[1]","TCD0[0]",null,"X","X"]
[]
["…"]
[]
["0x0600","ADC0","Analog to-Digital Converter 0","0x00","CTRLA","RUNSTDBY","-","CONVMODE","LEFTADJ","RESSEL[1]","RESSEL[0]","FREERUN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","SAMPNUM[2]","SAMPNUM[1]","SAMPNUM[0]",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","PRESC[3]","PRESC[2]","PRESC[1]","PRESC[0]",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","INITDLY[2]","INITDLY[1]","INITDLY[0]","-","SAMPDLY[3]","SAMPDLY[2]","SAMPDLY[1]","SAMPDLY[0]",null,"X","X"]
[{"$nulls":3},"0x04","CTRLE","-","-","-","-","-","WINCM[2]","WINCM[1]","WINCM[0]",null,"X","X"]
[{"$nulls":3},"0x05","SAMPCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","MUXPOS","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","MUXNEG","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","COMMAND","-","-","-","-","-","-","SPCONV","STCONV",null,"X","X"]
[{"$nulls":3},"0x0B","EVCTRL","-","-","-","-","-","-","-","STARTEI",null,"X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x10","RES","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x12","WINLT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x14","WINHT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["…"]
[]
["0x0680","AC0","Analog Comparator 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","POWER[1]","POWER[0]","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","INITVAL","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]","MUXNEG[2]","MUXNEG[1]","MUXNEG[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x05","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","INTMODE[1]","INTMODE[0]","-","-","-","CMP",null,"X","X"]
["reduced -CTRLB -Winstate[1:0] ",null,null,"0x07","STATUS","-","-","-","CMPSTATE","-","-","-","CMPIF",null,"X","X"]
[]
["…"]
[]
["0x06A0","DAC0","Digital-to-Analog converter 0","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","-","-","-","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x02","DATA","[1]","[0]","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":4}," ","[9]","[8]","[7]","[6]","[5]","[4]","[3]","[2]",null,"X","X"]
[]
["…"]
[]
["0x06D8","ZCD3 ","Zero-Cross Detector 3","0x00","CTRLA","RUNSTDBY","OUTEN","-","-","INVERT","-","-","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","INTMODE[1]","INTMODE[0]",null,"X","X"]
["addr",null,null,"0x03","STATUS","-","-","-","STATE","-","-","-","CROSSIF",null,"X","X"]
[]
[]
[]
["0x0800","USART0","Universal Sync. and Async RX TX 0","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x0820","USART1","Universal Sync. and Async RX TX 1","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
[]
[]
["0x0900","TWI0","Two-Wire Interface 0","0x00","CTRLA","-","INPUTLVL","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,"X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","INPUTLVL","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,"X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1]","BUSSTATE[0]",null,"X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,"X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,"X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,"X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,"X","X"]
[]
["0x0940","SPI0","Serial Peripheral Interface 0","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X"]
["ok",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0A00","TCA0 – [ Normal Mode ]","Timer/Counter Type A - instance 0 – [ Normal Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x09","EVCTRL","EVACTB[2]","EVACTB[1]","EVACTB[0]","CNTBEI","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",null,"X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0A00","TCA0 – [ Split Mode ]","Timer/Counter Type A - instance 0 – [ Split Mode ]","0x00","CTRLA","RUNSTDBY","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0B00","TCB0","Timer/Counter Type B - instance 0","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0B10","TCB1","Timer/Counter Type B - instance 1","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0B20","TCB2","Timer/Counter Type B - instance 2","0x00","CTRLA","-","RUNSTDBY","CASCADE","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","OVF","CAPT",null,"X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[]
["0x0B80","TCD0","Timer/Counter Type D - instance 0","0x00","CTRLA","-","CLKSEL[1]","CLKSEL[0]","CNTPRES[1]","CNTPRES[0]","SYNCPRES[1]","SYNCPRES[0]","ENABLE",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","-","WGMODE[1]","WGMODE[0]",null,"X","X"]
[{"$nulls":3},"0x02","CTRLC","CMPDSEL","CMPCSEL","-","-","FIFTY","-","AUPDATE","CMPOVR",null,"X","X"]
[{"$nulls":3},"0x03","CTRLD","CMPBVAL[3]","CMPBVAL[2]","CMPBVAL[1]","CMPBVAL[0]","CMPAVAL[3]","CMPAVAL[2]","CMPAVAL[1]","CMPAVAL[0]",null,"X","X"]
[{"$nulls":3},"0x04","CTRLE","DISEOC","-","-","SCAPTUREB","SCAPTUREA","RESTART","SYNC","SYNCEOC",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","EVCTRLA","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X"]
[{"$nulls":3},"0x09","EVCTRLB","CFG[1]","CFG[0]","-","EDGE","-","ACTION","-","TRIGEI",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0A","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0B","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x0C","INTCTRL","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X"]
[{"$nulls":3},"0x0D","INTFLAGS","-","-","-","-","TRIGB","TRIGA","-","OVF",null,"X","X"]
[{"$nulls":3},"0x0E","STATUS","PWMACTB","PWMACTA","-","-","-","-","CMDRDY","ENRDY",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x10","INPUTCTRLA","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[0]",null,"X","X"]
[{"$nulls":3},"0x11","INPUTCTRLB","-","-","-","-","INPUTMODE[3]","INPUTMODE[2]","INPUTMODE[1]","INPUTMODE[3]",null,"X","X"]
[{"$nulls":3},"0x12","FAULTCTRL","CMPDEN","CMPCEN","CMPBEN","CMPAEN","CMPD","CMPC","CMPB","CMPA",null,"X","X"]
[{"$nulls":3},"0x13","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x14","DLYCTRL","-","-","DLYPRESC[1]","DLYPRESC[0]","DLYTRIG[1]","DLYTRIG[0]","DLYSEL[1]","DLYSEL[0]",null,"X","X"]
[{"$nulls":3},"0x15","DLYVAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
[{"$nulls":3},"0x16","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x18","DITCTRL","-","-","-","-","-","-","DITHERSEL[1]","DITHERSEL[0]",null,"X","X"]
[{"$nulls":3},"0x19","DITVAL","-","-","-","-","DITHER[3]","DITHER[2]","DITHER[1]","DITHER[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x1D","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1E","DBGCTRL","-","-","-","-","-","FAULTDET","-","DBGRUN",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x21","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x22","CAPTUREA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x24","CAPTUREB","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x26","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x27","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x28","CMPASET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2A","CMPACLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x2C","CMPBSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","-","-","-","-","[B]","[A]","[9]","[8]",null,"X","X"]
["ok",null,null,"0x2E","CMPBCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["…"]
[]
["0x0F00","SYSCFG","System Configuration","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
["ok",null,null,"0x01","REVID","MAJOR[3]","MAJOR[2]","MAJOR[1]","MAJOR[0]","MINOR[3]","MINOR[2]","MINOR[1]","MINOR[0]",null,"X","X"]
[]
["0x1000","NVMCTRL","Nonvolatile Memory Controller","0x00","CTRLA","-","CMD[6]","CMD[5]","CMD[4]","CMD[3]","CMD[2]","CMD[1]","CMD[0]",null,"X","X"]
[{"$nulls":3},"0x01","CTRLB","FLMAPLOCK","-","FLMAP[1]","FLMAP[0]","-","APPDATAWP","BOOTRP","APPCODEWP",null,"X","X"]
[{"$nulls":3},"0x02","STATUS","-","ERROR[2]","ERROR[1]","ERROR[0]","-","-","EEBUSY","FBUSY",null,"X","X"]
[{"$nulls":3},"0x03","INTCTRL","-","-","-","-","-","-","-","EEREADY",null,"X","X"]
[{"$nulls":3},"0x04","INTFLAGS","-","-","-","-","-","-","-","EEREADY",null,"X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x06","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"X","X"]
[{"$nulls":3},"0x08","ADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
["ok",{"$nulls":3}," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X"]
[]
["0x1040","LOCK","Lock Bits","0x00","KEY","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3}," "," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3}," "," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X"]
["ok",null,null," "," ","[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X"]
[]
["0x1050","FUSE","Configuration and User Fuses","0x00","WDTCFG","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X"]
[{"$nulls":3},"0x01","BODCFG","LVL[2]","LVL[1]","LVL[0]","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X"]
[{"$nulls":3},"0x02","OSCCFG","-","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x05","SYSCFG0","CRCSRC[1]","CRCSRC[0]","CRCSEL","-","RSTPINCFG[1]","RSTPINCFG[0]","-","EESAVE",null,"X","X"]
[{"$nulls":3},"0x06","SYSCFG1","-","-","-","-","-","SUT[2]","SUT[1]","SUT[0]",null,"X","X"]
[{"$nulls":3},"0x07","CODESIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x08","BOOTSIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["0x1080","USERROW","User Row","0x00",null,"[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":5},"[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X"]
["ok",{"$nulls":4},"[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X"]
[]
["0x1100","SIGROW","Signature Row – [ READ ONLY  ]","0x00","DEVICEID0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x01","DEVICEID1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x02","DEVICEID2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x04","TEMPSENSE0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":3},"0x06","TEMPSENSE1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X"]
[{"$nulls":14},"X","X"]
[{"$nulls":3},"0x10","SERNUM0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[{"$nulls":3},"...","…","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
["ok",null,null,"0x1F","SERNUM15","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X"]
[]
["WITHOUT ANY WARRANTY"]
[]
[]
["Features"]
[]
["• AVR® CPU"]
[]
["  – Running at up to 24 MHz"]
["  – Single-cycle I/O access"]
["  – Two-level interrupt controller"]
["  – Two-cycle hardware multiplier"]
["  – Supply voltage range: 1.8V to 5.5V"]
[]
["• Memories"]
["  – 16KB or 32 KB in-system self-programmable Flash memory"]
["  – 256B EEPROM"]
["  – 2KB or 4 KB SRAM"]
["  – 32B of user row in nonvolatile memory that can keep data during chip erase and "]
["     can be programmed while the device is locked"]
["  – Write/erase endurance"]
["     • Flash 1,000 cycles"]
["     • EEPROM 100,000 cycles"]
["  – Data retention: 40 years at 55°C"]
[]
["• System"]
["  – Power-on Reset (POR) circuit"]
["  – Brown-out Detector (BOD)"]
["  – Clock options"]
["     • High-precision internal high-frequency oscillator with selectable frequency up to 24 MHz (OSCHF)"]
["        – Auto-tuning for improved internal oscillator accuracy"]
["     • Internal PLL up to 48 MHz for high-frequency operation of Timer/Counter type D (PLL)"]
["     • 32.768 kHz ultra-low power internal oscillator (OSC32K)"]
["     • 32.768 kHz external crystal oscillator (XOSC32K)"]
["     • External clock input"]
["     • External high-frequency crystal oscillator (XOSCHF) with Clock Failure Detection"]
["  – Single-pin Unified Program and Debug Interface (UPDI)"]
["  – Three sleep modes"]
["     • Idle with all peripherals running for immediate wake-up"]
["     • Standby with a configurable operation of selected peripherals"]
["     • Power-Down with full data retention"]
["  – Automated Cyclic Redundancy Check (CRC) Flash memory scan"]
["  – Watchdog Timer (WDT) with Window mode, with a separate on-chip oscillator"]
["  – External interrupt on all general purpose pins"]
[]
["• Peripherals"]
["  – One 16-bit Timer/Counter type A (TCA) with three compare channels for PWM and waveform generation"]
["  – Three 16-bit Timer/Counter type B (TCB) with input capture and signal measurements"]
["  – One 12-bit PWM Timer/Counter type D (TCD) optimized for power control"]
["  – One 16-bit Real-Time Counter (RTC) that can run from an external crystal or internal oscillator"]
["  – Two USARTs"]
["     • Operation modes: RS-485, LIN client, host SPI, and IrDA"]
["     • Fractional baud rate generator, auto-baud, and start-of-frame detection"]
["  – One SPI with host/client operation modes"]
["  – One Two-Wire Interface (TWI) with dual address match"]
["        • Simultaneous host/client operation (Dual mode)"]
["        • Philips I2C compatible"]
["        • Standard mode (Sm, 100 kHz)"]
["        • Fast mode (Fm, 400 kHz)"]
["        • Fast mode Plus (Fm+, 1 MHz) (1)"]
["  – Event System for CPU independent and predictable inter-peripheral signaling"]
["  – Configurable Custom Logic (CCL) with four programmable Look-up Tables (LUTs)"]
["  – One 12-bit differential 130 ksps Analog-to-Digital Converter (ADC)"]
["  – One 10-bit Digital-to-Analog Converter (DAC)"]
["  – One Analog Comparator (AC)"]
["  – One Zero-Cross Detector (ZCD)"]
["  – Internal 1.024V, 2.048V, 2.500V and 4.096V voltage references, and external reference option (VREF)"]
[]
["• I/O and Packages:"]
["  – Multi-Voltage I/O (MVIO) on I/O port C"]
["  – Selectable input voltage threshold"]
["  – Up to 27/26 programmable I/O pins"]
["  – 32-pin VQFN 5x5 mm and TQFP 7x7 mm"]
["  – 28-pin SPDIP, SSOP, SOIC and VQFN"]
[]
["• Temperature Ranges:"]
["  – Industrial: -40°C to +85°C"]
["  – Extended: -40°C to +125°C"]
[]
["  Note: "]
["  1. I2C Fm+ is only supported for 2.7V and above."]

{"sheet":"AVR4808|4809-28-32-40-48","index":4,"n_rows":772,"n_cols":31,"rows_kept":772,"flags":["formulas_cached_only"]}
["AVR4808|4809-28-32-40-48  [ 04-2023 ] "]
["Peripherals and Architecture"]
[]
[]
["Table 8-1. Peripheral Address Map",{"$nulls":20},"Table","8-3. Interrupt Vector Mapping"]
[{"$nulls":21},"***************************************************************************************************************************************************************************"]
["Base Address","Name","Description","Offset","Name","Bit 7","Bit 6"," Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0",null,"28-Pin","32-Pin","40-Pin","48-Pin",{"$nulls":3},"Vector","Program",{"$nulls":3},"28-Pin","32-Pin","48-Pin","64-Pin"]
[{"$nulls":21},"Number","Address","Peripheral","Description"]
["0x0000","VPORTA","Virtual Port A","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},0,"0x00","RESET","Reset",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},1,"0x02","NMI","Non-Maskable Interrupt available for CRCSCAN",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},2,"0x04","BOD_VLM","Voltage Level Monitor Interrupt",null,"X","X","X","X"]
[{"$nulls":21},3,"0x06","RTC_CNT","Configurable Custom Logic Interrupt",null,"X","X","X","X"]
["0x0004","VPORTB","Virtual Port B","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," "," ","X",{"$nulls":3},4,"0x08","RTC_PIT","PORTA External interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ",null,"X",{"$nulls":3},5,"0x0A","CCL_CCL","Normal: Timer/Counter Type A Overflow Interrupt ",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ",null,"X",{"$nulls":3},6,"0x0C","PORTA_PORT","Split: Timer/Counter Type A Low Underflow Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ",null,"X",{"$nulls":3},7,"0x0E","TCA0","Normal: Unused",null,"X","X","X","X"]
[{"$nulls":21},7,"0x0E","TCA0_LUNF","Split: Timer/Counter Type A High Underflow Interrupt",null,"X","X","X","X"]
["0x0008","VPORTC","Virtual Port C","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},8,"0x10","TCA0_HUNF","Normal: Unused",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},8,"0x10","TCA0_HUNF","Split: Timer/Counter Type A High Underflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},9,"0x12","TCA0_CMP0","Normal: Timer/Counter Type A Compare 0 Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},9,"0x12","TCA0_LCMP0","Split: Timer/Counter Type A Low Compare 0 Interrupt",null,"X","X","X","X"]
[{"$nulls":21},10,"0x14","TCA0_CMP1","Normal: Timer/Counter Type A Compare 1 Interrupt",null,"X","X","X","X"]
["0x000C","VPORTD","Virtual Port D","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},10,"0x14","TCA0_LCMP1","Split: Timer/Counter Type A Low Compare 1 Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},11,"0x16","TCA0_CMP2","Normal: Timer/Counter Type A Compare 2 Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},11,"0x16","TCA0_LCMP2","Split: Timer/Counter Type A Low Compare 2 Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},12,"0x18","TCB0_INT","Timer Counter Type B0 Capture/Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":21},13,"0x1A","TCB1_INT","Timer Counter Type B1 Capture/Overflow Interrupt",null,"X","X","X","X"]
["0x0010","VPORTE","Virtual Port E","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},14,"0x1C","TWI0_TWIS","Two-Wire Interface Client Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},15,"0x1E","TWI0_TWIM","Two-Wire Interface Host Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},16,"0x20","SPI0_INT","Serial Peripheral Interface Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null," "," ","X","X",{"$nulls":3},17,"0x22","USART0_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":21},18,"0x24","USART0_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
["0x0014 ","VPORTF","Virtual Port F","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},19,"0x26","USART0_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},20,"0x28","PORTD_PORT","PORTD External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},21,"0x2A","AC0_AC","Analog Comparator Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},22,"0x2C","ADC0_RESRDY","Analog-to-Digital Converter Result Ready Interrupt",null,"X","X","X","X"]
[{"$nulls":21},23,"0x2E","ADC0_WCMP","Analog-to-Digital Converter Window Compare Interrupt",null,"X","X","X","X"]
["0x001C","GPR","General Purpose Registers","0x00","GPIOR0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},24,"0x30","PORTC_PORT","PORTC External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x01","GPIOR1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},25,"0x32","TCB2_INT","Timer Counter Type B2 Capture/Overflow Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x02","GPIOR2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},26,"0x34","USART1_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
["ok",null,null,"0x03","GPR3IO","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},27,"0x36","USART1_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":21},28,"0x38","USART1_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
["0x0030","CPU","CPU","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},29,"0x3A","PORTF_PORT","PORTF External Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},30,"0x3C","NVMCTRL_EE","Nonvolatile Memory Controller EEPROM Ready Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},31,"0x3E","USART2_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},32,"0x40","USART2_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CCP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},33,"0x42","USART2_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},34,"0x44","PORTB_PORT","PORTB External Interrupt",null,"-","-","-","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},35,"0x46","PORTE_PORT","PORTE External Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},36,"0x48","TCB3_INT","Timer Counter Type B Capture/Overflow Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X",{"$nulls":3},37,"0x4A","USART3_RXC","Universal Synchronous Asynchronous Receiver and Transmitter Receive Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":14},"X","X","X","X",{"$nulls":3},38,"0x4C","USART3_DRE","Universal Synchronous Asynchronous Receiver and Transmitter Data Register Empty Interrupt",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","SP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X",{"$nulls":3},39,"0x4E","USART3_TXC","Universal Synchronous Asynchronous Receiver and Transmitter Transmit Complete Interrupt",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["reduced -RAMPZ",null,null,"0x0F","SREG","I","T","H","S","V","N","Z","C",null,"X","X","X","X",{"$nulls":4},"reduced"]
[{"$nulls":22},"modified"]
["0x0040","RSTCTRL","Reset Controller","0x00","RSTFR","-","-","UPDIRF","SWRF","WDRF","EXTRF","BORF","PORF"]
["mod name SWRST → SWRE",null,null,"0x01","SWRR","-","-","-","-","-","-","-","SWRE"]
[]
["0x0050","SLPCTRL","Sleep Controller","0x00","CTRLA","-","-","-","-","SMODE[2]","SMODE[1]","SMODE[0]","SEN",null,"X","X","X","X"]
["reduced -VREGCTRL"]
[{"$nulls":14},"X","X","X","X"]
["0x0060","CLKCTRL","Clock Controller ","0x00","MCLKCTRLA","CLKOUT","-","-","-","-","-","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","MCLKCTRLB","-","-","-","PDIV[3]","PDIV[2]","PDIV[1]","PDIV[0]","PEN",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MCLKLOCK","-","-","-","-","-","-","-","LOCKEN",null,"X","X","X","X"]
[{"$nulls":3},"0x03","MCLKSTATUS","EXTS"," XOSC32KS"," OSC32KS","OSC20MS","-","-","-","SOSC",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","OSC20MCTRLA","-","-","-","-","-","-","RUNSTDBY","-",null,"X","X","X","X"]
[{"$nulls":3},"0x11","OSC20MCALIBA","-","CAL20M[6]","CAL20M[5]","CAL20M[4]","CAL20M[3]","CAL20M[2]","CAL20M[1]","CAL20M[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","OSC20MCALIBB","LOCK","-","-","-","TEMPCAL20M[3]","TEMPCAL20M[2]","TEMPCAL20M[1]","TEMPCAL20M[0]",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x13","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"…","Reserved"]
[{"$nulls":3},"0x17","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x18","OSC32KCTRLA","-","-","-","-","-","-","RUNSTDBY","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x19","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["added     OSC20MCTRLA OSC20MCALIBA OSC20MCALIBB ",null,null,"0x1B","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["Reduced CLKSEL[3:2] -OSCHFCTRLA -OSCHFTUNE -PLLCTRLA",{"$nulls":13},"X","X","X","X"]
["Modified  MCLKSTATUS, XOSC32KCTRLA ",null,null,"0x1C","XOSC32KCTRLA","-","-","CSUT[1]","CSUT[0]","-","SEL","RUNSTDBY","ENABLE",null,"X","X","X","X"]
[]
["0x0080","BOD","Brown-out Detector","0x00","CTRLA","-","-","-","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","LVL[2]","LVL[1]","LVL[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","VLMCTRLA","-","-","-","-","-","-","VLMLVL[1]","VLMLVL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTCTRL","-","-","-","-","-","VLMCFG[1]","VLMCFG[0]","VLMIE",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTFLAGS","-","-","-","-","-","-","-","VLMIF",null,"X","X","X","X"]
["ok",null,null,"0x0B","STATUS","-","-","-","-","-","-","-","VLMS",null,"X","X","X","X",{"$nulls":12},"X"]
[]
["0x00A0","VREF","Voltage Reference","0x00","CTRLA","-","ADC0REFSEL[2]","ADC0REFSEL[1]","ADC0REFSEL[0]","AC0REFSEL[2]","-","AC0REFSEL[1]","AC0REFSEL[0]",null,"X","X","X","X"]
["different",null,null,"0x01","CTRLB","-","-","-","-","-","-","ADC0REFEN","AC0REFEN",null,"X","X","X","X"]
[]
["0x0100","WDT","Watchdog Timer","0x00","CTRLA","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X","X","X"]
["ok",null,null,"0x01","STATUS","LOCK","-","-","-","-","-","-","SYNCBUSY",null,"X","X","X","X"]
[]
["0x0110","CPUINT","Interrupt Controller","0x00","CTRLA","-","IVSEL","CVT","-","-","-","-","LVL0RR",null,"X","X","X","X"]
[{"$nulls":3},"0x01","STATUS","NMIEX","-","-","-","-","-","LVL1EX","LVL0EX",null,"X","X","X","X"]
[{"$nulls":3},"0x02","LVL0PRI","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x03","LVL1VEC","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0120","CRCSCAN","Cyclic Redundancy Check Memory Scan","0x00","CTRLA","RESET","-","-","-","-","-","NMIEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","MODE[1]","MODE[0]","-","-","SRC[1:0]","SRC[1:0]",null,"X","X","X","X"]
["Added MODE[1], MODE[1]",null,null,"0x02","STATUS","-","-","-","-","-","-","OK","BUSY",null,"X","X","X","X"]
[]
["0x0140","RTC","Real-Time Counter","0x00","CTRLA","RUNSTDBY","PRESCALER[3]","PRESCALER[2]","PRESCALER[1]","PRESCALER[0]","CORREN","-","RTCEN",null,"X","X","X","X"]
[{"$nulls":3},"0x01","STATUS","-","-","-","-","CMPBUSY","PERBUSY","CNTBUSY","CTRLABUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","-","-","-","-","-","-","CMP","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","-","-","-","-","-","-","CMP","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CALIB","SIGN","ERROR[6]","ERROR[5]","ERROR[4]","ERROR[3]","ERROR[2]","ERROR[1]","ERROR[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CLKSEL","-","-","-","-","-","-","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PER]","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","PITCTRLA","-","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]","-","-","PITEN",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PITSTATUS","-","-","-","-","-","-","-","CTRLBUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PITINTCTRL","-","-","-","-","-","-","-","PI",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PITINTFLAGS","-","-","-","-","-","-","-","PI",null,"X","X","X","X"]
[{"$nulls":3},"0x14","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ok",null,null,"0x15","PITDBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[]
["…"]
[]
["0x180","EVSYS","Event System","0x00","STROBEx","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
[{"$nulls":3},"0x01","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","CHANNEL0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","CHANNEL1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","CHANNEL2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","CHANNEL3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","CHANNEL4","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","CHANNEL5","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","CHANNEL6","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x17","CHANNEL7","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x1A","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
["removed   CHANNEL 8,9, SWEVENTA,B",null,null,"0x20","USER0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["renamed  STROBEx, USERCCLLUT0A",null,null,"..."," …",{"$nulls":9},"X","X","X","X"]
["modified   addr",null,null,"0x37","USERT23","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["…"]
[]
["0x01C0","CCL","Configurable Custom Logic","0x00","CTRLA","-","RUNSTDBY","-","-","-","-","-","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","SEQCTRL0","-","-","-","-","SEQSEL0[3]","SEQSEL0[2]","SEQSEL0[1]","SEQSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","SEQCTRL1","-","-","-","-","SEQSEL1[3]","SEQSEL1[2]","SEQSEL1[1]","SEQSEL1[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL0","INTMODE3[1]","INTMODE3[0]","INTMODE2[1]","INTMODE2[0]","INTMODE1[1]","INTMODE1[0]","INTMODE0[1]","INTMODE0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x07","INTFLAGS","-","-","INT5","INT4","INT3","INT2","INT1","INT0",null,"X","X","X","X"]
[{"$nulls":3},"0x08","LUT0CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x09","LUT0CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","LUT0CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","TRUTH0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","LUT1CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","LUT1CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL0[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","LUT1CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TRUTH1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x10","LUT2CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x11","LUT2CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","LUT2CTRLC","-","-","-","-","INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","TRUTH2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","LUT3CTRLA","EDGEDET","OUTEN","FILTSEL[1]","FILTSEL[0]","CLKSRC[2]","CLKSRC[1]","CLKSRC[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x15","LUT3CTRLB","INSEL1[3]","INSEL1[2]","INSEL1[1]","INSEL1[0]","INSEL0[3]","INSEL0[2]","INSEL0[1]","INSEL0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","LUT3CTRLC",{"$nulls":4},"INSEL2[3]","INSEL2[2]","INSEL2[1]","INSEL2[0]",null,"X","X","X","X"]
["removed SEQCTRL2, INTCTRL1, LUT4..",null,null,"0x17","TRUTH3","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["…"]
[]
["0x0400","PORTA","Port A Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ok",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0420","PORTB","Port B Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"-","-","-","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"-","-","-","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","-","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
["ok",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","-","X"]
[]
["0x0440","PORTC","Port C Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ok",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0460","PORTD","Port D Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ok",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["0x0480","PORTE","Port E Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
["ok",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"-","-","X","X"]
[]
["0x04A0","PORTF","Port F Configuration","0x00","DIR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DIRSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DIRCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","DIRTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","OUT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","OUTSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","OUTCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","OUTTGL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","IN","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","INTFLAGS","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","PORTCTRL","-","-","-","-","-","-","-","SRL",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","PINCONFIG","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","PINCTRLUPD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","PINCTRLSET","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","PINCTRLCLR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","PIN0CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x11","PIN1CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","PIN2CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x13","PIN3CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","PIN4CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x15","PIN5CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x16","PIN6CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
["ok",null,null,"0x17","PIN7CTRL","INVEN","-","-","-","PULLUPEN","ISC[2]","ISC[1]","ISC[0]",null,"X","X","X","X"]
[]
["…"]
[]
["0x05E0","PORTMUX","Port Multiplexer","0x00","EVSYSROUTEA","-","-","EVOUTF","EVOUTE","EVOUTD","EVOUTC","EVOUTB","EVOUTA",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CCLROUTEA","-","-","-","-","LUT3","LUT2","LUT1","LUT0",null,"X","X","X","X"]
[{"$nulls":3},"0x02","USARTROUTEA","USART3[1]","USART3[0]","USART2[1]","USART2[0]","USART1[1]","USART1[0]","USART0[1]","USART0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TWISPIROUTEA","-","-","TWI0[1]","TWI0[0]","-","-","SPI0[1]","SPI0[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TCAROUTEA","-","-","-","-","-","TCA0[2]","TCA0[1]","TCA0[0]",null,"X","X","X","X"]
["reduced ",null,null,"0x05","TCBROUTEA","-","-","-","-","TCB3","TCB2","TCB1","TCB0",null,"X","X","X","X"]
[]
["0x0600","ADC0","Analog to-Digital Converter 0","0x00","CTRLA","RUNSTDBY","-","-","-","-","RESSEL[0]","FREERUN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","-","-","-","-","SAMPNUM[2]","SAMPNUM[1]","SAMPNUM[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","SAMPCAP","REFSEL[1]","REFSEL[0]","-","PRESC[2]","PRESC[1]","PRESC[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","INITDLY[2]","INITDLY[1]","INITDLY[0]","ASDV","SAMPDLY[3]","SAMPDLY[2]","SAMPDLY[1]","SAMPDLY[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLE","-","-","-","-","-","WINCM[2]","WINCM[1]","WINCM[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","SAMPCTRL","-","-","-","SAMPLEN[4]","SAMPLEN[3]","SAMPLEN[2]","SAMPLEN[1]","SAMPLEN[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","MUXPOS",null,null,"-","MUXPOS[4]","MUXPOS[3]","MUXPOS[2]","MUXPOS[1]","MUXPOS[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","COMMAND","-","-","-","-","-","-","-","STCONV",null,"X","X","X","X"]
[{"$nulls":3},"0x09","EVCTRL","-","-","-","-","-","-","-","STARTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","-","-","-","-","-","WCMP","RESRDY",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x10","RES","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x12","WINLT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x14","WINHT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["modified"," ",null,"0x16","CALIB","-","-","-","-","-","-","-","DUTYCYC",null,"X","X","X","X"]
[]
["…"]
[]
["0x0680","AC0","Analog Comparator 0","0x00","CTRLA","RUNSTDBY","OUTEN","INTMODE[1]","INTMODE[0]","LPMODE","HYSMODE[1]","HYSMODE[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RESERVED","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x02","MUXCTRL","INVERT","-","-","MUXPOS[1]","MUXPOS[0]","-","MUXNEG[1]","MUXNEG[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","DACREF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","RESERVED","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTCTRL","-","-","-","-","-","-","-","CMP",null,"X","X","X","X"]
["modified"," ",null,"0x07","STATUS","-","-","-","STATE","-","-","-","CMP",null,"X","X","X","X"]
[]
["…"]
[]
["0x0800","USART0","Universal Sync. and Async RX TX 0","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","RS485[1]","RS485[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0820","USART1","Universal Sync. and Async RX TX 1","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0840","USART2","Universal Sync. and Async RX TX 2","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"X","X","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x0860","USART3","Universal Sync. and Async RX TX 3","0x00","RXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x01","RXDATAH","RXCIF","BUFOVF","-","-","-","FERR","PERR","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","TXDATAL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x03","TXDATAH","-","-","-","-","-","-","-","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x04","STATUS","RXCIF","TXCIF","DREIF","RXSIF","ISFIF","-","BDF","WFB",null,"-","-","X","X"]
[{"$nulls":3},"0x05","CTRLA","RXCIE","TXCIE","DREIE","RXSIE","LBME","ABEIE","-","RS485",null,"-","-","X","X"]
[{"$nulls":3},"0x06","CTRLB","RXEN","TXEN","-","SFDEN","ODME","RXMODE[1]","RXMODE[0]","MPCM",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","PMODE[1]","PMODE[0]","SBMODE","CHSIZE[2]","CHSIZE[1]","CHSIZE[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x07","CTRLC","CMODE[1]","CMODE[0]","-","-","-","UDORD","UCPHA","-",null,"-","-","X","X"]
[{"$nulls":3},"0x08","BAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","CTRLD","ABW[1]","ABW[0]","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x0B","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","EVCTRL","-","-","-","-","-","-","-","IREI",null,"-","-","X","X"]
[{"$nulls":3},"0x0D","TXPLCTRL","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["ok",null,null,"0x0E","RXPLCTRL","-","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[]
["0x08A0","TWI1","Two-Wire Interface 1","0x00","CTRLA","-","-","-","SDASETUP","SDAHOLD[1]","SDAHOLD[0]","FMPEN","-",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DUALCTRL","-","-","-","-","SDAHOLD[1]","SDAHOLD[0]","FMPEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x03","MCTRLA","RIEN","WIEN","-","QCEN","TIMEOUT[1]","TIMEOUT[0]","SMEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x04","MCTRLB","-","-","-","-","FLUSH","ACKACT","MCMD[1]","MCMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","MSTATUS","RIF","WIF","CLKHOLD","RXACK","ARBLOST","BUSERR","BUSSTATE[1]","BUSSTATE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","MBAUD","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","MADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","MDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x09","SCTRLA","DIEN","APIEN","PIEN","-","-","PMEN","SMEN","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","SCTRLB","-","-","-","-","-","ACKACT","SCMD[1]","SCMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","SSTATUS","DIF","APIF","CLKHOLD","RXACK","COLL","BUSERR","DIR","AP",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","SADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","SDATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["mod addr,-INPUTVL",null,null,"0x0E","SADDRMASK","[6]","[5]","[4]","[3]","[2]","[1]","[0]","ADDREN",null,"X","X","X","X"]
[]
["…"]
[]
["0x0940","SPI0","Serial Peripheral Interface 0","0x00","CTRLA","-","DORD","MASTER","CLK2X","-","PRESC[1:0]","PRESC[1]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","BUFEN","BUFWR","-","-","-","SSD","MODE[1]","MODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","INTCTRL","RXCIE","TXCIE","DREIE","SSIE","-","-","-","IE",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","IF","WRCOL","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTFLAGS","RXCIF","TXCIF","DREIF","SSIF","-","-","-","BUFOVF",null,"X","X","X","X"]
["ok",null,null,"0x04","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["…"]
[]
["0x0A00","TCA0 – [ Normal Mode ]","Timer/Counter Type A - instance 0 – [ Normal Mode ]","0x00","CTRLA","-","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","CMP2EN","CMP1EN","CMP0EN","ALUPD","WGMODE[2]","WGMODE[1]","WGMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","-","-","-","-","CMP2OV","CMP1OV","CMP0OV",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","LUPD","DIR",null,"X","X","X","X"]
[{"$nulls":3},"0x06","CTRLFCLR","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CTRLFSET","-","-","-","-","CMP2BV","CMP1BV","CMP0BV","PERBV",null,"X","X","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x09","EVCTRL","-","-","-","-","EVACTA[2]","EVACTA[1]","EVACTA[0]","CNTAEI",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","CMP2","CMP1","CMP0","-","-","-","OVF",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","PER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x28","CMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","CMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","CMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x2E","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x35","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x36","PERBUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x38","CMP0BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x3A","CMP1BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x3C","CMP2BUF","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["mod -RUNSTDBY,-CMP2EN,-CMP1EN,-CMP0EN,- ALUPD",{"$nulls":4},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0A00","TCA0 – [ Split Mode ]","Timer/Counter Type A - instance 0 – [ Split Mode ]","0x00","CTRLA","-","-","-","-","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","HCMP2EN","HCMP1EN","HCMP0EN","-","LCMP2EN","LCMP1EN","LCMP0EN",null,"X","X","X","X"]
[{"$nulls":3},"0x02","CTRLC","-","HCMP2OV","HCMP1OV","HCMP0OV","-","LCMP2OV","LCMP1OV","LCMP0OV",null,"X","X","X","X"]
[{"$nulls":3},"0x03","CTRLD","-","-","-","-","-","-","-","SPLITM",null,"X","X","X","X"]
[{"$nulls":3},"0x04","CTRLECLR","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x05","CTRLESET","-","-","-","-","CMD[1]","CMD[0]","CMDEN[1]","CMDEN[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x06","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x09","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0A","INTCTRL","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X","X","X"]
[{"$nulls":3},"0x0B","INTFLAGS","-","LCMP2","LCMP1","LCMP0","-","-","HUNF","LUNF",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0C","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0D","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0E","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x1F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x20","LCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x21","HCNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x22","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x25","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x26","LPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x27","HPER","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x28","LCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x29","HCMP0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2A","LCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2B","HCMP1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x2C","LCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["mod -RUNSTDBY",null,null,"0x2D","HCMP2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["…"]
[]
["0x0B00","TCB0","Timer/Counter Type B - instance 0","0x00","CTRLA","-","RUNSTDBY","-","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","-","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","-","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["mod addr,-CASCADE,-OVF",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0A90","TCB1","Timer/Counter Type B - instance 1","0x00","CTRLA","-","RUNSTDBY","-","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","-","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","-","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["mod addr,-CASCADE,-OVF",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0AA0","TCB2","Timer/Counter Type B - instance 2","0x00","CTRLA","-","RUNSTDBY","-","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"X","X","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","-","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","-","CAPT",null,"X","X","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"X","X","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"X","X","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["mod addr,-CASCADE,-OVF",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[]
["0x0AB0","TCB3","Timer/Counter Type B - instance 3","0x00","CTRLA","-","RUNSTDBY","-","SYNCUPD","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]","ENABLE",null,"-","-","X","X"]
[{"$nulls":3},"0x01","CTRLB","-","ASYNC","CCMPINIT","CCMPEN","-","CNTMODE[2]","CNTMODE[1]","CNTMODE[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x02","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"-","-","X","X"]
[{"$nulls":3},"0x04","EVCTRL","-","FILTER","-","EDGE","-","-","-","CAPTEI",null,"-","-","X","X"]
[{"$nulls":3},"0x05","INTCTRL","-","-","-","-","-","-","-","CAPT",null,"-","-","X","X"]
[{"$nulls":3},"0x06","INTFLAGS","-","-","-","-","-","-","-","CAPT",null,"-","-","X","X"]
[{"$nulls":3},"0x07","STATUS","-","-","-","-","-","-","-","RUN",null,"-","-","X","X"]
[{"$nulls":3},"0x08","DBGCTRL","-","-","-","-","-","-","-","DBGRUN",null,"-","-","X","X"]
[{"$nulls":3},"0x09","TEMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":3},"0x0A","CNT","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[{"$nulls":3},"0x0C","CCMP","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"-","-","X","X"]
["mod addr,-CASCADE,-OVF",{"$nulls":3}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"-","-","X","X"]
[]
["…"]
[]
["0x0F00","SYSCFG","System Configuration","0x00","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
["ok",null,null,"0x01","REVID","MAJOR[3]","MAJOR[2]","MAJOR[1]","MAJOR[0]","MINOR[3]","MINOR[2]","MINOR[1]","MINOR[0]",null,"X","X","X","X"]
[]
["0x1000","NVMCTRL","Nonvolatile Memory Controller","0x00","CTRLA","-","CMD[6]","CMD[5]","CMD[4]","CMD[3]","CMD[2]","CMD[1]","CMD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","CTRLB","FLMAPLOCK","-","FLMAP[1]","FLMAP[0]","-","APPDATAWP","BOOTRP","APPCODEWP",null,"X","X","X","X"]
[{"$nulls":3},"0x02","STATUS","-","ERROR[2]","ERROR[1]","ERROR[0]","-","-","EEBUSY","FBUSY",null,"X","X","X","X"]
[{"$nulls":3},"0x03","INTCTRL","-","-","-","-","-","-","-","EEREADY",null,"X","X","X","X"]
[{"$nulls":3},"0x04","INTFLAGS","-","-","-","-","-","-","-","EEREADY",null,"X","X","X","X"]
[{"$nulls":3},"0x05","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x06","DATA","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[8]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x08","ADDR","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":4}," ","[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
["ok",{"$nulls":3}," ","[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
[]
["…"]
[]
["0x1100","SIGROW","Signature Row  – [ READ ONLY  ]","0x00","DEVICEID0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","DEVICEID1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","DEVICEID2","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","TEMPSENSE0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":3},"0x06","TEMPSENSE1","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x08","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"...","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x0F","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x10","SERNUM0","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":3},"...","…","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x1F","SERNUM15","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x1280","FUSE","Configuration and User Fuses","0x00","WDTCFG","WINDOW[3]","WINDOW[2]","WINDOW[1]","WINDOW[0]","PERIOD[3]","PERIOD[2]","PERIOD[1]","PERIOD[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x01","BODCFG","LVL[2]","LVL[1]","LVL[0]","SAMPFREQ","ACTIVE[1]","ACTIVE[0]","SLEEP[1]","SLEEP[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x02","OSCCFG","-","-","-","-","CLKSEL[3]","CLKSEL[2]","CLKSEL[1]","CLKSEL[0]",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x03","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":3},"0x04","Reserved","-","-","-","-","-","-","-","-",null,"X","X","X","X"]
[{"$nulls":14},"X","X","X","X"]
[{"$nulls":3},"0x05","SYSCFG0","CRCSRC[1]","CRCSRC[0]","CRCSEL","-","RSTPINCFG[1]","RSTPINCFG[0]","-","EESAVE",null,"X","X","X","X"]
[{"$nulls":3},"0x06","SYSCFG1","-","-","-","-","-","SUT[2]","SUT[1]","SUT[0]",null,"X","X","X","X"]
[{"$nulls":3},"0x07","CODESIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
["ok",null,null,"0x08","BOOTSIZE","[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[]
["0x1300","USERROW","User Row","0x00",null,"[7]","[6]","[5]","[4]","[3]","[2]","[1]","[0]",null,"X","X","X","X"]
[{"$nulls":5},"[F]","[E]","[D]","[C]","[B]","[A]","[9]","[8]",null,"X","X","X","X"]
[{"$nulls":5},"[17]","[16]","[15]","[14]","[13]","[12]","[11]","[10]",null,"X","X","X","X"]
["ok",{"$nulls":4},"[1F]","[1E]","[1D]","[1C]","[1B]","[1A]","[19]","[18]",null,"X","X","X","X"]
[]
["WITHOUT ANY WARRANTY"]
[]
[]
[]
["Features"]
[]
["• AVR® CPU"]
["  – Single-cycle I/O access"]
["  – Two-level interrupt controller"]
["  – Two-cycle hardware multiplier"]
[]
["• Memories"]
["  – 48 KB In-System self-programmable Flash memory"]
["  – 256B EEPROM"]
["  – 6 KB SRAM"]
["  – Write/erase endurance"]
["     • Flash 10,000 cycles"]
["     • EEPROM 100,000 cycles"]
["  – Data retention: 40 years at 55°C"]
[]
["• System"]
["  – Power-on Reset (POR) circuit"]
["  – Brown-out Detector (BOD)"]
["  – Clock options"]
["     • 16/20 MHz low-power internal oscillator"]
["     • 32.768 kHz Ultra-Low Power internal oscillator (OSC32K)"]
["     • 32.768 kHz external crystal oscillator"]
["     • External clock input"]
["  – Single-pin Unified Program and Debug Interface (UPDI)"]
["  – Three sleep modes"]
["     • Idle with all peripherals running for immediate wake-up"]
["     • Standby "]
["      – Configurable operation of selected peripherals"]
["      – SleepWalking peripherals"]
["     • Power-Down with limited wake-up functionality"]
[]
["  • Peripherals"]
["    – Up to two 16-bit Timer/Counter type A (TCA) with a dedicated period register and three PWM channels"]
["    – Up to four 16-bit Timer/Counter type B (TCB) with input capture"]
["    – One 16-bit Real-Time Counter (RTC) running from an external crystal or internal oscillator"]
["    – Up to four USART with fractional baud rate generator, auto-baud, and start-of-frame detection"]
["    – One host/client Serial Peripheral Interface (SPI)"]
["    – One Two-Wire Interface (TWI) with dual address match"]
["       • Can operate simultaneously as host and client"]
["       • Standard mode (Sm, 100 kHz)"]
["       • Fast mode (Fm, 400 kHz)"]
["       • Fast mode plus (Fm+, 1 MHz) (1)"]
["  – Event System for core independent and predictable inter-peripheral signaling"]
["  – Configurable Custom Logic (CCL) with up to four programmable Look-up Tables (LUT)"]
["  – One Analog Comparator (AC) with a scalable reference input"]
["  – One 10-bit 150 ksps Analog-to-Digital Converter (ADC)"]
["  – Up to three Zero-Cross Detectors (ZCD)"]
["  – Five selectable internal voltage references: 0.55V, 1.1V, 1.5V, 2.5V, and 4.3V"]
["  – CRC code memory scan hardware"]
["     • Optional automatic CRC scan before code execution is allowed"]
["  – Watchdog Timer (WDT) with Window mode, with a separate on-chip oscillator"]
["  – External interrupt on all general purpose pins"]
[]
["• I/O and Packages:"]
["  – Up to 41 programmable I/O pins"]
["  – 28-pin SSOP"]
["  – 32-pin VQFN 5x5 mm and TQFP 7x7 mm"]
["  – 48-pin PDIP"]
["  – 48-pin VQFN 6x6 mm and TQFP 7x7 mm"]
[]
["• Temperature Ranges:"]
["  – Industrial: -40°C to +85°C"]
["  – Extended: -40°C to +125°C"]
[]
["• Speed Grades -40°C to +105°C:"]
["  – 0-5 MHz @ 1.8V – 5.5V"]
["  – 0-10 MHz @ 2.7V – 5.5V"]
["  – 0-20 MHz @ 4.5V – 5.5V"]
["• Speed Grades +105°C to +125°C:"]
["  – 0-8 MHz @ 2.7V - 5.5V"]
["  – 0-16 MHz @ 4.5V – 5.5V"]
["• Speed Grades -40°C to +125°C - Automotive Range Parts (-VAO):"]
["  – 0-8 MHz @ 2.7V - 5.5V"]
["  – 0-16 MHz @ 4.5V - 5.5V"]
["• VAO variants available: "]
["  – Designed, manufactured, tested, and qualified per the AEC-Q100 requirements for automotive applications. "]