<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_LED_TS5_9.2MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED - PTH&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/TSD1265.png"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_LED_PB06_15MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED - PTH&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/TSD1265.png"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="SWITCH-MOMENTARY-TS5-LED">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;</description>
<pin name="NO@3"/>
<pin name="NO@4"/>
<pin name="A_LED+" direction="pas"/>
<pin name="C_LED-" direction="pas"/>
<pin name="SW@2"/>
<pin name="SW@1"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-PB06-RGBLED">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;</description>
<pin name="SW@2"/>
<pin name="SW@1"/>
<pin name="BLUE1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="GREEN2-" direction="pas"/>
<pin name="RED2-" direction="pas"/>
<pin name="RED1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="GREEN1-" direction="pas"/>
<pin name="BLUE2-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MOMENTARY-SWITCH-TS5-LED" prefix="S">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-CHERRY - Cherry MX Switch&lt;/h5&gt;
&lt;p&gt;Cherry MX Keyswitches are top-of-the-line mechanical keyboard switches. They’re satisfyingly “clicky”, reliable up to tens-of-millions of key presses, and a standard in gaming and programming keyboards across the globe. This ‘blue’ version Cherry MX Switch is favored by most due to its secondary internal actuator making it less likely to “double-tap.” If you are looking for a noticeably audible and high-quality key switch, this is the perfect option for you!&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13834"&gt;Cherry MX Switch&lt;/a&gt; (COM-13834)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13773"&gt;Cherry MX Switch Breakout&lt;/a&gt; (BOB-13773)&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;PTH-12MM and PTH-12MM-KIT - 12mm Illuminated LED&lt;/h5&gt;
&lt;p&gt;KIT variant is for soldering kits. There is no tStop (covering up the top side of the pads with mask). This helps the beginner see which side they should be soldering too.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10467"&gt;LED Tactile Button Breakout&lt;/a&gt; (BOB-10467)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10442"&gt;LED Tactile Button - Red&lt;/a&gt; (COM-10442)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10443"&gt;LED Tactile Button - Blue&lt;/a&gt; (COM-10443)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10440"&gt;LED Tactile Button - Green&lt;/a&gt; (COM-10440)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10441"&gt;LED Tactile Button - Orange&lt;/a&gt; (COM-10441)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10439"&gt;LED Tactile Button - White&lt;/a&gt; (COM-10439)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-TS5-LED"/>
</gates>
<devices>
<device name="" package="TACTILE_SWITCH_LED_TS5_9.2MM">
<connects>
<connect gate="G$1" pin="A_LED+" pad="LED+"/>
<connect gate="G$1" pin="C_LED-" pad="LED-"/>
<connect gate="G$1" pin="NO@3" pad="K2@3"/>
<connect gate="G$1" pin="NO@4" pad="K2@4"/>
<connect gate="G$1" pin="SW@1" pad="K1@1"/>
<connect gate="G$1" pin="SW@2" pad="K1@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOMENTARY-SWITCH-PB06-LED">
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-PB06-RGBLED"/>
</gates>
<devices>
<device name="RGB" package="TACTILE_SWITCH_LED_PB06_15MM">
<connects>
<connect gate="G$1" pin="BLUE1-" pad="B1-"/>
<connect gate="G$1" pin="BLUE2-" pad="B2-"/>
<connect gate="G$1" pin="C1+" pad="C1+"/>
<connect gate="G$1" pin="C2+" pad="C2+"/>
<connect gate="G$1" pin="GREEN1-" pad="G1-"/>
<connect gate="G$1" pin="GREEN2-" pad="G2-"/>
<connect gate="G$1" pin="RED1-" pad="R1-"/>
<connect gate="G$1" pin="RED2-" pad="R2-"/>
<connect gate="G$1" pin="SW@1" pad="SW@1"/>
<connect gate="G$1" pin="SW@2" pad="SW@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
