(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Analog_Switch:CD4051B" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -10.16 16.51 0))
      (property "Value" "CD4051B" (at 3.81 16.51 0))
      (property "Footprint" "" (at 3.81 -19.05 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4052b.pdf" (at -0.508 2.54 0))
      (property "ki_keywords" "analog switch selector multiplexer" (at 0 0 0))
      (property "ki_description" "CMOS single 8-channel analog multiplexer demultiplexer, TSSOP-16/DIP-16/SOIC-16" (at 0 0 0))
      (property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* DIP*W7.62* SOIC*3.9x9.9mm*P1.27mm* SO*5.3x10.2mm*P1.27mm*" (at 0 0 0))
      (symbol "CD4051B_0_1"
        (rectangle (start -10.16 6.35) (end -5.08 13.97)
          (fill (type none))
        )
        (rectangle (start -10.16 15.24) (end 10.16 -15.24)
          (fill (type background))
        )
        (circle (center -6.096 2.54) (radius 0.508)
          (fill (type none))
        )
        (circle (center -2.286 2.54) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.128 2.54)
            (xy -6.604 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.588 2.794)
            (xy -3.302 3.556)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.572 0)
            (xy -5.207 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.572 0.254)
            (xy -4.572 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.572 1.524)
            (xy -4.572 2.159)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.572 10.16)
            (xy -5.08 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 10.16)
            (xy -3.175 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.794)
            (xy 2.286 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 10.16)
            (xy -2.286 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 3.81)
            (xy -0.508 4.445)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 5.08)
            (xy -0.508 5.715)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 6.35)
            (xy -0.508 6.985)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 7.62)
            (xy -0.508 8.255)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 8.636)
            (xy -0.508 9.144)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 9.652)
            (xy -0.508 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 10.16)
            (xy -1.016 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 -12.7)
            (xy 5.842 -12.7)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 -10.16)
            (xy 5.842 -10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 -7.62)
            (xy 5.842 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 -5.08)
            (xy 5.842 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 -2.54)
            (xy 5.842 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 0)
            (xy 5.842 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 2.54)
            (xy 5.842 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 5.08)
            (xy 5.842 5.08)
          )
          (fill (type none))
        )
        (circle (center 3.556 -12.7) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 -10.16) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 -7.62) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 -5.08) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 -2.54) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 2.54) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.556 5.08) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "CD4051B_1_1"
        (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
          (name "X4")
          (number "1")
        )
        (pin input line (at -12.7 10.16 0) (length 2.54)
          (name "B")
          (number "10")
        )
        (pin input line (at -12.7 12.7 0) (length 2.54)
          (name "A")
          (number "11")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "X3")
          (number "12")
        )
        (pin bidirectional line (at 12.7 5.08 180) (length 2.54)
          (name "X0")
          (number "13")
        )
        (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
          (name "X1")
          (number "14")
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "X2")
          (number "15")
        )
        (pin power_in line (at 2.54 17.78 270) (length 2.54)
          (name "VDD")
          (number "16")
        )
        (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
          (name "X6")
          (number "2")
        )
        (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
          (name "X")
          (number "3")
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "X7")
          (number "4")
        )
        (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
          (name "X5")
          (number "5")
        )
        (pin input line (at -12.7 0 0) (length 2.54)
          (name "INH")
          (number "6")
        )
        (pin power_in line (at -2.54 -17.78 90) (length 2.54)
          (name "VEE")
          (number "7")
        )
        (pin power_in line (at 0 -17.78 90) (length 2.54)
          (name "VSS")
          (number "8")
        )
        (pin input line (at -12.7 7.62 0) (length 2.54)
          (name "C")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:D_Zener" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "D_Zener" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "diode" (at 0 0 0))
      (property "ki_description" "Zener diode" (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (at 0 0 0))
      (symbol "D_Zener_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy -0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_Zener_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Transistor_BJT:BC847" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at 5.08 1.905 0))
      (property "Value" "BC847" (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 5.08 -1.905 0))
      (property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657" (at 0 0 0))
      (property "ki_keywords" "NPN Small Signal Transistor" (at 0 0 0))
      (property "ki_description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-23" (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (at 0 0 0))
      (symbol "BC847_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "BC847_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "Transistor_BJT:BC858" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at 5.08 1.905 0))
      (property "Value" "BC858" (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 5.08 -1.905 0))
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC860-D.pdf" (at 0 0 0))
      (property "ki_keywords" "PNP transistor" (at 0 0 0))
      (property "ki_description" "0.1A Ic, 30V Vce, PNP Transistor, SOT-23" (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (at 0 0 0))
      (symbol "BC858_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -1.778)
            (xy 1.778 -2.286)
            (xy 1.27 -1.27)
            (xy 2.286 -1.778)
            (xy 2.286 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "BC858_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "Transistor_BJT:MMBTA42" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at 5.08 1.905 0))
      (property "Value" "MMBTA42" (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 5.08 -1.905 0))
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBTA42LT1-D.PDF" (at 0 0 0))
      (property "ki_keywords" "NPN High Voltage Transistor" (at 0 0 0))
      (property "ki_description" "0.5A Ic, 300V Vce, NPN High Voltage Transistor, SOT-23" (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (at 0 0 0))
      (symbol "MMBTA42_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0.635 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "MMBTA42_1_1"
        (pin input line (at -5.08 0 0) (length 5.08)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 116.84 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 48.26 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 48.26) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 62.23 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 92.71 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 87.63 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 86.36 36.83) (diameter 0) (color 0 0 0 0))
  (junction (at 39.37 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 116.84 48.26) (diameter 0) (color 0 0 0 0))
  (junction (at 62.23 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 119.38) (diameter 0) (color 0 0 0 0))
  (junction (at 62.23 104.14) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 68.58) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 177.8 92.71) (xy 177.8 91.44)))
  (wire (pts (xy 102.87 55.88) (xy 109.22 55.88)))
  (wire (pts (xy 123.19 92.71) (xy 133.35 92.71)))
  (wire (pts (xy 102.87 48.26) (xy 102.87 55.88)))
  (wire (pts (xy 62.23 36.83) (xy 62.23 40.64)))
  (wire (pts (xy 116.84 46.99) (xy 116.84 48.26)))
  (wire (pts (xy 62.23 68.58) (xy 83.82 68.58)))
  (wire (pts (xy 85.09 107.95) (xy 85.09 119.38)))
  (wire (pts (xy 128.27 43.18) (xy 128.27 48.26)))
  (wire (pts (xy 50.8 68.58) (xy 62.23 68.58)))
  (wire (pts (xy 48.26 55.88) (xy 50.8 55.88)))
  (wire (pts (xy 85.09 90.17) (xy 74.93 90.17)))
  (wire (pts (xy 132.08 48.26) (xy 128.27 48.26)))
  (wire (pts (xy 102.87 68.58) (xy 116.84 68.58)))
  (wire (pts (xy 53.34 104.14) (xy 62.23 104.14)))
  (wire (pts (xy 128.27 48.26) (xy 128.27 52.07)))
  (wire (pts (xy 139.7 68.58) (xy 128.27 68.58)))
  (wire (pts (xy 86.36 36.83) (xy 62.23 36.83)))
  (wire (pts (xy 177.8 66.04) (xy 177.8 68.58)))
  (wire (pts (xy 128.27 59.69) (xy 128.27 68.58)))
  (wire (pts (xy 116.84 39.37) (xy 116.84 36.83)))
  (wire (pts (xy 74.93 90.17) (xy 74.93 99.06)))
  (wire (pts (xy 143.51 53.34) (xy 139.7 53.34)))
  (wire (pts (xy 62.23 49.53) (xy 62.23 50.8)))
  (wire (pts (xy 143.51 43.18) (xy 128.27 43.18)))
  (wire (pts (xy 116.84 48.26) (xy 116.84 50.8)))
  (wire (pts (xy 83.82 66.04) (xy 83.82 68.58)))
  (wire (pts (xy 62.23 118.11) (xy 74.93 118.11)))
  (wire (pts (xy 88.9 48.26) (xy 83.82 48.26)))
  (wire (pts (xy 83.82 55.88) (xy 88.9 55.88)))
  (wire (pts (xy 62.23 60.96) (xy 62.23 68.58)))
  (wire (pts (xy 33.02 104.14) (xy 45.72 104.14)))
  (wire (pts (xy 62.23 104.14) (xy 62.23 105.41)))
  (wire (pts (xy 36.83 55.88) (xy 39.37 55.88)))
  (wire (pts (xy 102.87 55.88) (xy 102.87 57.15)))
  (wire (pts (xy 62.23 113.03) (xy 62.23 118.11)))
  (wire (pts (xy 177.8 80.01) (xy 177.8 76.2)))
  (wire (pts (xy 189.23 90.17) (xy 189.23 91.44)))
  (wire (pts (xy 177.8 91.44) (xy 189.23 91.44)))
  (wire (pts (xy 97.79 90.17) (xy 92.71 90.17)))
  (wire (pts (xy 139.7 48.26) (xy 143.51 48.26)))
  (wire (pts (xy 92.71 90.17) (xy 85.09 90.17)))
  (wire (pts (xy 116.84 60.96) (xy 116.84 68.58)))
  (wire (pts (xy 62.23 104.14) (xy 67.31 104.14)))
  (wire (pts (xy 83.82 48.26) (xy 83.82 55.88)))
  (wire (pts (xy 81.28 55.88) (xy 83.82 55.88)))
  (wire (pts (xy 139.7 53.34) (xy 139.7 68.58)))
  (wire (pts (xy 92.71 119.38) (xy 92.71 109.22)))
  (wire (pts (xy 50.8 55.88) (xy 50.8 58.42)))
  (wire (pts (xy 48.26 60.96) (xy 48.26 55.88)))
  (wire (pts (xy 83.82 55.88) (xy 83.82 58.42)))
  (wire (pts (xy 177.8 80.01) (xy 177.8 81.28)))
  (wire (pts (xy 116.84 68.58) (xy 128.27 68.58)))
  (wire (pts (xy 88.9 119.38) (xy 92.71 119.38)))
  (wire (pts (xy 74.93 118.11) (xy 74.93 109.22)))
  (wire (pts (xy 102.87 64.77) (xy 102.87 68.58)))
  (wire (pts (xy 96.52 55.88) (xy 102.87 55.88)))
  (wire (pts (xy 85.09 90.17) (xy 85.09 100.33)))
  (wire (pts (xy 46.99 55.88) (xy 48.26 55.88)))
  (wire (pts (xy 50.8 66.04) (xy 50.8 68.58)))
  (wire (pts (xy 116.84 48.26) (xy 128.27 48.26)))
  (wire (pts (xy 46.99 60.96) (xy 48.26 60.96)))
  (wire (pts (xy 116.84 36.83) (xy 86.36 36.83)))
  (wire (pts (xy 73.66 49.53) (xy 73.66 55.88)))
  (wire (pts (xy 83.82 68.58) (xy 87.63 68.58)))
  (wire (pts (xy 39.37 55.88) (xy 39.37 60.96)))
  (wire (pts (xy 85.09 119.38) (xy 88.9 119.38)))
  (wire (pts (xy 189.23 80.01) (xy 189.23 82.55)))
  (wire (pts (xy 50.8 55.88) (xy 54.61 55.88)))
  (wire (pts (xy 170.18 80.01) (xy 177.8 80.01)))
  (wire (pts (xy 96.52 48.26) (xy 102.87 48.26)))
  (wire (pts (xy 87.63 68.58) (xy 102.87 68.58)))
  (wire (pts (xy 62.23 49.53) (xy 73.66 49.53)))
  (wire (pts (xy 92.71 90.17) (xy 92.71 101.6)))
  (wire (pts (xy 177.8 80.01) (xy 189.23 80.01)))
  (wire (pts (xy 62.23 48.26) (xy 62.23 49.53)))
  (global_label "DBUS_SIGNAL " (shape input) (at 170.18 80.01 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 153.6481 80.01 0))
  )
  (global_label "RX_FROM_CPU" (shape input) (at 143.51 48.26 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 159.9209 48.26 0))
  )
  (global_label "TO_CPU" (shape input) (at 133.35 92.71 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 143.4714 92.71 0))
  )
  (global_label "ANTENNA" (shape input) (at 33.02 104.14 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 21.7495 104.14 0))
  )
  (global_label "DBUS_SIGNAL " (shape input) (at 143.51 43.18 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 160.0419 43.18 0))
  )
  (global_label "DBUS_GND   " (shape input) (at 143.51 53.34 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 159.3161 53.34 0))
  )
  (global_label "TX_FROM_CPU" (shape input) (at 36.83 55.88 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 20.7215 55.88 0))
  )
  (symbol (lib_id "Device:C") (at 43.18 60.96 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C1" (at 38.1 59.69 90))
    (property "Value" "C" (at 38.1 62.23 90))
    (property "Footprint" "" (at 46.99 59.9948 0))
    (property "Datasheet" "~" (at 43.18 60.96 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 62.23 44.45 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R6" (at 64.77 43.18 0))
    (property "Value" "4.7K" (at 64.77 45.72 0))
    (property "Footprint" "" (at 60.452 44.45 90))
    (property "Datasheet" "~" (at 62.23 44.45 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 86.36 36.83 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 86.36 40.64 0))
    (property "Value" "+5V" (at 86.36 31.75 0))
    (property "Footprint" "" (at 86.36 36.83 0))
    (property "Datasheet" "" (at 86.36 36.83 0))
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 135.89 48.26 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R2" (at 135.89 41.91 90))
    (property "Value" "1K" (at 135.89 44.45 90))
    (property "Footprint" "" (at 135.89 50.038 90))
    (property "Datasheet" "~" (at 135.89 48.26 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 50.8 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R7" (at 53.34 60.96 0))
    (property "Value" "4.7K" (at 53.34 63.5 0))
    (property "Footprint" "" (at 49.022 62.23 90))
    (property "Datasheet" "~" (at 50.8 62.23 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:D_Zener") (at 189.23 86.36 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 191.77 85.09 90))
    (property "Value" "5.1V" (at 191.77 87.63 90))
    (property "Footprint" "" (at 189.23 86.36 0))
    (property "Datasheet" "~" (at 189.23 86.36 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 43.18 55.88 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 43.18 49.53 90))
    (property "Value" "10K" (at 43.18 52.07 90))
    (property "Footprint" "" (at 43.18 57.658 90))
    (property "Datasheet" "~" (at 43.18 55.88 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_BJT:BC847") (at 59.69 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "Q3" (at 64.77 54.61 0))
    (property "Value" "BC847" (at 64.77 57.15 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 64.77 57.785 0))
    (property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657" (at 59.69 55.88 0))
    (pin "2")
    (pin "3")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "Q3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 88.9 119.38 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 88.9 125.73 0))
    (property "Value" "GND" (at 88.9 124.46 0))
    (property "Footprint" "" (at 88.9 119.38 0))
    (property "Datasheet" "" (at 88.9 119.38 0))
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 177.8 92.71 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 177.8 99.06 0))
    (property "Value" "GND" (at 177.8 97.79 0))
    (property "Footprint" "" (at 177.8 92.71 0))
    (property "Datasheet" "" (at 177.8 92.71 0))
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 92.71 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C4" (at 96.52 104.14 0))
    (property "Value" "C" (at 96.52 106.68 0))
    (property "Footprint" "" (at 93.6752 109.22 0))
    (property "Datasheet" "~" (at 92.71 105.41 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "C4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 92.71 48.26 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C3" (at 92.71 40.64 90))
    (property "Value" "C" (at 92.71 43.18 90))
    (property "Footprint" "" (at 96.52 47.2948 0))
    (property "Datasheet" "~" (at 92.71 48.26 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "C3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 102.87 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R3" (at 105.41 59.69 0))
    (property "Value" "10K" (at 105.41 62.23 0))
    (property "Footprint" "" (at 101.092 60.96 90))
    (property "Datasheet" "~" (at 102.87 60.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 83.82 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C2" (at 87.63 60.96 0))
    (property "Value" "C" (at 87.63 63.5 0))
    (property "Footprint" "" (at 84.7852 66.04 0))
    (property "Datasheet" "~" (at 83.82 62.23 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 49.53 104.14 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R10" (at 49.53 97.79 90))
    (property "Value" "2.2K" (at 49.53 100.33 90))
    (property "Footprint" "" (at 49.53 105.918 90))
    (property "Datasheet" "~" (at 49.53 104.14 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "R10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 62.23 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R9" (at 64.77 107.95 0))
    (property "Value" "1M" (at 64.77 110.49 0))
    (property "Footprint" "" (at 60.452 109.22 90))
    (property "Datasheet" "~" (at 62.23 109.22 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_BJT:BC847") (at 114.3 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "Q1" (at 119.38 54.61 0))
    (property "Value" "BC847" (at 119.38 57.15 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 119.38 57.785 0))
    (property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657" (at 114.3 55.88 0))
    (pin "3")
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "Q1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Analog_Switch:CD4051B") (at 110.49 95.25 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 105.7559 74.93 0))
    (property "Value" "CD4051B" (at 105.7559 77.47 0))
    (property "Footprint" "" (at 106.68 114.3 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4052b.pdf" (at 110.998 92.71 0))
    (pin "7")
    (pin "11")
    (pin "15")
    (pin "12")
    (pin "3")
    (pin "4")
    (pin "10")
    (pin "16")
    (pin "1")
    (pin "8")
    (pin "9")
    (pin "5")
    (pin "13")
    (pin "14")
    (pin "2")
    (pin "6")
    (instances
      (project "BoschOven"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_BJT:BC858") (at 72.39 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q2" (at 77.47 102.87 0))
    (property "Value" "MMBTA06" (at 76.2 109.22 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 77.47 106.045 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC860-D.pdf" (at 72.39 104.14 0))
    (pin "3")
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "Q2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 85.09 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R11" (at 87.63 102.87 0))
    (property "Value" "100K" (at 86.36 107.95 0))
    (property "Footprint" "" (at 83.312 104.14 90))
    (property "Datasheet" "~" (at 85.09 104.14 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 92.71 55.88 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R4" (at 92.71 53.34 90))
    (property "Value" "4.7K" (at 92.71 58.42 90))
    (property "Footprint" "" (at 92.71 57.658 90))
    (property "Datasheet" "~" (at 92.71 55.88 0))
    (pin "1")
    (pin "2")
    (instances
      (project "BoschOven"
        (path
          (reference "R4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 77.47 55.88 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R5" (at 77.47 49.53 90))
    (property "Value" "100" (at 77.47 52.07 90))
    (property "Footprint" "" (at 77.47 57.658 90))
    (property "Datasheet" "~" (at 77.47 55.88 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "R5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 177.8 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R12" (at 180.34 71.12 0))
    (property "Value" "470" (at 180.34 73.66 0))
    (property "Footprint" "" (at 176.022 72.39 90))
    (property "Datasheet" "~" (at 177.8 72.39 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "R12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 177.8 66.04 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 177.8 69.85 0))
    (property "Value" "+5V" (at 177.8 60.96 0))
    (property "Footprint" "" (at 177.8 66.04 0))
    (property "Datasheet" "" (at 177.8 66.04 0))
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 87.63 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 87.63 74.93 0))
    (property "Value" "GND" (at 87.63 73.66 0))
    (property "Footprint" "" (at 87.63 68.58 0))
    (property "Datasheet" "" (at 87.63 68.58 0))
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:D_Zener") (at 128.27 55.88 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 130.81 54.61 90))
    (property "Value" "5.1V" (at 130.81 57.15 90))
    (property "Footprint" "" (at 128.27 55.88 0))
    (property "Datasheet" "~" (at 128.27 55.88 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_BJT:MMBTA42") (at 175.26 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "Q4" (at 180.34 85.09 0))
    (property "Value" "MMBTA06" (at 180.34 87.63 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 180.34 88.265 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBTA42LT1-D.PDF" (at 175.26 86.36 0))
    (pin "3")
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "Q4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 116.84 43.18 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 119.38 41.91 0))
    (property "Value" "10K" (at 119.38 44.45 0))
    (property "Footprint" "" (at 115.062 43.18 90))
    (property "Datasheet" "~" (at 116.84 43.18 0))
    (pin "2")
    (pin "1")
    (instances
      (project "BoschOven"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
