<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="12" x2="40" y2="12" width="0" layer="20"/>
<wire x1="40" y1="12" x2="40" y2="0" width="0" layer="20"/>
<wire x1="40" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="12" width="0" layer="20"/>
<wire x1="17.78" y1="5.35" x2="17.78" y2="9.16" width="1.27" layer="20"/>
<wire x1="17.78" y1="9.16" x2="22.86" y2="9.16" width="1.27" layer="20"/>
<wire x1="22.86" y1="9.16" x2="22.86" y2="5.35" width="1.27" layer="20"/>
<hole x="4.98" y="6.02" drill="3.3"/>
<hole x="35" y="6" drill="3.3"/>
</plain>
<libraries>
<library name="sht4x">
<packages>
<package name="SHT4X">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-TIGHT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="sht4x" package="SHT4X" value="SHT4X_"/>
<element name="C1" library="SparkFun-Capacitors" package="0402-TIGHT" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="PROD_ID" value="CAP-14993"/>
</element>
<element name="SDA" library="wirepad" package="SMD1,27-2,54" value=" ">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SCL" library="wirepad" package="SMD1,27-2,54" value=" ">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="VDD" library="wirepad" package="SMD1,27-2,54" value=" ">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="VSS" library="wirepad" package="SMD1,27-2,54" value=" ">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="X1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="VDD" pad="1"/>
</signal>
<signal name="VSS">
<contactref element="X1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="VSS" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="SDA" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="SCL" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
