(module NETTIE3_CLOSE_THT (layer F.Cu) (tedit 5D763A0F)
  (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
  (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
  (attr virtual)
  (fp_text reference REF** (at 0 -1.905) (layer F.SilkS) hide)
  (fp_text value NETTIE3_CLOSE_THT (at 0 1.905) (layer F.Fab) hide)
  (pad 3 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 1 smd circle (at 5.08 0) (size 1 1) (layers B.Cu))
  (pad 2 smd circle (at -5.08 0) (size 1 1) (layers F.Cu))
)
