<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<packages>
<package name="VT9-PT">
<description>9 pin Vacuum tube socket VT9-PT</description>
</package>
<package name="NOVAL">
</package>
<package name="NOVAL1">
</package>
<package name="OKTAL">
</package>
<package name="OKTAL1">
</package>
<package name="ZM1000">
</package>
<package name="Z5680M">
<description>Package für Z5680M (selbserstellt). !! perfect !!</description>
</package>
<package name="MAGNOVAL_S9MCPC">
<description>Magnoval, 9-Pin, ceramic, print pc-mount

Magnoval Tube Socket, 9-Pin
ceramic, print pc-mount
used for EL519, EL500, EL503, EL504, EL509, PL500, PL504, PL509, PL519, 7868, 6GT5, 6KG6, 36KG6, 40KG6</description>
</package>
<package name="VT9-PT-2">
<description>Specially designed 9 pin vacuum tube socket for autowave
solder&gt;Belton Engineering Co.,Ltd.</description>
</package>
<package name="IN-19">
</package>
<package name="IN-18">
<description>May be used with socket: &lt;b&gt;PL31-P&lt;/b&gt;</description>
</package>
<package name="IN-17">
</package>
<package name="IN-16">
</package>
<package name="IN-14">
</package>
<package name="IN-13">
</package>
<package name="IN-12">
<description>May be used with socket: &lt;b&gt;SK-136&lt;/b&gt;</description>
</package>
<package name="IN-9">
</package>
<package name="IN-8-2">
</package>
<package name="IN-8">
<description>May be used with socket: &lt;b&gt;11-pin- Russian&lt;/b&gt;</description>
</package>
<package name="IN-6">
</package>
<package name="IN-3">
</package>
<package name="IN-1">
<description>May be used with socket: &lt;b&gt;U11&lt;/b&gt;</description>
</package>
<package name="ZM1042-MULTI-CONTACT">
<description>Socket with Multi-Contact (Mini-line Discret Socket Contact) Typ B1-B 41.0002</description>
</package>
<package name="ZM1042-AMP">
<description>Socket with AMP-Discret Socket Contact Typ 1-380758-1</description>
</package>
<package name="IN-18-MULTI-CONTACT">
<description>Socket with Multi-Contact (Mini-line Discret Socket Contact) Typ B1-B 41.0002</description>
</package>
<package name="IN-18-AMP">
<description>Socket with AMP-Discret Socket Contact Typ 1-380758-1</description>
</package>
<package name="B13B">
<description>Socket B13B print</description>
</package>
<package name="SK-207">
<description>&lt;b&gt;SK-207 Socket&lt;/b&gt;
&lt;p&gt;
The SK-207 Sockets are intented for use with Burroughs B-5750S and B-5850S Nixie tubes.</description>
</package>
<package name="MT-9P-PC">
<description>TUBE STOCKES</description>
</package>
<package name="VT8-PTS">
<description>VT8-PTS-B(High Insulated 8 Pin Vacuum Tube Socket)</description>
</package>
<package name="SK509">
<description>The Svetlana SK509 socket is an off-white ceramic socket which correctly
mates with 9-pin glass tubes having a standard magnoval base. Tube pinout
connections are made made through silver-plated solder wiring points.
Please refer to the appropriate tube technical data sheet for electrical
connections and cooling requirements.</description>
</package>
<package name="VT8-PTL-01">
<description>Fixing terminals on the P.C.B instead of bolt &amp; nut</description>
</package>
<package name="AMPEREX16_ZM1001">
</package>
<package name="MINI_P7">
</package>
</packages>
<symbols>
</symbols>
<devicesets>
</devicesets>
</library>
</drawing>
</eagle>
