(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "Signalkonverter Supersense > CBE DS300")
		(date "2026-01-25")
		(rev "1")
	)
	(lib_symbols
		(symbol "74xx:74LS573"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 16.51 0)
			)
			(property "Value" "74LS573"
				(at -7.62 -16.51 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "74xx/74hc573.pdf"
				(at 0 0 0)
			)
			(property "Description" "8-bit Latch 3-state outputs"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "TTL DFF DFF8 LATCH 3State"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP?20*"
				(at 0 0 0)
			)
			(symbol "74LS573_1_0"
				(pin input line
					(at -12.7 12.7 0)
					(length 5.08)
					(name "D0")
					(number "2")
				)
				(pin input line
					(at -12.7 10.16 0)
					(length 5.08)
					(name "D1")
					(number "3")
				)
				(pin input line
					(at -12.7 7.62 0)
					(length 5.08)
					(name "D2")
					(number "4")
				)
				(pin input line
					(at -12.7 5.08 0)
					(length 5.08)
					(name "D3")
					(number "5")
				)
				(pin input line
					(at -12.7 2.54 0)
					(length 5.08)
					(name "D4")
					(number "6")
				)
				(pin input line
					(at -12.7 0 0)
					(length 5.08)
					(name "D5")
					(number "7")
				)
				(pin input line
					(at -12.7 -2.54 0)
					(length 5.08)
					(name "D6")
					(number "8")
				)
				(pin input line
					(at -12.7 -5.08 0)
					(length 5.08)
					(name "D7")
					(number "9")
				)
				(pin input line
					(at -12.7 -10.16 0)
					(length 5.08)
					(name "Load")
					(number "11")
				)
				(pin input inverted
					(at -12.7 -12.7 0)
					(length 5.08)
					(name "OE")
					(number "1")
				)
				(pin power_in line
					(at 0 20.32 270)
					(length 5.08)
					(name "VCC")
					(number "20")
				)
				(pin power_in line
					(at 0 -20.32 90)
					(length 5.08)
					(name "GND")
					(number "10")
				)
				(pin tri_state line
					(at 12.7 12.7 180)
					(length 5.08)
					(name "Q0")
					(number "19")
				)
				(pin tri_state line
					(at 12.7 10.16 180)
					(length 5.08)
					(name "Q1")
					(number "18")
				)
				(pin tri_state line
					(at 12.7 7.62 180)
					(length 5.08)
					(name "Q2")
					(number "17")
				)
				(pin tri_state line
					(at 12.7 5.08 180)
					(length 5.08)
					(name "Q3")
					(number "16")
				)
				(pin tri_state line
					(at 12.7 2.54 180)
					(length 5.08)
					(name "Q4")
					(number "15")
				)
				(pin tri_state line
					(at 12.7 0 180)
					(length 5.08)
					(name "Q5")
					(number "14")
				)
				(pin tri_state line
					(at 12.7 -2.54 180)
					(length 5.08)
					(name "Q6")
					(number "13")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "Q7")
					(number "12")
				)
			)
			(symbol "74LS573_1_1"
				(rectangle
					(start -7.62 15.24)
					(end 7.62 -15.24)
					(fill
						(type background)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "AM2302_1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "VEHICLE ELECTRONIC"
				(at 9.144 11.938 0)
			)
			(property "Value" "~"
				(at -6.35 -1.2699 0)
			)
			(property "Footprint" "Sensor:ASAIR_AM2302_P2.54mm_Vertical"
				(at 0 -10.16 0)
			)
			(property "Datasheet" ""
				(at 3.81 6.35 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "digital sensor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "ASAIR*AM2302*P2.54mm*"
				(at 0 0 0)
			)
			(symbol "AM2302_1_0_1"
				(rectangle
					(start -5.08 10.16)
					(end 5.08 -5.08)
					(fill
						(type color)
						(color 255 190 90 1)
					)
				)
			)
			(symbol "AM2302_1_1_1"
				(pin passive line
					(at 0 -7.62 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 7.62 7.62 180)
					(length 2.54)
					(name "COM")
					(number "1")
				)
				(pin bidirectional line
					(at 7.62 3.81 180)
					(length 2.54)
					(name "33%")
					(number "2")
				)
				(pin bidirectional line
					(at 7.62 0 180)
					(length 2.54)
					(name "66%")
					(number "3")
				)
				(pin bidirectional line
					(at 7.62 -3.81 180)
					(length 2.54)
					(name "100%")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Converter_DCDC:R-78E5.0-0.5"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -3.81 3.175 0)
			)
			(property "Value" "R-78E5.0-0.5"
				(at 0 3.175 0)
			)
			(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
				(at 1.27 -6.35 0)
			)
			(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
				(at 0 0 0)
			)
			(property "Description" "500mA Step-Down DC/DC-Regulator, 7-28V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
				(at 0 0 0)
			)
			(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
				(at 0 0 0)
			)
			(symbol "R-78E5.0-0.5_0_1"
				(rectangle
					(start -5.08 1.905)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "R-78E5.0-0.5_1_1"
				(pin power_in line
					(at -7.62 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_out line
					(at 7.62 0 180)
					(length 2.54)
					(name "OUT")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C_Small"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.254 1.778 0)
			)
			(property "Value" "C_Small"
				(at 0.254 -2.032 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "capacitor cap"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_Small_0_1"
				(polyline
					(pts
						(xy -1.524 0.508) (xy 1.524 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.524 -0.508) (xy 1.524 -0.508)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 2.032)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.032)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:D_Schottky"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "D_Schottky"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Schottky diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode Schottky"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
				(at 0 0 0)
			)
			(symbol "D_Schottky_0_1"
				(polyline
					(pts
						(xy -1.905 0.635) (xy -1.905 1.27) (xy -1.27 1.27) (xy -1.27 -1.27) (xy -0.635 -1.27) (xy -0.635 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "D_Schottky_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:Fuse"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "F"
				(at 2.032 0 90)
			)
			(property "Value" "Fuse"
				(at -1.905 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Fuse"
				(at 0 0 0)
			)
			(property "ki_keywords" "fuse"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*Fuse*"
				(at 0 0 0)
			)
			(symbol "Fuse_0_1"
				(rectangle
					(start -0.762 -2.54)
					(end 0.762 2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Fuse_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:LED"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Isolator:EL817"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 5.08 0)
			)
			(property "Value" "EL817"
				(at 0 5.08 0)
			)
			(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
				(at -5.08 -5.08 0)
			)
			(property "Datasheet" "http://www.everlight.com/file/ProductFile/EL817.pdf"
				(at 0 0 0)
			)
			(property "Description" "DC Optocoupler, Vce 35V, DIP-4"
				(at 0 0 0)
			)
			(property "ki_keywords" "NPN DC Optocoupler"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm*"
				(at 0 0 0)
			)
			(symbol "EL817_0_1"
				(rectangle
					(start -5.08 3.81)
					(end 5.08 -3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -5.08 2.54) (xy -2.54 2.54) (xy -2.54 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -0.635) (xy -1.905 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -0.635) (xy -2.54 -2.54) (xy -5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -0.635) (xy -3.175 0.635) (xy -1.905 0.635) (xy -2.54 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.508) (xy 0.762 0.508) (xy 0.381 0.381) (xy 0.381 0.635) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.508) (xy 0.762 -0.508) (xy 0.381 -0.635) (xy 0.381 -0.381) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.905) (xy 2.54 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0.635) (xy 4.445 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -1.651) (xy 3.556 -1.143) (xy 4.064 -2.159) (xy 3.048 -1.651)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.445 2.54) (xy 5.08 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.445 -2.54) (xy 2.54 -0.635)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.445 -2.54) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "EL817_1_1"
				(pin passive line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "~")
					(number "2")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "~")
					(number "4")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "~")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "RF_Module:WEMOS_D1_mini"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 3.81 19.05 0)
			)
			(property "Value" "WEMOS_D1_mini"
				(at 1.27 -19.05 0)
			)
			(property "Footprint" "RF_Module:WEMOS_D1_mini_light"
				(at 0 -29.21 0)
			)
			(property "Datasheet" "https://wiki.wemos.cc/products:d1:d1_mini#documentation"
				(at -46.99 -29.21 0)
			)
			(property "Description" "32-bit microcontroller module with WiFi"
				(at 0 0 0)
			)
			(property "ki_keywords" "ESP8266 WiFi microcontroller ESP8266EX"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "WEMOS*D1*mini*"
				(at 0 0 0)
			)
			(symbol "WEMOS_D1_mini_1_1"
				(rectangle
					(start -7.62 17.78)
					(end 7.62 -17.78)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -10.16 10.16 0)
					(length 2.54)
					(name "~{RST}")
					(number "1")
				)
				(pin input line
					(at -10.16 2.54 0)
					(length 2.54)
					(name "RX")
					(number "15")
				)
				(pin output line
					(at -10.16 0 0)
					(length 2.54)
					(name "TX")
					(number "16")
				)
				(pin power_in line
					(at -2.54 20.32 270)
					(length 2.54)
					(name "5V")
					(number "9")
				)
				(pin power_in line
					(at 0 -20.32 90)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin power_out line
					(at 2.54 20.32 270)
					(length 2.54)
					(name "3V3")
					(number "8")
				)
				(pin input line
					(at 10.16 12.7 180)
					(length 2.54)
					(name "A0")
					(number "2")
				)
				(pin bidirectional line
					(at 10.16 10.16 180)
					(length 2.54)
					(name "D0")
					(number "3")
				)
				(pin bidirectional line
					(at 10.16 7.62 180)
					(length 2.54)
					(name "SCL/D1")
					(number "14")
				)
				(pin bidirectional line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "SDA/D2")
					(number "13")
				)
				(pin bidirectional line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "D3")
					(number "12")
				)
				(pin bidirectional line
					(at 10.16 0 180)
					(length 2.54)
					(name "D4")
					(number "11")
				)
				(pin bidirectional line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "SCK/D5")
					(number "4")
				)
				(pin bidirectional line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "MISO/D6")
					(number "5")
				)
				(pin bidirectional line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "MOSI/D7")
					(number "6")
				)
				(pin bidirectional line
					(at 10.16 -10.16 180)
					(length 2.54)
					(name "CS/D8")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Sensor:AM2302"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SENSOR1"
				(at -6.35 1.2701 0)
			)
			(property "Value" "~"
				(at -6.35 -1.2699 0)
			)
			(property "Footprint" "Sensor:ASAIR_AM2302_P2.54mm_Vertical"
				(at 0 -10.16 0)
			)
			(property "Datasheet" ""
				(at 3.81 6.35 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "digital sensor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "ASAIR*AM2302*P2.54mm*"
				(at 0 0 0)
			)
			(symbol "AM2302_0_1"
				(rectangle
					(start -5.08 10.16)
					(end 5.08 -5.08)
					(fill
						(type color)
						(color 255 190 90 1)
					)
				)
			)
			(symbol "AM2302_1_1"
				(pin power_in line
					(at 0 12.7 270)
					(length 2.54)
					(name "+Vin")
					(number "")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin output line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "Signal")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+12V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+12V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+12V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+12V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+12V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 233.68 35.56)
		(end 279.4 160.02)
		(fill
			(type color)
			(color 194 194 194 1)
		)
	)
	(text "externe Systeme"
		(exclude_from_sim no)
		(at 255.27 40.64 0)
	)
	(junction
		(at 104.1932 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 26.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 180.34 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 59.69 26.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 228.6 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 156.21 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 67.31 63.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 69.85 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 213.36 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 59.69 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 156.21 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.1932 26.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 63.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 194.31 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 208.28 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 107.95 153.67) (xy 95.25 153.67)
		)
	)
	(wire
		(pts
			(xy 120.65 90.17) (xy 133.35 90.17)
		)
	)
	(wire
		(pts
			(xy 215.9 95.25) (xy 237.49 95.25)
		)
	)
	(wire
		(pts
			(xy 86.36 26.67) (xy 82.55 26.67)
		)
	)
	(wire
		(pts
			(xy 209.55 107.95) (xy 215.9 107.95)
		)
	)
	(wire
		(pts
			(xy 20.32 52.07) (xy 59.69 52.07)
		)
	)
	(wire
		(pts
			(xy 184.15 67.31) (xy 255.27 67.31)
		)
	)
	(wire
		(pts
			(xy 156.21 153.67) (xy 180.34 153.67)
		)
	)
	(wire
		(pts
			(xy 120.65 92.71) (xy 143.51 92.71)
		)
	)
	(wire
		(pts
			(xy 262.89 153.67) (xy 262.89 77.47)
		)
	)
	(wire
		(pts
			(xy 80.01 92.71) (xy 95.25 92.71)
		)
	)
	(wire
		(pts
			(xy 104.1932 26.67) (xy 104.1932 38.1)
		)
	)
	(wire
		(pts
			(xy 88.9 107.95) (xy 88.9 97.79)
		)
	)
	(wire
		(pts
			(xy 59.69 52.07) (xy 74.93 52.07)
		)
	)
	(wire
		(pts
			(xy 95.25 153.67) (xy 69.85 153.67)
		)
	)
	(wire
		(pts
			(xy 86.36 26.67) (xy 86.36 38.1)
		)
	)
	(wire
		(pts
			(xy 40.64 26.67) (xy 49.53 26.67)
		)
	)
	(wire
		(pts
			(xy 88.9 82.55) (xy 80.01 82.55)
		)
	)
	(wire
		(pts
			(xy 228.6 119.38) (xy 228.6 87.63)
		)
	)
	(wire
		(pts
			(xy 20.32 26.67) (xy 33.02 26.67)
		)
	)
	(wire
		(pts
			(xy 67.31 63.5) (xy 67.31 74.93)
		)
	)
	(wire
		(pts
			(xy 237.49 87.63) (xy 228.6 87.63)
		)
	)
	(wire
		(pts
			(xy 57.15 26.67) (xy 59.69 26.67)
		)
	)
	(wire
		(pts
			(xy 143.51 121.92) (xy 156.21 121.92)
		)
	)
	(wire
		(pts
			(xy 80.01 90.17) (xy 95.25 90.17)
		)
	)
	(wire
		(pts
			(xy 86.36 52.07) (xy 104.1932 52.07)
		)
	)
	(wire
		(pts
			(xy 120.65 87.63) (xy 123.19 87.63)
		)
	)
	(wire
		(pts
			(xy 156.21 142.24) (xy 156.21 153.67)
		)
	)
	(wire
		(pts
			(xy 143.51 97.79) (xy 143.51 121.92)
		)
	)
	(wire
		(pts
			(xy 209.55 102.87) (xy 213.36 102.87)
		)
	)
	(wire
		(pts
			(xy 120.65 100.33) (xy 130.81 100.33)
		)
	)
	(wire
		(pts
			(xy 194.31 153.67) (xy 208.28 153.67)
		)
	)
	(wire
		(pts
			(xy 88.9 97.79) (xy 80.01 97.79)
		)
	)
	(wire
		(pts
			(xy 231.14 99.06) (xy 231.14 124.46)
		)
	)
	(wire
		(pts
			(xy 208.28 124.46) (xy 208.28 153.67)
		)
	)
	(wire
		(pts
			(xy 194.31 107.95) (xy 194.31 153.67)
		)
	)
	(wire
		(pts
			(xy 95.25 110.49) (xy 95.25 153.67)
		)
	)
	(wire
		(pts
			(xy 59.69 26.67) (xy 67.31 26.67)
		)
	)
	(wire
		(pts
			(xy 231.14 99.06) (xy 237.49 99.06)
		)
	)
	(wire
		(pts
			(xy 107.95 63.5) (xy 156.21 63.5)
		)
	)
	(wire
		(pts
			(xy 104.1932 52.07) (xy 114.3 52.07)
		)
	)
	(wire
		(pts
			(xy 74.93 34.29) (xy 74.93 52.07)
		)
	)
	(wire
		(pts
			(xy 231.14 124.46) (xy 223.52 124.46)
		)
	)
	(wire
		(pts
			(xy 171.45 90.17) (xy 171.45 102.87)
		)
	)
	(wire
		(pts
			(xy 95.25 107.95) (xy 88.9 107.95)
		)
	)
	(wire
		(pts
			(xy 107.95 63.5) (xy 107.95 77.47)
		)
	)
	(wire
		(pts
			(xy 168.91 92.71) (xy 168.91 119.38)
		)
	)
	(wire
		(pts
			(xy 67.31 63.5) (xy 107.95 63.5)
		)
	)
	(wire
		(pts
			(xy 120.65 97.79) (xy 143.51 97.79)
		)
	)
	(wire
		(pts
			(xy 113.03 26.67) (xy 104.1932 26.67)
		)
	)
	(wire
		(pts
			(xy 176.53 67.31) (xy 88.9 67.31)
		)
	)
	(wire
		(pts
			(xy 130.81 153.67) (xy 156.21 153.67)
		)
	)
	(wire
		(pts
			(xy 69.85 115.57) (xy 69.85 153.67)
		)
	)
	(wire
		(pts
			(xy 74.93 52.07) (xy 86.36 52.07)
		)
	)
	(wire
		(pts
			(xy 59.69 26.67) (xy 59.69 38.1)
		)
	)
	(wire
		(pts
			(xy 180.34 92.71) (xy 180.34 153.67)
		)
	)
	(wire
		(pts
			(xy 130.81 87.63) (xy 180.34 87.63)
		)
	)
	(wire
		(pts
			(xy 156.21 107.95) (xy 156.21 121.92)
		)
	)
	(wire
		(pts
			(xy 208.28 153.67) (xy 262.89 153.67)
		)
	)
	(wire
		(pts
			(xy 168.91 119.38) (xy 208.28 119.38)
		)
	)
	(wire
		(pts
			(xy 228.6 87.63) (xy 213.36 87.63)
		)
	)
	(wire
		(pts
			(xy 24.13 63.5) (xy 67.31 63.5)
		)
	)
	(wire
		(pts
			(xy 180.34 153.67) (xy 194.31 153.67)
		)
	)
	(wire
		(pts
			(xy 88.9 67.31) (xy 88.9 82.55)
		)
	)
	(wire
		(pts
			(xy 213.36 87.63) (xy 195.58 87.63)
		)
	)
	(wire
		(pts
			(xy 130.81 128.27) (xy 130.81 133.35)
		)
	)
	(wire
		(pts
			(xy 223.52 119.38) (xy 228.6 119.38)
		)
	)
	(wire
		(pts
			(xy 140.97 90.17) (xy 171.45 90.17)
		)
	)
	(wire
		(pts
			(xy 80.01 87.63) (xy 95.25 87.63)
		)
	)
	(wire
		(pts
			(xy 200.66 92.71) (xy 195.58 92.71)
		)
	)
	(wire
		(pts
			(xy 130.81 140.97) (xy 130.81 153.67)
		)
	)
	(wire
		(pts
			(xy 80.01 95.25) (xy 95.25 95.25)
		)
	)
	(wire
		(pts
			(xy 215.9 107.95) (xy 215.9 95.25)
		)
	)
	(wire
		(pts
			(xy 237.49 91.44) (xy 200.66 91.44)
		)
	)
	(wire
		(pts
			(xy 104.1932 43.18) (xy 104.1932 52.07)
		)
	)
	(wire
		(pts
			(xy 171.45 102.87) (xy 194.31 102.87)
		)
	)
	(wire
		(pts
			(xy 86.36 43.18) (xy 86.36 52.07)
		)
	)
	(wire
		(pts
			(xy 156.21 121.92) (xy 156.21 132.08)
		)
	)
	(wire
		(pts
			(xy 107.95 153.67) (xy 130.81 153.67)
		)
	)
	(wire
		(pts
			(xy 59.69 43.18) (xy 59.69 52.07)
		)
	)
	(wire
		(pts
			(xy 130.81 100.33) (xy 130.81 120.65)
		)
	)
	(wire
		(pts
			(xy 156.21 63.5) (xy 156.21 100.33)
		)
	)
	(wire
		(pts
			(xy 213.36 102.87) (xy 213.36 87.63)
		)
	)
	(wire
		(pts
			(xy 104.1932 26.67) (xy 86.36 26.67)
		)
	)
	(wire
		(pts
			(xy 69.85 153.67) (xy 21.59 153.67)
		)
	)
	(wire
		(pts
			(xy 200.66 91.44) (xy 200.66 92.71)
		)
	)
	(wire
		(pts
			(xy 107.95 118.11) (xy 107.95 153.67)
		)
	)
	(wire
		(pts
			(xy 168.91 92.71) (xy 151.13 92.71)
		)
	)
	(global_label "5V"
		(shape input)
		(at 24.13 63.5 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 18.8467 63.5 0)
		)
	)
	(global_label "+5V"
		(shape input)
		(at 113.03 26.67 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 119.8857 26.67 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 21.59 153.67 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 14.7343 153.67 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 114.3 52.07 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.1557 52.07 0)
		)
	)
	(symbol
		(lib_id "power:+12V")
		(at 262.89 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 262.89 60.96 0)
		)
		(property "Value" "+12V"
			(at 262.89 52.07 0)
		)
		(property "Footprint" ""
			(at 262.89 57.15 0)
		)
		(property "Datasheet" ""
			(at 262.89 57.15 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+12V\""
			(at 262.89 57.15 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Converter_DCDC:R-78E5.0-0.5")
		(at 74.93 26.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 74.93 20.32 0)
		)
		(property "Value" "RECOM R-78E5.0-0.5"
			(at 74.93 22.86 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 76.2 33.02 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
			(at 74.93 26.67 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 7-28V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 74.93 26.67 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Isolator:EL817")
		(at 187.96 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Opt1"
			(at 187.96 81.28 0)
		)
		(property "Value" "EL817"
			(at 187.96 83.82 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 182.88 95.25 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/EL817.pdf"
			(at 187.96 90.17 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, DIP-4"
			(at 187.96 90.17 0)
		)
		(pin "1")
		(pin "4")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "Opt1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 86.36 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C2"
			(at 88.9 39.3762 0)
		)
		(property "Value" "100uF 10V"
			(at 88.9 41.9162 0)
		)
		(property "Footprint" ""
			(at 86.36 40.64 0)
		)
		(property "Datasheet" "~"
			(at 86.36 40.64 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 86.36 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "test"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 20.32 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 20.32 58.42 0)
		)
		(property "Value" "GND"
			(at 20.32 57.15 0)
		)
		(property "Footprint" ""
			(at 20.32 52.07 0)
		)
		(property "Datasheet" ""
			(at 20.32 52.07 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 20.32 52.07 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 59.69 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 62.23 39.3762 0)
		)
		(property "Value" "100uF 16V"
			(at 62.23 41.9162 0)
		)
		(property "Footprint" ""
			(at 59.69 40.64 0)
		)
		(property "Datasheet" "~"
			(at 59.69 40.64 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 59.69 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 180.34 67.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 180.34 60.96 90)
		)
		(property "Value" "1k"
			(at 180.34 63.5 90)
		)
		(property "Footprint" ""
			(at 180.34 65.532 90)
		)
		(property "Datasheet" "~"
			(at 180.34 67.31 0)
		)
		(property "Description" "Resistor"
			(at 180.34 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "RF_Module:WEMOS_D1_mini")
		(at 69.85 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "MC"
			(at 71.9933 115.57 0)
		)
		(property "Value" "WEMOS_D1_mini"
			(at 72.136 118.618 0)
		)
		(property "Footprint" "RF_Module:WEMOS_D1_mini_light"
			(at 69.85 124.46 0)
		)
		(property "Datasheet" "https://wiki.wemos.cc/products:d1:d1_mini#documentation"
			(at 22.86 124.46 0)
		)
		(property "Description" "32-bit microcontroller module with WiFi"
			(at 69.85 95.25 0)
		)
		(pin "10")
		(pin "2")
		(pin "1")
		(pin "9")
		(pin "16")
		(pin "15")
		(pin "8")
		(pin "14")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "3")
		(pin "13")
		(pin "11")
		(pin "7")
		(pin "12")
		(instances
			(project ""
				(path
					(reference "MC")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 137.16 90.17 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 137.16 83.82 90)
		)
		(property "Value" "1k"
			(at 137.16 86.36 90)
		)
		(property "Footprint" ""
			(at 137.16 88.392 90)
		)
		(property "Datasheet" "~"
			(at 137.16 90.17 0)
		)
		(property "Description" "Resistor"
			(at 137.16 90.17 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "test"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Sensor:AM2302")
		(at 262.89 69.85 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SENSOR1"
			(at 269.24 68.5799 0)
		)
		(property "Value" "~"
			(at 269.24 71.1199 0)
		)
		(property "Footprint" ""
			(at 262.89 80.01 0)
		)
		(property "Datasheet" ""
			(at 259.08 63.5 0)
		)
		(property "Description" ""
			(at 262.89 69.85 0)
		)
		(pin "4")
		(pin "2")
		(pin "")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "SENSOR1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Isolator:EL817")
		(at 201.93 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Opt2"
			(at 201.93 96.52 0)
		)
		(property "Value" "EL817"
			(at 201.93 99.06 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 196.85 110.49 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/EL817.pdf"
			(at 201.93 105.41 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, DIP-4"
			(at 201.93 105.41 0)
		)
		(pin "1")
		(pin "4")
		(pin "3")
		(pin "2")
		(instances
			(project "test"
				(path
					(reference "Opt2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 104.14 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 106.68 39.3762 0)
		)
		(property "Value" "100nF (Keramik)"
			(at 106.68 41.9162 0)
		)
		(property "Footprint" ""
			(at 104.14 40.64 0)
		)
		(property "Datasheet" "~"
			(at 104.14 40.64 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 104.14 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "test"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Isolator:EL817")
		(at 215.9 121.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Opt3"
			(at 215.9 113.03 0)
		)
		(property "Value" "EL817"
			(at 215.9 115.57 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 210.82 127 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/EL817.pdf"
			(at 215.9 121.92 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, DIP-4"
			(at 215.9 121.92 0)
		)
		(pin "1")
		(pin "4")
		(pin "3")
		(pin "2")
		(instances
			(project "test"
				(path
					(reference "Opt3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Fuse")
		(at 53.34 26.67 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "F1"
			(at 53.34 20.32 90)
		)
		(property "Value" "Fuse 500mA träge"
			(at 53.34 22.86 90)
		)
		(property "Footprint" ""
			(at 53.34 24.892 90)
		)
		(property "Datasheet" "~"
			(at 53.34 26.67 0)
		)
		(property "Description" "Fuse"
			(at 53.34 26.67 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "F1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 147.32 92.71 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 147.32 86.36 90)
		)
		(property "Value" "1k"
			(at 147.32 88.9 90)
		)
		(property "Footprint" ""
			(at 147.32 90.932 90)
		)
		(property "Datasheet" "~"
			(at 147.32 92.71 0)
		)
		(property "Description" "Resistor"
			(at 147.32 92.71 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "test"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 130.81 124.46 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 133.35 123.1899 0)
		)
		(property "Value" "1k"
			(at 133.35 125.7299 0)
		)
		(property "Footprint" ""
			(at 132.588 124.46 90)
		)
		(property "Datasheet" "~"
			(at 130.81 124.46 0)
		)
		(property "Description" "Resistor"
			(at 130.81 124.46 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "test"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 127 87.63 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 127 81.28 90)
		)
		(property "Value" "1k"
			(at 127 83.82 90)
		)
		(property "Footprint" ""
			(at 127 85.852 90)
		)
		(property "Datasheet" "~"
			(at 127 87.63 0)
		)
		(property "Description" "Resistor"
			(at 127 87.63 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "test"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 130.81 137.16 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 134.62 137.4774 90)
		)
		(property "Value" "LED"
			(at 134.62 140.0174 90)
		)
		(property "Footprint" ""
			(at 130.81 137.16 0)
		)
		(property "Datasheet" "~"
			(at 130.81 137.16 0)
		)
		(property "Description" "Light emitting diode"
			(at 130.81 137.16 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 130.81 137.16 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS573")
		(at 107.95 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Latch1"
			(at 110.0933 77.47 0)
		)
		(property "Value" "74LS573"
			(at 110.0933 80.01 0)
		)
		(property "Footprint" ""
			(at 107.95 97.79 0)
		)
		(property "Datasheet" "74xx/74hc573.pdf"
			(at 107.95 97.79 0)
		)
		(property "Description" "8-bit Latch 3-state outputs"
			(at 107.95 97.79 0)
		)
		(pin "2")
		(pin "4")
		(pin "7")
		(pin "3")
		(pin "5")
		(pin "6")
		(pin "8")
		(pin "12")
		(pin "13")
		(pin "20")
		(pin "19")
		(pin "18")
		(pin "1")
		(pin "10")
		(pin "16")
		(pin "15")
		(pin "14")
		(pin "11")
		(pin "9")
		(pin "17")
		(instances
			(project ""
				(path
					(reference "Latch1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+12V")
		(at 20.32 26.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 20.32 30.48 0)
		)
		(property "Value" "+12V"
			(at 20.32 21.59 0)
		)
		(property "Footprint" ""
			(at 20.32 26.67 0)
		)
		(property "Datasheet" ""
			(at 20.32 26.67 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+12V\""
			(at 20.32 26.67 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:D_Schottky")
		(at 36.83 26.67 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 37.1475 20.32 0)
		)
		(property "Value" "D_Schottky"
			(at 37.1475 22.86 0)
		)
		(property "Footprint" ""
			(at 36.83 26.67 0)
		)
		(property "Datasheet" "~"
			(at 36.83 26.67 0)
		)
		(property "Description" "Schottky diode"
			(at 36.83 26.67 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 156.21 104.14 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 158.75 102.8699 0)
		)
		(property "Value" "10k"
			(at 158.75 105.4099 0)
		)
		(property "Footprint" ""
			(at 157.988 104.14 90)
		)
		(property "Datasheet" "~"
			(at 156.21 104.14 0)
		)
		(property "Description" "Resistor"
			(at 156.21 104.14 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "test"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 156.21 137.16 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 160.02 135.8899 90)
		)
		(property "Value" "SW_Push"
			(at 160.02 138.4299 90)
		)
		(property "Footprint" ""
			(at 161.29 137.16 0)
		)
		(property "Datasheet" "~"
			(at 161.29 137.16 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 156.21 137.16 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "AM2302_1")
		(lib_id "Sensor:AM2302")
		(at 245.11 95.25 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "VEHICLE ELECTRONIC"
			(at 235.966 83.312 0)
		)
		(property "Value" "~"
			(at 251.46 96.5199 0)
		)
		(property "Footprint" "Sensor:ASAIR_AM2302_P2.54mm_Vertical"
			(at 245.11 105.41 0)
		)
		(property "Datasheet" ""
			(at 241.3 88.9 0)
		)
		(property "Description" ""
			(at 245.11 95.25 0)
		)
		(pin "4")
		(pin "2")
		(pin "1")
		(pin "3")
		(pin "4")
		(instances
			(project "test"
				(path
					(reference "VEHICLE ELECTRONIC")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
