(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "BD139_1"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "BD139"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
				(at 0 0 0)
			)
			(property "Description" "1.5A Ic, 80V Vce, Low Voltage Transistor, TO-126"
				(at 0 0 0)
			)
			(property "Sim.Device" "NPN"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=E 2=C 3=B"
				(at 0 0 0)
			)
			(property "ki_keywords" "Low Voltage Transistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO?126*"
				(at 0 0 0)
			)
			(symbol "BD139_1_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 0.635 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
			)
			(symbol "BD139_1_1_1"
				(polyline
					(pts
						(xy 0.635 0.635) (xy 2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 -0.635) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.778) (xy 1.778 -1.27) (xy 2.286 -2.286) (xy 1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "3")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "C")
					(number "2")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "E")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C_Polarized_Small"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.254 1.778 0)
			)
			(property "Value" "C_Polarized_Small"
				(at 0.254 -2.032 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Polarized capacitor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "CP_*"
				(at 0 0 0)
			)
			(symbol "C_Polarized_Small_0_1"
				(rectangle
					(start -1.524 0.6858)
					(end 1.524 0.3048)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.524 -0.3048)
					(end 1.524 -0.6858)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.524) (xy -0.762 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 1.27) (xy -1.016 1.778)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_Polarized_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 1.8542)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 1.8542)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R_Small"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 0 0 90)
			)
			(property "Value" "R_Small"
				(at 1.778 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "R resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_Small_0_1"
				(rectangle
					(start -0.762 1.778)
					(end 0.762 -1.778)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 0.762)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.762)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diode:1N4006"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "1N4006"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
				(at 0 -4.445 0)
			)
			(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
				(at 0 0 0)
			)
			(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*DO?41*"
				(at 0 0 0)
			)
			(symbol "1N4006_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "1N4006_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diode:1N4148"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "1N4148"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
				(at 0 0 0)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
				(at 0 0 0)
			)
			(property "Description" "100V 0.15A standard switching diode, DO-35"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*DO?35*"
				(at 0 0 0)
			)
			(symbol "1N4148_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "1N4148_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
			)
			(property "Value" ""
				(at 0 0 0)
			)
			(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "hongfa_hfd2/012-s-l2-d_0_1"
				(rectangle
					(start -41.91 5.08)
					(end -13.97 -5.08)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -41.275 1.905)
					(end -34.925 -1.905)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -41.275 0) (xy -34.29 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -41.021 0) (xy -35.306 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -41.021 -1.905) (xy -35.433 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -40.64 5.08) (xy -40.64 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -40.64 -5.08) (xy -40.64 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -35.56 5.08) (xy -35.56 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -35.56 -5.08) (xy -35.56 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -33.655 0) (xy -33.02 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -32.385 0) (xy -31.75 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -31.115 0) (xy -30.48 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -29.845 0) (xy -29.21 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -28.575 0) (xy -27.94 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -27.94 5.08) (xy -27.94 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -27.94 3.81) (xy -27.94 1.27) (xy -21.59 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -27.94 -3.81) (xy -27.94 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -27.94 -3.81) (xy -27.94 -1.27) (xy -21.59 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -27.305 0) (xy -26.67 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -26.035 0) (xy -25.4 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -24.765 0) (xy -24.13 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -23.495 0) (xy -22.86 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -22.225 0) (xy -21.59 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 5.08) (xy -21.59 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 1.27) (xy -21.59 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 1.27) (xy -15.24 1.27) (xy -15.24 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 -1.27) (xy -21.59 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 -1.27) (xy -15.24 -1.27) (xy -15.24 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 -3.81) (xy -21.59 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -20.955 0) (xy -20.32 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -19.685 0) (xy -19.05 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -15.24 5.08) (xy -15.24 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -15.24 -2.54) (xy -15.24 -6.35)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "hongfa_hfd2/012-s-l2-d_1_1"
				(pin input line
					(at -40.64 7.62 270)
					(length 2.54)
					(name "-")
					(number "16")
				)
				(pin input line
					(at -40.64 -7.62 90)
					(length 2.54)
					(name "+")
					(number "1")
				)
				(pin input line
					(at -35.56 7.62 270)
					(length 2.54)
					(name "-")
					(number "15")
				)
				(pin input line
					(at -35.56 -7.62 90)
					(length 2.54)
					(name "+")
					(number "2")
				)
				(pin input line
					(at -27.94 7.62 270)
					(length 2.54)
					(name "~")
					(number "13")
				)
				(pin input line
					(at -27.94 -7.62 90)
					(length 2.54)
					(name "~")
					(number "4")
				)
				(pin output line
					(at -21.59 7.62 270)
					(length 2.54)
					(name "~")
					(number "11")
				)
				(pin output line
					(at -21.59 -7.62 90)
					(length 2.54)
					(name "~")
					(number "6")
				)
				(pin output line
					(at -15.24 7.62 270)
					(length 2.54)
					(name "~")
					(number "9")
				)
				(pin output line
					(at -15.24 -7.62 90)
					(length 2.54)
					(name "~")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistor_BJT:BD139"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "BD139"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
				(at 0 0 0)
			)
			(property "Description" "1.5A Ic, 80V Vce, Low Voltage Transistor, TO-126"
				(at 0 0 0)
			)
			(property "Sim.Device" "NPN"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=E 2=C 3=B"
				(at 0 0 0)
			)
			(property "ki_keywords" "Low Voltage Transistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO?126*"
				(at 0 0 0)
			)
			(symbol "BD139_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 0.635 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
			)
			(symbol "BD139_1_1"
				(polyline
					(pts
						(xy 0.635 0.635) (xy 2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 -0.635) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.778) (xy 1.778 -1.27) (xy 2.286 -2.286) (xy 1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "3")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "C")
					(number "2")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "E")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 213.36 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.2 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 209.55 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 210.82 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 233.68 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 87.63 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 213.36 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 41.91 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 16.51 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 233.68 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 180.34 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 41.91 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 205.74 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 90.17 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 21.59 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 19.05 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 20.32 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 134.62 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 234.95 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 180.34 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 67.31 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 19.05 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 49.53 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 156.21 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 224.79 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 16.51 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 21.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 180.34 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 132.08 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 213.36 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 16.51 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 44.45 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 160.02 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 87.63 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 26.67 54.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 177.8 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 228.6 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 213.36 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 34.29 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.2 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 26.67 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 181.61 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 204.47 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 34.29 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 213.36 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 180.34 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 204.47 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 200.66 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 31.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 231.14 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 213.36 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 31.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 231.14 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 177.8 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 54.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 41.91 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 118.11 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 212.09 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 205.74 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 132.08 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 185.42 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 90.17 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 49.53 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 21.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 224.79 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 209.55 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 228.6 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 181.61 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 66.04 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 135.89 149.86) (xy 135.89 158.75)
		)
	)
	(wire
		(pts
			(xy 57.15 146.05) (xy 60.96 146.05)
		)
	)
	(wire
		(pts
			(xy 33.02 91.44) (xy 21.59 91.44)
		)
	)
	(wire
		(pts
			(xy 81.28 86.36) (xy 80.01 86.36)
		)
	)
	(wire
		(pts
			(xy 114.3 92.71) (xy 118.11 92.71)
		)
	)
	(wire
		(pts
			(xy 148.59 142.24) (xy 147.32 142.24)
		)
	)
	(wire
		(pts
			(xy 66.04 105.41) (xy 68.58 105.41)
		)
	)
	(wire
		(pts
			(xy 160.02 96.52) (xy 160.02 105.41)
		)
	)
	(wire
		(pts
			(xy 113.03 149.86) (xy 118.11 149.86)
		)
	)
	(wire
		(pts
			(xy 91.44 138.43) (xy 92.71 138.43)
		)
	)
	(wire
		(pts
			(xy 130.81 142.24) (xy 130.81 130.81)
		)
	)
	(wire
		(pts
			(xy 207.01 142.24) (xy 217.17 142.24)
		)
	)
	(wire
		(pts
			(xy 21.59 91.44) (xy 21.59 96.52)
		)
	)
	(wire
		(pts
			(xy 134.62 96.52) (xy 134.62 105.41)
		)
	)
	(wire
		(pts
			(xy 86.36 96.52) (xy 86.36 105.41)
		)
	)
	(wire
		(pts
			(xy 86.36 153.67) (xy 86.36 146.05)
		)
	)
	(wire
		(pts
			(xy 177.8 153.67) (xy 180.34 153.67)
		)
	)
	(wire
		(pts
			(xy 223.52 144.78) (xy 212.09 144.78)
		)
	)
	(wire
		(pts
			(xy 63.5 68.58) (xy 63.5 96.52)
		)
	)
	(wire
		(pts
			(xy 129.54 105.41) (xy 132.08 105.41)
		)
	)
	(wire
		(pts
			(xy 228.6 85.09) (xy 228.6 72.39)
		)
	)
	(wire
		(pts
			(xy 162.56 146.05) (xy 162.56 138.43)
		)
	)
	(wire
		(pts
			(xy 125.73 142.24) (xy 124.46 142.24)
		)
	)
	(wire
		(pts
			(xy 185.42 105.41) (xy 187.96 105.41)
		)
	)
	(wire
		(pts
			(xy 162.56 153.67) (xy 162.56 146.05)
		)
	)
	(wire
		(pts
			(xy 154.94 149.86) (xy 154.94 132.08)
		)
	)
	(wire
		(pts
			(xy 113.03 96.52) (xy 113.03 105.41)
		)
	)
	(wire
		(pts
			(xy 181.61 132.08) (xy 209.55 132.08)
		)
	)
	(wire
		(pts
			(xy 45.72 138.43) (xy 45.72 146.05)
		)
	)
	(wire
		(pts
			(xy 118.11 69.85) (xy 118.11 88.9)
		)
	)
	(wire
		(pts
			(xy 154.94 68.58) (xy 154.94 96.52)
		)
	)
	(wire
		(pts
			(xy 212.09 144.78) (xy 212.09 149.86)
		)
	)
	(wire
		(pts
			(xy 104.14 88.9) (xy 104.14 90.17)
		)
	)
	(wire
		(pts
			(xy 180.34 153.67) (xy 180.34 146.05)
		)
	)
	(wire
		(pts
			(xy 114.3 86.36) (xy 116.84 86.36)
		)
	)
	(wire
		(pts
			(xy 189.23 138.43) (xy 189.23 146.05)
		)
	)
	(wire
		(pts
			(xy 85.09 130.81) (xy 107.95 130.81)
		)
	)
	(wire
		(pts
			(xy 57.15 92.71) (xy 60.96 92.71)
		)
	)
	(wire
		(pts
			(xy 90.17 90.17) (xy 90.17 96.52)
		)
	)
	(wire
		(pts
			(xy 31.75 31.75) (xy 31.75 35.56)
		)
	)
	(wire
		(pts
			(xy 148.59 149.86) (xy 154.94 149.86)
		)
	)
	(wire
		(pts
			(xy 21.59 105.41) (xy 22.86 105.41)
		)
	)
	(wire
		(pts
			(xy 107.95 142.24) (xy 118.11 142.24)
		)
	)
	(wire
		(pts
			(xy 187.96 149.86) (xy 193.04 149.86)
		)
	)
	(wire
		(pts
			(xy 68.58 73.66) (xy 91.44 73.66)
		)
	)
	(wire
		(pts
			(xy 45.72 146.05) (xy 49.53 146.05)
		)
	)
	(wire
		(pts
			(xy 39.37 130.81) (xy 16.51 130.81)
		)
	)
	(wire
		(pts
			(xy 234.95 58.42) (xy 234.95 68.58)
		)
	)
	(wire
		(pts
			(xy 140.97 69.85) (xy 140.97 88.9)
		)
	)
	(wire
		(pts
			(xy 232.41 85.09) (xy 232.41 133.35)
		)
	)
	(wire
		(pts
			(xy 41.91 132.08) (xy 64.77 132.08)
		)
	)
	(wire
		(pts
			(xy 189.23 146.05) (xy 189.23 153.67)
		)
	)
	(wire
		(pts
			(xy 21.59 64.77) (xy 21.59 58.42)
		)
	)
	(wire
		(pts
			(xy 45.72 134.62) (xy 45.72 138.43)
		)
	)
	(wire
		(pts
			(xy 181.61 149.86) (xy 181.61 132.08)
		)
	)
	(wire
		(pts
			(xy 213.36 138.43) (xy 213.36 134.62)
		)
	)
	(wire
		(pts
			(xy 38.1 21.59) (xy 38.1 31.75)
		)
	)
	(wire
		(pts
			(xy 172.72 144.78) (xy 161.29 144.78)
		)
	)
	(wire
		(pts
			(xy 162.56 134.62) (xy 189.23 134.62)
		)
	)
	(wire
		(pts
			(xy 213.36 86.36) (xy 213.36 92.71)
		)
	)
	(wire
		(pts
			(xy 182.88 130.81) (xy 156.21 130.81)
		)
	)
	(wire
		(pts
			(xy 224.79 146.05) (xy 231.14 146.05)
		)
	)
	(wire
		(pts
			(xy 45.72 73.66) (xy 68.58 73.66)
		)
	)
	(wire
		(pts
			(xy 114.3 146.05) (xy 114.3 138.43)
		)
	)
	(wire
		(pts
			(xy 86.36 68.58) (xy 86.36 96.52)
		)
	)
	(wire
		(pts
			(xy 205.74 68.58) (xy 229.87 68.58)
		)
	)
	(wire
		(pts
			(xy 180.34 146.05) (xy 180.34 133.35)
		)
	)
	(wire
		(pts
			(xy 107.95 72.39) (xy 107.95 92.71)
		)
	)
	(wire
		(pts
			(xy 91.44 85.09) (xy 93.98 85.09)
		)
	)
	(wire
		(pts
			(xy 191.77 92.71) (xy 187.96 92.71)
		)
	)
	(wire
		(pts
			(xy 224.79 86.36) (xy 224.79 88.9)
		)
	)
	(wire
		(pts
			(xy 60.96 92.71) (xy 60.96 100.33)
		)
	)
	(wire
		(pts
			(xy 187.96 85.09) (xy 187.96 92.71)
		)
	)
	(wire
		(pts
			(xy 34.29 146.05) (xy 38.1 146.05)
		)
	)
	(wire
		(pts
			(xy 38.1 158.75) (xy 41.91 158.75)
		)
	)
	(wire
		(pts
			(xy 199.39 92.71) (xy 203.2 92.71)
		)
	)
	(wire
		(pts
			(xy 72.39 69.85) (xy 72.39 88.9)
		)
	)
	(wire
		(pts
			(xy 22.86 73.66) (xy 22.86 85.09)
		)
	)
	(wire
		(pts
			(xy 39.37 31.75) (xy 38.1 31.75)
		)
	)
	(wire
		(pts
			(xy 173.99 88.9) (xy 173.99 90.17)
		)
	)
	(wire
		(pts
			(xy 152.4 72.39) (xy 177.8 72.39)
		)
	)
	(wire
		(pts
			(xy 66.04 91.44) (xy 66.04 96.52)
		)
	)
	(wire
		(pts
			(xy 234.95 68.58) (xy 234.95 132.08)
		)
	)
	(wire
		(pts
			(xy 162.56 146.05) (xy 166.37 146.05)
		)
	)
	(wire
		(pts
			(xy 22.86 134.62) (xy 45.72 134.62)
		)
	)
	(wire
		(pts
			(xy 213.36 92.71) (xy 213.36 100.33)
		)
	)
	(wire
		(pts
			(xy 104.14 90.17) (xy 90.17 90.17)
		)
	)
	(wire
		(pts
			(xy 173.99 142.24) (xy 172.72 142.24)
		)
	)
	(wire
		(pts
			(xy 87.63 158.75) (xy 87.63 149.86)
		)
	)
	(wire
		(pts
			(xy 40.64 77.47) (xy 60.96 77.47)
		)
	)
	(wire
		(pts
			(xy 113.03 96.52) (xy 118.11 96.52)
		)
	)
	(wire
		(pts
			(xy 58.42 85.09) (xy 58.42 88.9)
		)
	)
	(wire
		(pts
			(xy 91.44 134.62) (xy 114.3 134.62)
		)
	)
	(wire
		(pts
			(xy 57.15 138.43) (xy 57.15 142.24)
		)
	)
	(wire
		(pts
			(xy 161.29 149.86) (xy 166.37 149.86)
		)
	)
	(wire
		(pts
			(xy 38.1 133.35) (xy 38.1 146.05)
		)
	)
	(wire
		(pts
			(xy 213.36 73.66) (xy 213.36 86.36)
		)
	)
	(wire
		(pts
			(xy 83.82 158.75) (xy 87.63 158.75)
		)
	)
	(wire
		(pts
			(xy 87.63 132.08) (xy 111.76 132.08)
		)
	)
	(wire
		(pts
			(xy 217.17 80.01) (xy 217.17 88.9)
		)
	)
	(wire
		(pts
			(xy 38.1 133.35) (xy 60.96 133.35)
		)
	)
	(wire
		(pts
			(xy 39.37 64.77) (xy 31.75 64.77)
		)
	)
	(wire
		(pts
			(xy 199.39 96.52) (xy 205.74 96.52)
		)
	)
	(wire
		(pts
			(xy 38.1 146.05) (xy 38.1 153.67)
		)
	)
	(wire
		(pts
			(xy 213.36 146.05) (xy 213.36 138.43)
		)
	)
	(wire
		(pts
			(xy 156.21 142.24) (xy 156.21 130.81)
		)
	)
	(wire
		(pts
			(xy 173.99 138.43) (xy 173.99 142.24)
		)
	)
	(wire
		(pts
			(xy 148.59 138.43) (xy 148.59 142.24)
		)
	)
	(wire
		(pts
			(xy 80.01 96.52) (xy 86.36 96.52)
		)
	)
	(wire
		(pts
			(xy 152.4 92.71) (xy 152.4 100.33)
		)
	)
	(wire
		(pts
			(xy 20.32 144.78) (xy 20.32 149.86)
		)
	)
	(wire
		(pts
			(xy 49.53 69.85) (xy 72.39 69.85)
		)
	)
	(wire
		(pts
			(xy 162.56 92.71) (xy 162.56 100.33)
		)
	)
	(wire
		(pts
			(xy 38.1 100.33) (xy 40.64 100.33)
		)
	)
	(wire
		(pts
			(xy 34.29 92.71) (xy 38.1 92.71)
		)
	)
	(wire
		(pts
			(xy 16.51 130.81) (xy 16.51 142.24)
		)
	)
	(wire
		(pts
			(xy 44.45 158.75) (xy 45.72 158.75)
		)
	)
	(wire
		(pts
			(xy 109.22 146.05) (xy 109.22 133.35)
		)
	)
	(wire
		(pts
			(xy 177.8 158.75) (xy 181.61 158.75)
		)
	)
	(wire
		(pts
			(xy 204.47 158.75) (xy 209.55 158.75)
		)
	)
	(wire
		(pts
			(xy 44.45 88.9) (xy 49.53 88.9)
		)
	)
	(wire
		(pts
			(xy 41.91 149.86) (xy 41.91 132.08)
		)
	)
	(wire
		(pts
			(xy 213.36 153.67) (xy 213.36 146.05)
		)
	)
	(wire
		(pts
			(xy 200.66 85.09) (xy 200.66 88.9)
		)
	)
	(wire
		(pts
			(xy 213.36 45.72) (xy 213.36 73.66)
		)
	)
	(wire
		(pts
			(xy 162.56 138.43) (xy 162.56 134.62)
		)
	)
	(wire
		(pts
			(xy 45.72 73.66) (xy 45.72 85.09)
		)
	)
	(wire
		(pts
			(xy 200.66 138.43) (xy 200.66 142.24)
		)
	)
	(wire
		(pts
			(xy 102.87 92.71) (xy 107.95 92.71)
		)
	)
	(wire
		(pts
			(xy 152.4 105.41) (xy 154.94 105.41)
		)
	)
	(wire
		(pts
			(xy 160.02 96.52) (xy 166.37 96.52)
		)
	)
	(wire
		(pts
			(xy 38.1 92.71) (xy 38.1 100.33)
		)
	)
	(wire
		(pts
			(xy 60.96 158.75) (xy 64.77 158.75)
		)
	)
	(wire
		(pts
			(xy 180.34 68.58) (xy 205.74 68.58)
		)
	)
	(wire
		(pts
			(xy 210.82 96.52) (xy 210.82 105.41)
		)
	)
	(wire
		(pts
			(xy 67.31 158.75) (xy 68.58 158.75)
		)
	)
	(wire
		(pts
			(xy 86.36 146.05) (xy 86.36 133.35)
		)
	)
	(wire
		(pts
			(xy 191.77 76.2) (xy 191.77 88.9)
		)
	)
	(wire
		(pts
			(xy 43.18 96.52) (xy 43.18 105.41)
		)
	)
	(wire
		(pts
			(xy 177.8 72.39) (xy 203.2 72.39)
		)
	)
	(wire
		(pts
			(xy 44.45 105.41) (xy 45.72 105.41)
		)
	)
	(wire
		(pts
			(xy 137.16 134.62) (xy 162.56 134.62)
		)
	)
	(wire
		(pts
			(xy 36.83 133.35) (xy 38.1 133.35)
		)
	)
	(wire
		(pts
			(xy 90.17 96.52) (xy 90.17 105.41)
		)
	)
	(wire
		(pts
			(xy 180.34 96.52) (xy 180.34 105.41)
		)
	)
	(wire
		(pts
			(xy 90.17 149.86) (xy 95.25 149.86)
		)
	)
	(wire
		(pts
			(xy 199.39 144.78) (xy 187.96 144.78)
		)
	)
	(wire
		(pts
			(xy 152.4 72.39) (xy 152.4 92.71)
		)
	)
	(wire
		(pts
			(xy 16.51 69.85) (xy 16.51 88.9)
		)
	)
	(wire
		(pts
			(xy 125.73 146.05) (xy 129.54 146.05)
		)
	)
	(wire
		(pts
			(xy 231.14 146.05) (xy 231.14 133.35)
		)
	)
	(wire
		(pts
			(xy 228.6 105.41) (xy 229.87 105.41)
		)
	)
	(wire
		(pts
			(xy 228.6 92.71) (xy 228.6 100.33)
		)
	)
	(wire
		(pts
			(xy 187.96 85.09) (xy 190.5 85.09)
		)
	)
	(wire
		(pts
			(xy 154.94 68.58) (xy 180.34 68.58)
		)
	)
	(wire
		(pts
			(xy 217.17 92.71) (xy 213.36 92.71)
		)
	)
	(wire
		(pts
			(xy 161.29 149.86) (xy 161.29 158.75)
		)
	)
	(wire
		(pts
			(xy 204.47 153.67) (xy 204.47 146.05)
		)
	)
	(wire
		(pts
			(xy 210.82 105.41) (xy 213.36 105.41)
		)
	)
	(wire
		(pts
			(xy 134.62 105.41) (xy 137.16 105.41)
		)
	)
	(wire
		(pts
			(xy 85.09 142.24) (xy 95.25 142.24)
		)
	)
	(wire
		(pts
			(xy 91.44 92.71) (xy 95.25 92.71)
		)
	)
	(wire
		(pts
			(xy 199.39 142.24) (xy 199.39 144.78)
		)
	)
	(wire
		(pts
			(xy 147.32 142.24) (xy 147.32 144.78)
		)
	)
	(wire
		(pts
			(xy 26.67 149.86) (xy 20.32 149.86)
		)
	)
	(wire
		(pts
			(xy 228.6 158.75) (xy 233.68 158.75)
		)
	)
	(wire
		(pts
			(xy 109.22 133.35) (xy 129.54 133.35)
		)
	)
	(wire
		(pts
			(xy 114.3 138.43) (xy 114.3 134.62)
		)
	)
	(wire
		(pts
			(xy 189.23 134.62) (xy 189.23 138.43)
		)
	)
	(wire
		(pts
			(xy 49.53 69.85) (xy 49.53 88.9)
		)
	)
	(wire
		(pts
			(xy 66.04 96.52) (xy 72.39 96.52)
		)
	)
	(wire
		(pts
			(xy 107.95 72.39) (xy 129.54 72.39)
		)
	)
	(wire
		(pts
			(xy 224.79 96.52) (xy 229.87 96.52)
		)
	)
	(wire
		(pts
			(xy 189.23 134.62) (xy 213.36 134.62)
		)
	)
	(wire
		(pts
			(xy 154.94 96.52) (xy 154.94 105.41)
		)
	)
	(wire
		(pts
			(xy 137.16 73.66) (xy 137.16 85.09)
		)
	)
	(wire
		(pts
			(xy 130.81 142.24) (xy 140.97 142.24)
		)
	)
	(wire
		(pts
			(xy 229.87 68.58) (xy 229.87 96.52)
		)
	)
	(wire
		(pts
			(xy 200.66 146.05) (xy 204.47 146.05)
		)
	)
	(wire
		(pts
			(xy 83.82 153.67) (xy 86.36 153.67)
		)
	)
	(wire
		(pts
			(xy 187.96 73.66) (xy 187.96 85.09)
		)
	)
	(wire
		(pts
			(xy 36.83 31.75) (xy 38.1 31.75)
		)
	)
	(wire
		(pts
			(xy 148.59 92.71) (xy 152.4 92.71)
		)
	)
	(wire
		(pts
			(xy 210.82 91.44) (xy 210.82 96.52)
		)
	)
	(wire
		(pts
			(xy 60.96 146.05) (xy 60.96 133.35)
		)
	)
	(wire
		(pts
			(xy 187.96 73.66) (xy 213.36 73.66)
		)
	)
	(wire
		(pts
			(xy 233.68 132.08) (xy 233.68 149.86)
		)
	)
	(wire
		(pts
			(xy 60.96 153.67) (xy 60.96 146.05)
		)
	)
	(wire
		(pts
			(xy 111.76 132.08) (xy 133.35 132.08)
		)
	)
	(wire
		(pts
			(xy 83.82 72.39) (xy 107.95 72.39)
		)
	)
	(wire
		(pts
			(xy 125.73 96.52) (xy 132.08 96.52)
		)
	)
	(wire
		(pts
			(xy 204.47 146.05) (xy 204.47 133.35)
		)
	)
	(wire
		(pts
			(xy 45.72 85.09) (xy 45.72 92.71)
		)
	)
	(wire
		(pts
			(xy 22.86 92.71) (xy 22.86 100.33)
		)
	)
	(wire
		(pts
			(xy 110.49 96.52) (xy 110.49 105.41)
		)
	)
	(wire
		(pts
			(xy 85.09 130.81) (xy 62.23 130.81)
		)
	)
	(wire
		(pts
			(xy 135.89 144.78) (xy 135.89 149.86)
		)
	)
	(wire
		(pts
			(xy 156.21 142.24) (xy 166.37 142.24)
		)
	)
	(wire
		(pts
			(xy 19.05 73.66) (xy 19.05 134.62)
		)
	)
	(wire
		(pts
			(xy 125.73 138.43) (xy 125.73 142.24)
		)
	)
	(wire
		(pts
			(xy 26.67 96.52) (xy 21.59 96.52)
		)
	)
	(wire
		(pts
			(xy 19.05 134.62) (xy 19.05 138.43)
		)
	)
	(wire
		(pts
			(xy 95.25 146.05) (xy 91.44 146.05)
		)
	)
	(wire
		(pts
			(xy 64.77 149.86) (xy 64.77 132.08)
		)
	)
	(wire
		(pts
			(xy 39.37 54.61) (xy 39.37 64.77)
		)
	)
	(wire
		(pts
			(xy 45.72 92.71) (xy 49.53 92.71)
		)
	)
	(wire
		(pts
			(xy 26.67 43.18) (xy 26.67 45.72)
		)
	)
	(wire
		(pts
			(xy 130.81 130.81) (xy 156.21 130.81)
		)
	)
	(wire
		(pts
			(xy 147.32 144.78) (xy 135.89 144.78)
		)
	)
	(wire
		(pts
			(xy 22.86 73.66) (xy 45.72 73.66)
		)
	)
	(wire
		(pts
			(xy 180.34 68.58) (xy 180.34 96.52)
		)
	)
	(wire
		(pts
			(xy 80.01 142.24) (xy 78.74 142.24)
		)
	)
	(wire
		(pts
			(xy 22.86 146.05) (xy 22.86 153.67)
		)
	)
	(wire
		(pts
			(xy 41.91 158.75) (xy 41.91 149.86)
		)
	)
	(wire
		(pts
			(xy 111.76 158.75) (xy 111.76 149.86)
		)
	)
	(wire
		(pts
			(xy 205.74 68.58) (xy 205.74 96.52)
		)
	)
	(wire
		(pts
			(xy 44.45 149.86) (xy 49.53 149.86)
		)
	)
	(wire
		(pts
			(xy 177.8 72.39) (xy 177.8 92.71)
		)
	)
	(wire
		(pts
			(xy 129.54 92.71) (xy 129.54 100.33)
		)
	)
	(wire
		(pts
			(xy 41.91 96.52) (xy 41.91 105.41)
		)
	)
	(wire
		(pts
			(xy 80.01 149.86) (xy 87.63 149.86)
		)
	)
	(wire
		(pts
			(xy 129.54 72.39) (xy 129.54 92.71)
		)
	)
	(wire
		(pts
			(xy 68.58 92.71) (xy 68.58 100.33)
		)
	)
	(wire
		(pts
			(xy 185.42 96.52) (xy 185.42 105.41)
		)
	)
	(wire
		(pts
			(xy 152.4 133.35) (xy 152.4 146.05)
		)
	)
	(wire
		(pts
			(xy 162.56 73.66) (xy 187.96 73.66)
		)
	)
	(wire
		(pts
			(xy 60.96 77.47) (xy 60.96 92.71)
		)
	)
	(wire
		(pts
			(xy 134.62 96.52) (xy 140.97 96.52)
		)
	)
	(wire
		(pts
			(xy 45.72 92.71) (xy 45.72 100.33)
		)
	)
	(wire
		(pts
			(xy 125.73 92.71) (xy 129.54 92.71)
		)
	)
	(wire
		(pts
			(xy 152.4 133.35) (xy 180.34 133.35)
		)
	)
	(wire
		(pts
			(xy 125.73 88.9) (xy 125.73 91.44)
		)
	)
	(wire
		(pts
			(xy 91.44 85.09) (xy 91.44 92.71)
		)
	)
	(wire
		(pts
			(xy 68.58 86.36) (xy 71.12 86.36)
		)
	)
	(wire
		(pts
			(xy 129.54 146.05) (xy 129.54 133.35)
		)
	)
	(wire
		(pts
			(xy 87.63 149.86) (xy 87.63 132.08)
		)
	)
	(wire
		(pts
			(xy 160.02 90.17) (xy 160.02 96.52)
		)
	)
	(wire
		(pts
			(xy 16.51 142.24) (xy 26.67 142.24)
		)
	)
	(wire
		(pts
			(xy 218.44 80.01) (xy 218.44 76.2)
		)
	)
	(wire
		(pts
			(xy 187.96 92.71) (xy 187.96 100.33)
		)
	)
	(wire
		(pts
			(xy 152.4 146.05) (xy 152.4 153.67)
		)
	)
	(wire
		(pts
			(xy 67.31 21.59) (xy 67.31 67.31)
		)
	)
	(wire
		(pts
			(xy 60.96 105.41) (xy 63.5 105.41)
		)
	)
	(wire
		(pts
			(xy 22.86 146.05) (xy 26.67 146.05)
		)
	)
	(wire
		(pts
			(xy 160.02 105.41) (xy 162.56 105.41)
		)
	)
	(wire
		(pts
			(xy 132.08 68.58) (xy 132.08 96.52)
		)
	)
	(wire
		(pts
			(xy 34.29 96.52) (xy 41.91 96.52)
		)
	)
	(wire
		(pts
			(xy 129.54 133.35) (xy 152.4 133.35)
		)
	)
	(wire
		(pts
			(xy 199.39 88.9) (xy 199.39 90.17)
		)
	)
	(wire
		(pts
			(xy 182.88 142.24) (xy 193.04 142.24)
		)
	)
	(wire
		(pts
			(xy 228.6 85.09) (xy 232.41 85.09)
		)
	)
	(wire
		(pts
			(xy 43.18 96.52) (xy 49.53 96.52)
		)
	)
	(wire
		(pts
			(xy 125.73 149.86) (xy 133.35 149.86)
		)
	)
	(wire
		(pts
			(xy 113.03 158.75) (xy 114.3 158.75)
		)
	)
	(wire
		(pts
			(xy 187.96 144.78) (xy 187.96 149.86)
		)
	)
	(wire
		(pts
			(xy 20.32 158.75) (xy 22.86 158.75)
		)
	)
	(wire
		(pts
			(xy 68.58 73.66) (xy 68.58 86.36)
		)
	)
	(wire
		(pts
			(xy 24.13 138.43) (xy 19.05 138.43)
		)
	)
	(wire
		(pts
			(xy 16.51 88.9) (xy 26.67 88.9)
		)
	)
	(wire
		(pts
			(xy 182.88 142.24) (xy 182.88 130.81)
		)
	)
	(wire
		(pts
			(xy 31.75 21.59) (xy 31.75 22.86)
		)
	)
	(wire
		(pts
			(xy 207.01 142.24) (xy 207.01 130.81)
		)
	)
	(wire
		(pts
			(xy 90.17 149.86) (xy 90.17 158.75)
		)
	)
	(wire
		(pts
			(xy 224.79 138.43) (xy 224.79 142.24)
		)
	)
	(wire
		(pts
			(xy 64.77 158.75) (xy 64.77 149.86)
		)
	)
	(wire
		(pts
			(xy 161.29 158.75) (xy 162.56 158.75)
		)
	)
	(wire
		(pts
			(xy 107.95 142.24) (xy 107.95 130.81)
		)
	)
	(wire
		(pts
			(xy 72.39 92.71) (xy 68.58 92.71)
		)
	)
	(wire
		(pts
			(xy 39.37 35.56) (xy 39.37 43.18)
		)
	)
	(wire
		(pts
			(xy 34.29 142.24) (xy 33.02 142.24)
		)
	)
	(wire
		(pts
			(xy 200.66 142.24) (xy 199.39 142.24)
		)
	)
	(wire
		(pts
			(xy 113.03 105.41) (xy 114.3 105.41)
		)
	)
	(wire
		(pts
			(xy 40.64 100.33) (xy 40.64 77.47)
		)
	)
	(wire
		(pts
			(xy 21.59 58.42) (xy 234.95 58.42)
		)
	)
	(wire
		(pts
			(xy 55.88 144.78) (xy 44.45 144.78)
		)
	)
	(wire
		(pts
			(xy 102.87 96.52) (xy 110.49 96.52)
		)
	)
	(wire
		(pts
			(xy 231.14 153.67) (xy 231.14 146.05)
		)
	)
	(wire
		(pts
			(xy 39.37 43.18) (xy 36.83 43.18)
		)
	)
	(wire
		(pts
			(xy 34.29 149.86) (xy 41.91 149.86)
		)
	)
	(wire
		(pts
			(xy 60.96 77.47) (xy 60.96 72.39)
		)
	)
	(wire
		(pts
			(xy 16.51 69.85) (xy 49.53 69.85)
		)
	)
	(wire
		(pts
			(xy 38.1 21.59) (xy 49.53 21.59)
		)
	)
	(wire
		(pts
			(xy 64.77 132.08) (xy 87.63 132.08)
		)
	)
	(wire
		(pts
			(xy 111.76 149.86) (xy 111.76 132.08)
		)
	)
	(wire
		(pts
			(xy 110.49 68.58) (xy 110.49 96.52)
		)
	)
	(wire
		(pts
			(xy 22.86 85.09) (xy 22.86 92.71)
		)
	)
	(wire
		(pts
			(xy 114.3 153.67) (xy 114.3 146.05)
		)
	)
	(wire
		(pts
			(xy 80.01 88.9) (xy 80.01 91.44)
		)
	)
	(wire
		(pts
			(xy 67.31 149.86) (xy 67.31 158.75)
		)
	)
	(wire
		(pts
			(xy 36.83 132.08) (xy 41.91 132.08)
		)
	)
	(wire
		(pts
			(xy 80.01 91.44) (xy 66.04 91.44)
		)
	)
	(wire
		(pts
			(xy 229.87 96.52) (xy 229.87 105.41)
		)
	)
	(wire
		(pts
			(xy 210.82 96.52) (xy 217.17 96.52)
		)
	)
	(wire
		(pts
			(xy 78.74 144.78) (xy 67.31 144.78)
		)
	)
	(wire
		(pts
			(xy 224.79 92.71) (xy 228.6 92.71)
		)
	)
	(wire
		(pts
			(xy 68.58 138.43) (xy 69.85 138.43)
		)
	)
	(wire
		(pts
			(xy 191.77 76.2) (xy 218.44 76.2)
		)
	)
	(wire
		(pts
			(xy 149.86 85.09) (xy 149.86 88.9)
		)
	)
	(wire
		(pts
			(xy 91.44 138.43) (xy 91.44 134.62)
		)
	)
	(wire
		(pts
			(xy 67.31 149.86) (xy 72.39 149.86)
		)
	)
	(wire
		(pts
			(xy 90.17 96.52) (xy 95.25 96.52)
		)
	)
	(wire
		(pts
			(xy 68.58 134.62) (xy 91.44 134.62)
		)
	)
	(wire
		(pts
			(xy 26.67 50.8) (xy 26.67 54.61)
		)
	)
	(wire
		(pts
			(xy 114.3 134.62) (xy 137.16 134.62)
		)
	)
	(wire
		(pts
			(xy 149.86 88.9) (xy 148.59 88.9)
		)
	)
	(wire
		(pts
			(xy 110.49 68.58) (xy 132.08 68.58)
		)
	)
	(wire
		(pts
			(xy 30.48 21.59) (xy 31.75 21.59)
		)
	)
	(wire
		(pts
			(xy 162.56 85.09) (xy 162.56 92.71)
		)
	)
	(wire
		(pts
			(xy 22.86 134.62) (xy 22.86 146.05)
		)
	)
	(wire
		(pts
			(xy 137.16 138.43) (xy 138.43 138.43)
		)
	)
	(wire
		(pts
			(xy 90.17 144.78) (xy 90.17 149.86)
		)
	)
	(wire
		(pts
			(xy 125.73 91.44) (xy 113.03 91.44)
		)
	)
	(wire
		(pts
			(xy 68.58 134.62) (xy 68.58 138.43)
		)
	)
	(wire
		(pts
			(xy 80.01 92.71) (xy 83.82 92.71)
		)
	)
	(wire
		(pts
			(xy 140.97 149.86) (xy 135.89 149.86)
		)
	)
	(wire
		(pts
			(xy 137.16 85.09) (xy 139.7 85.09)
		)
	)
	(wire
		(pts
			(xy 43.18 68.58) (xy 43.18 96.52)
		)
	)
	(wire
		(pts
			(xy 83.82 105.41) (xy 86.36 105.41)
		)
	)
	(wire
		(pts
			(xy 148.59 88.9) (xy 148.59 90.17)
		)
	)
	(wire
		(pts
			(xy 133.35 158.75) (xy 133.35 149.86)
		)
	)
	(wire
		(pts
			(xy 85.09 142.24) (xy 85.09 130.81)
		)
	)
	(wire
		(pts
			(xy 224.79 88.9) (xy 224.79 91.44)
		)
	)
	(wire
		(pts
			(xy 19.05 73.66) (xy 22.86 73.66)
		)
	)
	(wire
		(pts
			(xy 233.68 132.08) (xy 234.95 132.08)
		)
	)
	(wire
		(pts
			(xy 132.08 68.58) (xy 154.94 68.58)
		)
	)
	(wire
		(pts
			(xy 133.35 149.86) (xy 133.35 132.08)
		)
	)
	(wire
		(pts
			(xy 203.2 105.41) (xy 205.74 105.41)
		)
	)
	(wire
		(pts
			(xy 67.31 144.78) (xy 67.31 149.86)
		)
	)
	(wire
		(pts
			(xy 62.23 130.81) (xy 39.37 130.81)
		)
	)
	(wire
		(pts
			(xy 113.03 144.78) (xy 113.03 149.86)
		)
	)
	(wire
		(pts
			(xy 43.18 68.58) (xy 63.5 68.58)
		)
	)
	(wire
		(pts
			(xy 26.67 54.61) (xy 26.67 57.15)
		)
	)
	(wire
		(pts
			(xy 113.03 91.44) (xy 113.03 96.52)
		)
	)
	(wire
		(pts
			(xy 68.58 138.43) (xy 68.58 146.05)
		)
	)
	(wire
		(pts
			(xy 16.51 21.59) (xy 16.51 69.85)
		)
	)
	(wire
		(pts
			(xy 66.04 96.52) (xy 66.04 105.41)
		)
	)
	(wire
		(pts
			(xy 127 88.9) (xy 125.73 88.9)
		)
	)
	(wire
		(pts
			(xy 148.59 96.52) (xy 154.94 96.52)
		)
	)
	(wire
		(pts
			(xy 129.54 158.75) (xy 133.35 158.75)
		)
	)
	(wire
		(pts
			(xy 118.11 69.85) (xy 140.97 69.85)
		)
	)
	(wire
		(pts
			(xy 205.74 96.52) (xy 205.74 105.41)
		)
	)
	(wire
		(pts
			(xy 72.39 69.85) (xy 95.25 69.85)
		)
	)
	(wire
		(pts
			(xy 39.37 142.24) (xy 39.37 130.81)
		)
	)
	(wire
		(pts
			(xy 106.68 153.67) (xy 109.22 153.67)
		)
	)
	(wire
		(pts
			(xy 44.45 149.86) (xy 44.45 158.75)
		)
	)
	(wire
		(pts
			(xy 203.2 92.71) (xy 203.2 100.33)
		)
	)
	(wire
		(pts
			(xy 25.4 21.59) (xy 16.51 21.59)
		)
	)
	(wire
		(pts
			(xy 114.3 92.71) (xy 114.3 100.33)
		)
	)
	(wire
		(pts
			(xy 40.64 68.58) (xy 43.18 68.58)
		)
	)
	(wire
		(pts
			(xy 80.01 138.43) (xy 80.01 142.24)
		)
	)
	(wire
		(pts
			(xy 68.58 146.05) (xy 68.58 153.67)
		)
	)
	(wire
		(pts
			(xy 34.29 138.43) (xy 34.29 142.24)
		)
	)
	(wire
		(pts
			(xy 180.34 133.35) (xy 204.47 133.35)
		)
	)
	(wire
		(pts
			(xy 91.44 146.05) (xy 91.44 153.67)
		)
	)
	(wire
		(pts
			(xy 60.96 133.35) (xy 86.36 133.35)
		)
	)
	(wire
		(pts
			(xy 102.87 149.86) (xy 111.76 149.86)
		)
	)
	(wire
		(pts
			(xy 133.35 132.08) (xy 154.94 132.08)
		)
	)
	(wire
		(pts
			(xy 154.94 158.75) (xy 154.94 149.86)
		)
	)
	(wire
		(pts
			(xy 19.05 134.62) (xy 22.86 134.62)
		)
	)
	(wire
		(pts
			(xy 189.23 146.05) (xy 193.04 146.05)
		)
	)
	(wire
		(pts
			(xy 229.87 68.58) (xy 234.95 68.58)
		)
	)
	(wire
		(pts
			(xy 224.79 91.44) (xy 210.82 91.44)
		)
	)
	(wire
		(pts
			(xy 102.87 142.24) (xy 101.6 142.24)
		)
	)
	(wire
		(pts
			(xy 137.16 146.05) (xy 137.16 153.67)
		)
	)
	(wire
		(pts
			(xy 137.16 92.71) (xy 137.16 100.33)
		)
	)
	(wire
		(pts
			(xy 173.99 146.05) (xy 180.34 146.05)
		)
	)
	(wire
		(pts
			(xy 91.44 73.66) (xy 91.44 85.09)
		)
	)
	(wire
		(pts
			(xy 172.72 142.24) (xy 172.72 144.78)
		)
	)
	(wire
		(pts
			(xy 166.37 69.85) (xy 191.77 69.85)
		)
	)
	(wire
		(pts
			(xy 45.72 134.62) (xy 68.58 134.62)
		)
	)
	(wire
		(pts
			(xy 33.02 88.9) (xy 33.02 91.44)
		)
	)
	(wire
		(pts
			(xy 173.99 96.52) (xy 180.34 96.52)
		)
	)
	(wire
		(pts
			(xy 204.47 133.35) (xy 231.14 133.35)
		)
	)
	(wire
		(pts
			(xy 203.2 72.39) (xy 228.6 72.39)
		)
	)
	(wire
		(pts
			(xy 173.99 149.86) (xy 181.61 149.86)
		)
	)
	(wire
		(pts
			(xy 224.79 149.86) (xy 233.68 149.86)
		)
	)
	(wire
		(pts
			(xy 45.72 138.43) (xy 46.99 138.43)
		)
	)
	(wire
		(pts
			(xy 91.44 92.71) (xy 91.44 100.33)
		)
	)
	(wire
		(pts
			(xy 62.23 142.24) (xy 62.23 130.81)
		)
	)
	(wire
		(pts
			(xy 162.56 92.71) (xy 166.37 92.71)
		)
	)
	(wire
		(pts
			(xy 106.68 158.75) (xy 111.76 158.75)
		)
	)
	(wire
		(pts
			(xy 127 86.36) (xy 127 88.9)
		)
	)
	(wire
		(pts
			(xy 60.96 72.39) (xy 83.82 72.39)
		)
	)
	(wire
		(pts
			(xy 39.37 43.18) (xy 39.37 54.61)
		)
	)
	(wire
		(pts
			(xy 101.6 142.24) (xy 101.6 144.78)
		)
	)
	(wire
		(pts
			(xy 212.09 149.86) (xy 217.17 149.86)
		)
	)
	(wire
		(pts
			(xy 209.55 158.75) (xy 209.55 149.86)
		)
	)
	(wire
		(pts
			(xy 166.37 69.85) (xy 166.37 88.9)
		)
	)
	(wire
		(pts
			(xy 68.58 86.36) (xy 68.58 92.71)
		)
	)
	(wire
		(pts
			(xy 114.3 73.66) (xy 137.16 73.66)
		)
	)
	(wire
		(pts
			(xy 162.56 138.43) (xy 163.83 138.43)
		)
	)
	(wire
		(pts
			(xy 161.29 144.78) (xy 161.29 149.86)
		)
	)
	(wire
		(pts
			(xy 114.3 146.05) (xy 118.11 146.05)
		)
	)
	(wire
		(pts
			(xy 102.87 146.05) (xy 109.22 146.05)
		)
	)
	(wire
		(pts
			(xy 45.72 85.09) (xy 48.26 85.09)
		)
	)
	(wire
		(pts
			(xy 113.03 149.86) (xy 113.03 158.75)
		)
	)
	(wire
		(pts
			(xy 90.17 158.75) (xy 91.44 158.75)
		)
	)
	(wire
		(pts
			(xy 39.37 142.24) (xy 49.53 142.24)
		)
	)
	(wire
		(pts
			(xy 34.29 88.9) (xy 33.02 88.9)
		)
	)
	(wire
		(pts
			(xy 83.82 92.71) (xy 83.82 100.33)
		)
	)
	(wire
		(pts
			(xy 137.16 92.71) (xy 140.97 92.71)
		)
	)
	(wire
		(pts
			(xy 137.16 138.43) (xy 137.16 146.05)
		)
	)
	(wire
		(pts
			(xy 63.5 96.52) (xy 63.5 105.41)
		)
	)
	(wire
		(pts
			(xy 134.62 90.17) (xy 134.62 96.52)
		)
	)
	(wire
		(pts
			(xy 41.91 105.41) (xy 43.18 105.41)
		)
	)
	(wire
		(pts
			(xy 185.42 90.17) (xy 185.42 96.52)
		)
	)
	(wire
		(pts
			(xy 207.01 130.81) (xy 182.88 130.81)
		)
	)
	(wire
		(pts
			(xy 21.59 96.52) (xy 21.59 105.41)
		)
	)
	(wire
		(pts
			(xy 22.86 85.09) (xy 24.13 85.09)
		)
	)
	(wire
		(pts
			(xy 102.87 138.43) (xy 102.87 142.24)
		)
	)
	(wire
		(pts
			(xy 38.1 105.41) (xy 41.91 105.41)
		)
	)
	(wire
		(pts
			(xy 80.01 146.05) (xy 86.36 146.05)
		)
	)
	(wire
		(pts
			(xy 90.17 105.41) (xy 91.44 105.41)
		)
	)
	(wire
		(pts
			(xy 80.01 86.36) (xy 80.01 88.9)
		)
	)
	(wire
		(pts
			(xy 91.44 133.35) (xy 109.22 133.35)
		)
	)
	(wire
		(pts
			(xy 124.46 144.78) (xy 113.03 144.78)
		)
	)
	(wire
		(pts
			(xy 209.55 149.86) (xy 209.55 132.08)
		)
	)
	(wire
		(pts
			(xy 34.29 85.09) (xy 34.29 88.9)
		)
	)
	(wire
		(pts
			(xy 57.15 149.86) (xy 64.77 149.86)
		)
	)
	(wire
		(pts
			(xy 86.36 133.35) (xy 91.44 133.35)
		)
	)
	(wire
		(pts
			(xy 137.16 134.62) (xy 137.16 138.43)
		)
	)
	(wire
		(pts
			(xy 185.42 96.52) (xy 191.77 96.52)
		)
	)
	(wire
		(pts
			(xy 177.8 105.41) (xy 180.34 105.41)
		)
	)
	(wire
		(pts
			(xy 124.46 142.24) (xy 124.46 144.78)
		)
	)
	(wire
		(pts
			(xy 137.16 85.09) (xy 137.16 92.71)
		)
	)
	(wire
		(pts
			(xy 187.96 158.75) (xy 189.23 158.75)
		)
	)
	(wire
		(pts
			(xy 55.88 142.24) (xy 55.88 144.78)
		)
	)
	(wire
		(pts
			(xy 106.68 105.41) (xy 110.49 105.41)
		)
	)
	(wire
		(pts
			(xy 95.25 69.85) (xy 95.25 88.9)
		)
	)
	(wire
		(pts
			(xy 233.68 149.86) (xy 233.68 158.75)
		)
	)
	(wire
		(pts
			(xy 104.14 88.9) (xy 102.87 88.9)
		)
	)
	(wire
		(pts
			(xy 224.79 142.24) (xy 223.52 142.24)
		)
	)
	(wire
		(pts
			(xy 223.52 142.24) (xy 223.52 144.78)
		)
	)
	(wire
		(pts
			(xy 162.56 85.09) (xy 163.83 85.09)
		)
	)
	(wire
		(pts
			(xy 19.05 67.31) (xy 19.05 73.66)
		)
	)
	(wire
		(pts
			(xy 57.15 96.52) (xy 63.5 96.52)
		)
	)
	(wire
		(pts
			(xy 137.16 73.66) (xy 162.56 73.66)
		)
	)
	(wire
		(pts
			(xy 114.3 73.66) (xy 114.3 86.36)
		)
	)
	(wire
		(pts
			(xy 62.23 142.24) (xy 72.39 142.24)
		)
	)
	(wire
		(pts
			(xy 212.09 149.86) (xy 212.09 158.75)
		)
	)
	(wire
		(pts
			(xy 177.8 92.71) (xy 177.8 100.33)
		)
	)
	(wire
		(pts
			(xy 57.15 142.24) (xy 55.88 142.24)
		)
	)
	(wire
		(pts
			(xy 44.45 88.9) (xy 44.45 105.41)
		)
	)
	(wire
		(pts
			(xy 228.6 165.1) (xy 229.87 165.1)
		)
	)
	(wire
		(pts
			(xy 132.08 96.52) (xy 132.08 105.41)
		)
	)
	(wire
		(pts
			(xy 152.4 158.75) (xy 154.94 158.75)
		)
	)
	(wire
		(pts
			(xy 154.94 132.08) (xy 181.61 132.08)
		)
	)
	(wire
		(pts
			(xy 181.61 158.75) (xy 181.61 149.86)
		)
	)
	(wire
		(pts
			(xy 91.44 73.66) (xy 114.3 73.66)
		)
	)
	(wire
		(pts
			(xy 91.44 133.35) (xy 91.44 134.62)
		)
	)
	(wire
		(pts
			(xy 101.6 144.78) (xy 90.17 144.78)
		)
	)
	(wire
		(pts
			(xy 33.02 142.24) (xy 33.02 144.78)
		)
	)
	(wire
		(pts
			(xy 218.44 80.01) (xy 217.17 80.01)
		)
	)
	(wire
		(pts
			(xy 187.96 149.86) (xy 187.96 158.75)
		)
	)
	(wire
		(pts
			(xy 33.02 144.78) (xy 20.32 144.78)
		)
	)
	(wire
		(pts
			(xy 148.59 90.17) (xy 134.62 90.17)
		)
	)
	(wire
		(pts
			(xy 20.32 149.86) (xy 20.32 158.75)
		)
	)
	(wire
		(pts
			(xy 31.75 21.59) (xy 33.02 21.59)
		)
	)
	(wire
		(pts
			(xy 57.15 88.9) (xy 58.42 88.9)
		)
	)
	(wire
		(pts
			(xy 68.58 146.05) (xy 72.39 146.05)
		)
	)
	(wire
		(pts
			(xy 200.66 149.86) (xy 209.55 149.86)
		)
	)
	(wire
		(pts
			(xy 109.22 153.67) (xy 109.22 146.05)
		)
	)
	(wire
		(pts
			(xy 200.66 88.9) (xy 199.39 88.9)
		)
	)
	(wire
		(pts
			(xy 63.5 68.58) (xy 86.36 68.58)
		)
	)
	(wire
		(pts
			(xy 86.36 68.58) (xy 110.49 68.58)
		)
	)
	(wire
		(pts
			(xy 26.67 92.71) (xy 22.86 92.71)
		)
	)
	(wire
		(pts
			(xy 213.36 146.05) (xy 217.17 146.05)
		)
	)
	(wire
		(pts
			(xy 162.56 73.66) (xy 162.56 85.09)
		)
	)
	(wire
		(pts
			(xy 189.23 138.43) (xy 190.5 138.43)
		)
	)
	(wire
		(pts
			(xy 213.36 45.72) (xy 26.67 45.72)
		)
	)
	(wire
		(pts
			(xy 213.36 134.62) (xy 222.25 134.62)
		)
	)
	(wire
		(pts
			(xy 55.88 21.59) (xy 67.31 21.59)
		)
	)
	(wire
		(pts
			(xy 212.09 158.75) (xy 213.36 158.75)
		)
	)
	(wire
		(pts
			(xy 107.95 130.81) (xy 130.81 130.81)
		)
	)
	(wire
		(pts
			(xy 67.31 67.31) (xy 19.05 67.31)
		)
	)
	(wire
		(pts
			(xy 91.44 138.43) (xy 91.44 146.05)
		)
	)
	(wire
		(pts
			(xy 16.51 88.9) (xy 16.51 130.81)
		)
	)
	(wire
		(pts
			(xy 231.14 133.35) (xy 232.41 133.35)
		)
	)
	(wire
		(pts
			(xy 44.45 144.78) (xy 44.45 149.86)
		)
	)
	(wire
		(pts
			(xy 114.3 86.36) (xy 114.3 92.71)
		)
	)
	(wire
		(pts
			(xy 135.89 158.75) (xy 137.16 158.75)
		)
	)
	(wire
		(pts
			(xy 95.25 69.85) (xy 118.11 69.85)
		)
	)
	(wire
		(pts
			(xy 129.54 72.39) (xy 152.4 72.39)
		)
	)
	(wire
		(pts
			(xy 39.37 54.61) (xy 31.75 54.61)
		)
	)
	(wire
		(pts
			(xy 114.3 138.43) (xy 115.57 138.43)
		)
	)
	(wire
		(pts
			(xy 106.68 100.33) (xy 107.95 100.33)
		)
	)
	(wire
		(pts
			(xy 199.39 90.17) (xy 185.42 90.17)
		)
	)
	(wire
		(pts
			(xy 31.75 27.94) (xy 31.75 31.75)
		)
	)
	(wire
		(pts
			(xy 173.99 92.71) (xy 177.8 92.71)
		)
	)
	(wire
		(pts
			(xy 148.59 146.05) (xy 152.4 146.05)
		)
	)
	(wire
		(pts
			(xy 228.6 85.09) (xy 228.6 92.71)
		)
	)
	(wire
		(pts
			(xy 140.97 146.05) (xy 137.16 146.05)
		)
	)
	(wire
		(pts
			(xy 104.14 85.09) (xy 104.14 88.9)
		)
	)
	(wire
		(pts
			(xy 213.36 138.43) (xy 214.63 138.43)
		)
	)
	(wire
		(pts
			(xy 191.77 76.2) (xy 191.77 69.85)
		)
	)
	(wire
		(pts
			(xy 203.2 72.39) (xy 203.2 92.71)
		)
	)
	(wire
		(pts
			(xy 39.37 35.56) (xy 39.37 31.75)
		)
	)
	(wire
		(pts
			(xy 45.72 146.05) (xy 45.72 153.67)
		)
	)
	(wire
		(pts
			(xy 83.82 72.39) (xy 83.82 92.71)
		)
	)
	(wire
		(pts
			(xy 140.97 69.85) (xy 166.37 69.85)
		)
	)
	(wire
		(pts
			(xy 209.55 132.08) (xy 233.68 132.08)
		)
	)
	(wire
		(pts
			(xy 213.36 86.36) (xy 214.63 86.36)
		)
	)
	(wire
		(pts
			(xy 78.74 142.24) (xy 78.74 144.78)
		)
	)
	(wire
		(pts
			(xy 129.54 153.67) (xy 129.54 146.05)
		)
	)
	(wire
		(pts
			(xy 228.6 153.67) (xy 231.14 153.67)
		)
	)
	(wire
		(pts
			(xy 173.99 85.09) (xy 173.99 88.9)
		)
	)
	(wire
		(pts
			(xy 107.95 92.71) (xy 107.95 100.33)
		)
	)
	(wire
		(pts
			(xy 173.99 90.17) (xy 160.02 90.17)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 30.48 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D5"
			(at 30.48 86.36 0)
		)
		(property "Value" "1N4006"
			(at 30.48 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 30.48 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 30.48 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 30.48 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 30.48 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 30.48 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 53.34 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D6"
			(at 53.34 86.36 0)
		)
		(property "Value" "1N4006"
			(at 53.34 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 53.34 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 53.34 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 53.34 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 53.34 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 53.34 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 170.18 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D20"
			(at 170.18 82.55 0)
		)
		(property "Value" "1N4148"
			(at 170.18 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 170.18 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 170.18 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 170.18 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 170.18 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 170.18 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 121.92 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D14"
			(at 121.92 82.55 0)
		)
		(property "Value" "1N4148"
			(at 121.92 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 121.92 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 121.92 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 121.92 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 121.92 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 121.92 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 196.85 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D48"
			(at 196.85 139.7 0)
		)
		(property "Value" "1N4006"
			(at 196.85 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 196.85 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 196.85 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 196.85 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 196.85 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 196.85 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D48")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 99.06 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U13"
			(at 99.7586 181.61 0)
		)
		(property "Value" "~"
			(at 97.2186 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 99.06 194.31 0)
		)
		(property "Datasheet" ""
			(at 99.06 194.31 0)
		)
		(property "Description" ""
			(at 99.06 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 195.58 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D23"
			(at 195.58 82.55 0)
		)
		(property "Value" "1N4148"
			(at 195.58 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 195.58 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 195.58 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 195.58 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 195.58 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 195.58 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D23")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 26.67 48.26 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 29.21 48.2599 0)
		)
		(property "Value" "R_Small"
			(at 24.13 46.9901 0)
		)
		(property "Footprint" ""
			(at 26.67 48.26 0)
		)
		(property "Datasheet" "~"
			(at 26.67 48.26 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 26.67 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 219.71 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW18"
			(at 219.71 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 219.71 133.35 0)
		)
		(property "Footprint" ""
			(at 219.71 133.35 0)
		)
		(property "Datasheet" "~"
			(at 219.71 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 219.71 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 144.78 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D19"
			(at 144.78 90.17 0)
		)
		(property "Value" "1N4006"
			(at 144.78 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 144.78 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 144.78 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 144.78 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 144.78 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 144.78 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 144.78 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D43"
			(at 144.78 143.51 0)
		)
		(property "Value" "1N4006"
			(at 144.78 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 144.78 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 144.78 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 144.78 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 144.78 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 144.78 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D43")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 143.51 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW15"
			(at 143.51 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 143.51 133.35 0)
		)
		(property "Footprint" ""
			(at 143.51 133.35 0)
		)
		(property "Datasheet" "~"
			(at 143.51 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 143.51 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 195.58 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW17"
			(at 195.58 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 195.58 133.35 0)
		)
		(property "Footprint" ""
			(at 195.58 133.35 0)
		)
		(property "Datasheet" "~"
			(at 195.58 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 195.58 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 195.58 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U8"
			(at 196.2786 128.27 0)
		)
		(property "Value" "~"
			(at 193.7386 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 195.58 140.97 0)
		)
		(property "Datasheet" ""
			(at 195.58 140.97 0)
		)
		(property "Description" ""
			(at 195.58 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 196.85 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D47"
			(at 196.85 135.89 0)
		)
		(property "Value" "1N4148"
			(at 196.85 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 196.85 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 196.85 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 196.85 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 196.85 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 196.85 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D47")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 195.58 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW8"
			(at 195.58 77.47 0)
		)
		(property "Value" "SW_Push"
			(at 195.58 80.01 0)
		)
		(property "Footprint" ""
			(at 195.58 80.01 0)
		)
		(property "Datasheet" "~"
			(at 195.58 80.01 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 195.58 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 220.98 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D54"
			(at 220.98 139.7 0)
		)
		(property "Value" "1N4006"
			(at 220.98 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 220.98 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 220.98 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 220.98 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 220.98 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 220.98 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D54")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 76.2 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D10"
			(at 76.2 90.17 0)
		)
		(property "Value" "1N4006"
			(at 76.2 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 76.2 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 76.2 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 76.2 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 76.2 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 76.2 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 30.48 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U10"
			(at 31.1786 181.61 0)
		)
		(property "Value" "~"
			(at 28.6386 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 30.48 194.31 0)
		)
		(property "Datasheet" ""
			(at 30.48 194.31 0)
		)
		(property "Description" ""
			(at 30.48 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 99.06 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D12"
			(at 99.06 86.36 0)
		)
		(property "Value" "1N4006"
			(at 99.06 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 99.06 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 99.06 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 99.06 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 99.06 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 99.06 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 220.98 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D50"
			(at 220.98 82.55 0)
		)
		(property "Value" "1N4148"
			(at 220.98 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 220.98 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 220.98 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 220.98 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 220.98 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 220.98 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D50")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 99.06 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D35"
			(at 99.06 135.89 0)
		)
		(property "Value" "1N4148"
			(at 99.06 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 99.06 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 99.06 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 99.06 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 99.06 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 99.06 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D35")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 220.98 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D53"
			(at 220.98 135.89 0)
		)
		(property "Value" "1N4148"
			(at 220.98 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 220.98 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 220.98 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 220.98 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 220.98 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 220.98 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D53")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 76.2 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U4"
			(at 76.8986 128.27 0)
		)
		(property "Value" "~"
			(at 74.3586 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 76.2 140.97 0)
		)
		(property "Datasheet" ""
			(at 76.2 140.97 0)
		)
		(property "Description" ""
			(at 76.2 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 35.56 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 35.56 29.21 0)
		)
		(property "Value" "1N4148"
			(at 35.56 31.75 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 35.56 35.56 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 35.56 35.56 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 35.56 35.56 0)
		)
		(property "Sim.Device" "D"
			(at 35.56 35.56 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 35.56 35.56 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 121.92 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 122.6186 128.27 0)
		)
		(property "Value" "~"
			(at 120.0786 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 121.92 140.97 0)
		)
		(property "Datasheet" ""
			(at 121.92 140.97 0)
		)
		(property "Description" ""
			(at 121.92 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 30.48 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D27"
			(at 30.48 139.7 0)
		)
		(property "Value" "1N4006"
			(at 30.48 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 30.48 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 30.48 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 30.48 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 30.48 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 30.48 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D27")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 53.34 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D30"
			(at 53.34 139.7 0)
		)
		(property "Value" "1N4006"
			(at 53.34 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 53.34 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 53.34 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 53.34 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 53.34 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 53.34 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D30")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 144.78 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D42"
			(at 144.78 139.7 0)
		)
		(property "Value" "1N4006"
			(at 144.78 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 144.78 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 144.78 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 144.78 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 144.78 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 144.78 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D42")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Polarized_Small")
		(at 31.75 25.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 34.29 24.8538 0)
		)
		(property "Value" "C_Polarized_Small"
			(at 27.94 24.8539 90)
		)
		(property "Footprint" ""
			(at 31.75 25.4 0)
		)
		(property "Datasheet" "~"
			(at 31.75 25.4 0)
		)
		(property "Description" "Polarized capacitor, small symbol"
			(at 31.75 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 76.2 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D32"
			(at 76.2 135.89 0)
		)
		(property "Value" "1N4148"
			(at 76.2 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 76.2 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 76.2 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 76.2 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 76.2 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 76.2 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D32")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 220.98 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D51"
			(at 220.98 86.36 0)
		)
		(property "Value" "1N4006"
			(at 220.98 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 220.98 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 220.98 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 220.98 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 220.98 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 220.98 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D51")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_BJT:BD139")
		(at 31.75 40.64 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q1"
			(at 31.7499 45.72 0)
		)
		(property "Value" "BD139"
			(at 31.75 46.99 90)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 33.655 45.72 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 31.75 40.64 0)
		)
		(property "Description" "1.5A Ic, 80V Vce, Low Voltage Transistor, TO-126"
			(at 31.75 40.64 0)
		)
		(property "Sim.Device" "NPN"
			(at 31.75 40.64 0)
		)
		(property "Sim.Pins" "1=E 2=C 3=B"
			(at 31.75 40.64 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 144.78 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D17"
			(at 144.78 82.55 0)
		)
		(property "Value" "1N4148"
			(at 144.78 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 144.78 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 144.78 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 144.78 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 144.78 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 144.78 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 170.18 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D46"
			(at 170.18 143.51 0)
		)
		(property "Value" "1N4006"
			(at 170.18 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 170.18 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 170.18 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 170.18 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 170.18 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 170.18 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D46")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 168.91 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW16"
			(at 168.91 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 168.91 133.35 0)
		)
		(property "Footprint" ""
			(at 168.91 133.35 0)
		)
		(property "Datasheet" "~"
			(at 168.91 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 168.91 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 99.06 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U5"
			(at 99.7586 128.27 0)
		)
		(property "Value" "~"
			(at 97.2186 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 99.06 140.97 0)
		)
		(property "Datasheet" ""
			(at 99.06 140.97 0)
		)
		(property "Description" ""
			(at 99.06 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 170.18 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D44"
			(at 170.18 135.89 0)
		)
		(property "Value" "1N4148"
			(at 170.18 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 170.18 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 170.18 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 170.18 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 170.18 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 170.18 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D44")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 53.34 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U11"
			(at 54.0386 181.61 0)
		)
		(property "Value" "~"
			(at 51.4986 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 53.34 194.31 0)
		)
		(property "Datasheet" ""
			(at 53.34 194.31 0)
		)
		(property "Description" ""
			(at 53.34 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 144.78 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D41"
			(at 144.78 135.89 0)
		)
		(property "Value" "1N4148"
			(at 144.78 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 144.78 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 144.78 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 144.78 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 144.78 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 144.78 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D41")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 220.98 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D55"
			(at 220.98 143.51 0)
		)
		(property "Value" "1N4006"
			(at 220.98 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 220.98 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 220.98 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 220.98 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 220.98 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 220.98 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D55")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 170.18 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D22"
			(at 170.18 90.17 0)
		)
		(property "Value" "1N4006"
			(at 170.18 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 170.18 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 170.18 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 170.18 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 170.18 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 170.18 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 53.34 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D7"
			(at 53.34 90.17 0)
		)
		(property "Value" "1N4006"
			(at 53.34 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 53.34 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 53.34 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 53.34 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 53.34 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 53.34 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 121.92 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D16"
			(at 121.92 90.17 0)
		)
		(property "Value" "1N4006"
			(at 121.92 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 121.92 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 121.92 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 121.92 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 121.92 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 121.92 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Polarized_Small")
		(at 29.21 54.61 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C2"
			(at 28.6639 50.8 90)
		)
		(property "Value" "C_Polarized_Small"
			(at 28.6639 58.42 90)
		)
		(property "Footprint" ""
			(at 29.21 54.61 0)
		)
		(property "Datasheet" "~"
			(at 29.21 54.61 0)
		)
		(property "Description" "Polarized capacitor, small symbol"
			(at 29.21 54.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 76.2 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D34"
			(at 76.2 143.51 0)
		)
		(property "Value" "1N4006"
			(at 76.2 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 76.2 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 76.2 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 76.2 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 76.2 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 76.2 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D34")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 99.06 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D11"
			(at 99.06 82.55 0)
		)
		(property "Value" "1N4148"
			(at 99.06 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 99.06 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 99.06 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 99.06 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 99.06 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 99.06 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 170.18 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U7"
			(at 170.8786 128.27 0)
		)
		(property "Value" "~"
			(at 168.3386 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 170.18 140.97 0)
		)
		(property "Datasheet" ""
			(at 170.18 140.97 0)
		)
		(property "Description" ""
			(at 170.18 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 76.2 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U12"
			(at 76.8986 181.61 0)
		)
		(property "Value" "~"
			(at 74.3586 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 76.2 194.31 0)
		)
		(property "Datasheet" ""
			(at 76.2 194.31 0)
		)
		(property "Description" ""
			(at 76.2 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 30.48 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 31.1786 128.27 0)
		)
		(property "Value" "~"
			(at 28.6386 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 30.48 140.97 0)
		)
		(property "Datasheet" ""
			(at 30.48 140.97 0)
		)
		(property "Description" ""
			(at 30.48 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 99.06 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D37"
			(at 99.06 143.51 0)
		)
		(property "Value" "1N4006"
			(at 99.06 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 99.06 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 99.06 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 99.06 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 99.06 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 99.06 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D37")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 30.48 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D4"
			(at 30.48 82.55 0)
		)
		(property "Value" "1N4148"
			(at 30.48 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 30.48 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 30.48 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 30.48 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 30.48 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 30.48 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 195.58 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D25"
			(at 195.58 90.17 0)
		)
		(property "Value" "1N4006"
			(at 195.58 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 195.58 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 195.58 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 195.58 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 195.58 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 195.58 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D25")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 120.65 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW14"
			(at 120.65 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 120.65 133.35 0)
		)
		(property "Footprint" ""
			(at 120.65 133.35 0)
		)
		(property "Datasheet" "~"
			(at 120.65 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 120.65 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 29.21 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW10"
			(at 29.21 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 29.21 133.35 0)
		)
		(property "Footprint" ""
			(at 29.21 133.35 0)
		)
		(property "Datasheet" "~"
			(at 29.21 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 29.21 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 53.34 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D3"
			(at 53.34 82.55 0)
		)
		(property "Value" "1N4148"
			(at 53.34 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 53.34 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 53.34 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 53.34 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 53.34 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 53.34 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 30.48 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D28"
			(at 30.48 143.51 0)
		)
		(property "Value" "1N4006"
			(at 30.48 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 30.48 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 30.48 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 30.48 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 30.48 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 30.48 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D28")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 121.92 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D38"
			(at 121.92 135.89 0)
		)
		(property "Value" "1N4148"
			(at 121.92 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 121.92 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 121.92 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 121.92 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 121.92 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 121.92 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D38")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 53.34 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D29"
			(at 53.34 135.89 0)
		)
		(property "Value" "1N4148"
			(at 53.34 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 53.34 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 53.34 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 53.34 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 53.34 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 53.34 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D29")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 121.92 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW5"
			(at 121.92 78.74 0)
		)
		(property "Value" "SW_Push"
			(at 121.92 81.28 0)
		)
		(property "Footprint" ""
			(at 121.92 81.28 0)
		)
		(property "Datasheet" "~"
			(at 121.92 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 121.92 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 30.48 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D26"
			(at 30.48 135.89 0)
		)
		(property "Value" "1N4148"
			(at 30.48 138.43 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 30.48 142.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 30.48 142.24 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 30.48 142.24 0)
		)
		(property "Sim.Device" "D"
			(at 30.48 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 30.48 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D26")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 53.34 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D31"
			(at 53.34 143.51 0)
		)
		(property "Value" "1N4006"
			(at 53.34 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 53.34 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 53.34 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 53.34 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 53.34 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 53.34 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D31")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 76.2 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW3"
			(at 76.2 78.74 0)
		)
		(property "Value" "SW_Push"
			(at 76.2 81.28 0)
		)
		(property "Footprint" ""
			(at 76.2 81.28 0)
		)
		(property "Datasheet" "~"
			(at 76.2 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 76.2 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 195.58 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D24"
			(at 195.58 86.36 0)
		)
		(property "Value" "1N4006"
			(at 195.58 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 195.58 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 195.58 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 195.58 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 195.58 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 195.58 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 144.78 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW6"
			(at 144.78 77.47 0)
		)
		(property "Value" "SW_Push"
			(at 144.78 80.01 0)
		)
		(property "Footprint" ""
			(at 144.78 80.01 0)
		)
		(property "Datasheet" "~"
			(at 144.78 80.01 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 144.78 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 53.34 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 53.34 77.47 0)
		)
		(property "Value" "SW_Push"
			(at 53.34 80.01 0)
		)
		(property "Footprint" ""
			(at 53.34 80.01 0)
		)
		(property "Datasheet" "~"
			(at 53.34 80.01 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 53.34 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 99.06 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D13"
			(at 99.06 90.17 0)
		)
		(property "Value" "1N4006"
			(at 99.06 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 99.06 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 99.06 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 99.06 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 99.06 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 99.06 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 170.18 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U16"
			(at 170.8786 181.61 0)
		)
		(property "Value" "~"
			(at 168.3386 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 170.18 194.31 0)
		)
		(property "Datasheet" ""
			(at 170.18 194.31 0)
		)
		(property "Description" ""
			(at 170.18 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 27.94 21.59 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 27.94 19.05 90)
		)
		(property "Value" "R_Small"
			(at 29.2099 19.05 0)
		)
		(property "Footprint" ""
			(at 27.94 21.59 0)
		)
		(property "Datasheet" "~"
			(at 27.94 21.59 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 27.94 21.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 121.92 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D39"
			(at 121.92 139.7 0)
		)
		(property "Value" "1N4006"
			(at 121.92 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 121.92 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 121.92 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 121.92 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 121.92 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 121.92 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D39")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 144.78 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U6"
			(at 145.4786 128.27 0)
		)
		(property "Value" "~"
			(at 142.9386 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 144.78 140.97 0)
		)
		(property "Datasheet" ""
			(at 144.78 140.97 0)
		)
		(property "Description" ""
			(at 144.78 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 30.48 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 30.48 90.17 0)
		)
		(property "Value" "1N4006"
			(at 30.48 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 30.48 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 30.48 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 30.48 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 30.48 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 30.48 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 144.78 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D18"
			(at 144.78 86.36 0)
		)
		(property "Value" "1N4006"
			(at 144.78 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 144.78 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 144.78 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 144.78 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 144.78 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 144.78 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 121.92 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U14"
			(at 122.6186 181.61 0)
		)
		(property "Value" "~"
			(at 120.0786 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 121.92 194.31 0)
		)
		(property "Datasheet" ""
			(at 121.92 194.31 0)
		)
		(property "Description" ""
			(at 121.92 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "BD139_1")
		(lib_id "Transistor_BJT:BD139")
		(at 26.67 62.23 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q2"
			(at 25.3999 67.31 0)
		)
		(property "Value" "BD1679"
			(at 27.9399 67.31 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 28.575 67.31 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 26.67 62.23 0)
		)
		(property "Description" "1.5A Ic, 80V Vce, Low Voltage Transistor, TO-126"
			(at 26.67 62.23 0)
		)
		(property "Sim.Device" "NPN"
			(at 26.67 62.23 0)
		)
		(property "Sim.Pins" "1=E 2=C 3=B"
			(at 26.67 62.23 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148")
		(at 76.2 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D8"
			(at 76.2 82.55 0)
		)
		(property "Value" "1N4148"
			(at 76.2 85.09 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 76.2 88.9 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 76.2 88.9 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 76.2 88.9 0)
		)
		(property "Sim.Device" "D"
			(at 76.2 88.9 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 76.2 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 76.2 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D9"
			(at 76.2 86.36 0)
		)
		(property "Value" "1N4006"
			(at 76.2 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 76.2 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 76.2 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 76.2 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 76.2 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 76.2 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 52.07 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW11"
			(at 52.07 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 52.07 133.35 0)
		)
		(property "Footprint" ""
			(at 52.07 133.35 0)
		)
		(property "Datasheet" "~"
			(at 52.07 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 52.07 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 170.18 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D21"
			(at 170.18 86.36 0)
		)
		(property "Value" "1N4006"
			(at 170.18 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 170.18 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 170.18 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 170.18 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 170.18 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 170.18 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 121.92 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D15"
			(at 121.92 86.36 0)
		)
		(property "Value" "1N4006"
			(at 121.92 88.9 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 121.92 97.155 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 121.92 92.71 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 121.92 92.71 0)
		)
		(property "Sim.Device" "D"
			(at 121.92 92.71 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 121.92 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 53.34 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 54.0386 128.27 0)
		)
		(property "Value" "~"
			(at 51.4986 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 53.34 140.97 0)
		)
		(property "Datasheet" ""
			(at 53.34 140.97 0)
		)
		(property "Description" ""
			(at 53.34 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 196.85 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D49"
			(at 196.85 143.51 0)
		)
		(property "Value" "1N4006"
			(at 196.85 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 196.85 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 196.85 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 196.85 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 196.85 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 196.85 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D49")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 99.06 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D36"
			(at 99.06 139.7 0)
		)
		(property "Value" "1N4006"
			(at 99.06 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 99.06 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 99.06 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 99.06 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 99.06 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 99.06 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D36")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 170.18 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D45"
			(at 170.18 139.7 0)
		)
		(property "Value" "1N4006"
			(at 170.18 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 170.18 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 170.18 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 170.18 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 170.18 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 170.18 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D45")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 220.98 140.97 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U9"
			(at 221.6786 128.27 0)
		)
		(property "Value" "~"
			(at 219.1386 128.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 220.98 140.97 0)
		)
		(property "Datasheet" ""
			(at 220.98 140.97 0)
		)
		(property "Description" ""
			(at 220.98 140.97 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 34.29 31.75 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 34.29 29.21 90)
		)
		(property "Value" "R_Small"
			(at 35.5599 29.21 0)
		)
		(property "Footprint" ""
			(at 34.29 31.75 0)
		)
		(property "Datasheet" "~"
			(at 34.29 31.75 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 34.29 31.75 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 144.78 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U15"
			(at 145.4786 181.61 0)
		)
		(property "Value" "~"
			(at 142.9386 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 144.78 194.31 0)
		)
		(property "Datasheet" ""
			(at 144.78 194.31 0)
		)
		(property "Description" ""
			(at 144.78 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 220.98 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D52"
			(at 220.98 90.17 0)
		)
		(property "Value" "1N4006"
			(at 220.98 92.71 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 220.98 100.965 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 220.98 96.52 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 220.98 96.52 0)
		)
		(property "Sim.Device" "D"
			(at 220.98 96.52 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 220.98 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D52")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 219.71 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW9"
			(at 219.71 78.74 0)
		)
		(property "Value" "SW_Push"
			(at 219.71 81.28 0)
		)
		(property "Footprint" ""
			(at 219.71 81.28 0)
		)
		(property "Datasheet" "~"
			(at 219.71 81.28 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 219.71 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 97.79 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW13"
			(at 97.79 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 97.79 133.35 0)
		)
		(property "Footprint" ""
			(at 97.79 133.35 0)
		)
		(property "Datasheet" "~"
			(at 97.79 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 97.79 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 35.56 21.59 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 35.56 19.05 90)
		)
		(property "Value" "R_Small"
			(at 36.8299 19.05 0)
		)
		(property "Footprint" ""
			(at 35.56 21.59 0)
		)
		(property "Datasheet" "~"
			(at 35.56 21.59 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 35.56 21.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 220.98 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U18"
			(at 221.6786 181.61 0)
		)
		(property "Value" "~"
			(at 219.1386 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 220.98 194.31 0)
		)
		(property "Datasheet" ""
			(at 220.98 194.31 0)
		)
		(property "Description" ""
			(at 220.98 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Hongfa_Bistabil:hongfa_hfd2/012-s-l2-d")
		(at 196.85 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U17"
			(at 197.5486 181.61 0)
		)
		(property "Value" "~"
			(at 195.0086 181.61 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 196.85 194.31 0)
		)
		(property "Datasheet" ""
			(at 196.85 194.31 0)
		)
		(property "Description" ""
			(at 196.85 194.31 0)
		)
		(pin "13")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "16")
		(pin "2")
		(pin "11")
		(pin "9")
		(pin "6")
		(pin "15")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "U17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 121.92 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D40"
			(at 121.92 143.51 0)
		)
		(property "Value" "1N4006"
			(at 121.92 146.05 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 121.92 154.305 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 121.92 149.86 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 121.92 149.86 0)
		)
		(property "Sim.Device" "D"
			(at 121.92 149.86 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 121.92 149.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D40")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 29.21 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 29.21 77.47 0)
		)
		(property "Value" "SW_Push"
			(at 29.21 80.01 0)
		)
		(property "Footprint" ""
			(at 29.21 80.01 0)
		)
		(property "Datasheet" "~"
			(at 29.21 80.01 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 29.21 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 168.91 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW7"
			(at 168.91 77.47 0)
		)
		(property "Value" "SW_Push"
			(at 168.91 80.01 0)
		)
		(property "Footprint" ""
			(at 168.91 80.01 0)
		)
		(property "Datasheet" "~"
			(at 168.91 80.01 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 168.91 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 74.93 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW12"
			(at 74.93 130.81 0)
		)
		(property "Value" "SW_Push"
			(at 74.93 133.35 0)
		)
		(property "Footprint" ""
			(at 74.93 133.35 0)
		)
		(property "Datasheet" "~"
			(at 74.93 133.35 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 74.93 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4006")
		(at 76.2 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D33"
			(at 76.2 139.7 0)
		)
		(property "Value" "1N4006"
			(at 76.2 142.24 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 76.2 150.495 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 76.2 146.05 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 76.2 146.05 0)
		)
		(property "Sim.Device" "D"
			(at 76.2 146.05 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 76.2 146.05 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "D33")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 99.06 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW4"
			(at 99.06 77.47 0)
		)
		(property "Value" "SW_Push"
			(at 99.06 80.01 0)
		)
		(property "Footprint" ""
			(at 99.06 80.01 0)
		)
		(property "Datasheet" "~"
			(at 99.06 80.01 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 99.06 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Relaisteuerung"
				(path
					(reference "SW4")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
